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	Description
	Specifications

	New Thickness/MeasuredAt
	4.972-4.980" (126.289-126.492 MM)

	Minimum Thickness
	4.964" (126.086 MM)

	Warp Spec.
	.004" OVERALL (.102 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	1.1024-1.1033" (28.001-28.024 MM)

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	1.3380-1.3390" (33.985-34.011 MM)

	Comments
	* 1.654-1.674" REPORTED INSTALLED HEIGHT. STEM END REFACE LIMIT .008 I & E


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.654-1.674" (42.012-42.520 MM) *
	1.654-1.674" (42.012-42.520 MM) *

	Stem Diameter
	.2742-.2748" (6.965-6.98 MM)
	.2734-.2740" (6.944-6.96 MM)

	Total Length
	3.9772-4.0008" (101.021-101.62 MM)
	3.8787-3.9260" (98.519-99.72 MM)

	Head Diameter
	1.437-1.445" (36.5-36.703 MM)
	1.228-1.236" (31.191-31.394 MM)

	Angle
	45.5°
	45.5°

	Margin
	.020" MIN. (.508 MM)
	.020" MIN. (.508 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.524-.547" (13.31-13.894 MM)
	.524-.547" (13.31-13.894 MM)

	Guide Clearance
	.0008-.0021" (.02-.053 MM)
	.0016-.0029" (.041-.074 MM)

	Guide OD
	
	

	Valve Seal Type
	POSITIVE
	POSITIVE

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.058-.064" (1.473-1.626 MM)
	.071-.079" (1.803-2.007 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	1.4961-1.4967" (38.001-38.016 MM)
	1.2874-1.2880" (32.700-32.715 MM)

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	1.756" (44.602 MM) or 1.980" (50.3mm)
	1.756" (44.602 MM) OR 1.980" (50.3MM)

	Installed Height
	
	

	Open Test Press
	123# @ 1.024 Or 88-94 #s @ 1.150"
	123# @ 1.024 Or 88-94 #s @ 1.150"

	Close Test Press
	
	

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
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	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
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	Description
	Specifications

	Intake Valve Lash
	.012-.015" Hot (.304-.381 MM) for checking, .0146" Cold (.370 MM) for ADJUSTING

	Exhaust Valve Lash
	.013-.016" Hot (.330-.406 MM) for checking, .0146" Cold (.370 MM) for ADJUSTING

	Lash Adjustment Method
	ADJUSTING SHIMS

	Precup Torque Spec.
	

	Cyl Head Torque
	22, 58 FT/LBS, LOOSEN, 22, 54-61 FT/LBS

	Camshaft Cap Torque
	1ST 16.8 INCH/LBS, 2ND 80.4-104.4 INCH/LBS
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