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Cylinder Head
Casting
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	Description
	Specifications

	New Thickness/MeasuredAt
	5.0820" (129.083 MM) NEW

	Minimum Thickness
	5.0700" (128.900 MM)

	Warp Spec.
	.004" (.100 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	.4730-.4739" (12.013-12.037 MM)

	Comments
	


Valve
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	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.595-1.605" (40.513-40.767 MM)
	1.595-1.605" (40.513-40.767 MM)

	Stem Diameter
	.2344-.2355" (5.955-5.970 MM)
	.2337-.2343" (5.935-5.950 MM)

	Total Length
	
	

	Head Diameter
	1.3760-1.4154" (34.950-35.250 MM)
	1.1791-1.1909" (29.950-30.250 MM)

	Angle
	45°
	45°

	Margin
	.041" (1.053 MM)
	.044" (1.117 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	
	

	Guide Clearance
	.0012-.0022" (.030-.057 MM)
	.0020-.0026" (.050-.077 MM)

	Guide OD
	
	

	Valve Seal Type
	
	

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.0472" (1.200 MM)
	.0630" (1.600 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
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	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	1.6299-1.7402" (41.400-44.200 MM)
	1.6299-1.7402" (41.400-44.200 MM)

	Installed Height
	1.2795"
	1.2795"

	Open Test Press
	118-129 LBS @ .8858"
	118-129 LBS @ .8858"

	Close Test Press
	55-61 LBS @ 1.2795"
	55-61 LBS @ 1.2795"

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
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	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	1.68:1


Installation
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	Description
	Specifications

	Intake Valve Lash
	HYDRAULIC

	Exhaust Valve Lash
	HYDRAULIC

	Lash Adjustment Method
	NONE

	Precup Torque Spec.
	

	Cyl Head Torque
	22 FT/LBS + 155°

	Camshaft Cap Torque
	TIGHTEN IN THREE STEPS TO 89 INCH/LBS
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