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Cylinder Head

	Description
	Specifications

	[bookmark: _GoBack]New Thickness/Measured At
	3.539-3.547" (89.900-90.100 MM)

	Minimum Thickness
	3.5230" (89.484 MM)

	Warp Spec.
	.008" OVERALL (.203 MM)

	Chamber Volume (cc)
	75.2 CC

	Surface Finish
	

	OHC Camshaft Bore Diameter
	1.3390" (34.011 MM)

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	* VALVE SPG FREE LENGTH FROM 5/84->90 = 1.961" AUX VALVE ASSEMBLY PART #MD009440


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.690-1.710" (42.926-43.434 MM)
	1.680-1.700" (42.672-43.18 MM)

	Stem Diameter
	.3150" (8.001 MM)
	.3150" (8.001 MM)

	Total Length
	4.330" (109.982 MM)
	4.250" (107.95 MM)

	Head Diameter
	1.800" (45.72 MM)
	1.500" (38.1 MM)

	Angle
	45°
	45°

	Margin
	.028-.047" (.711-1.194 MM)
	.039-.079" (.991-2.007 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.460" (11.684 MM)
	.460" (11.684 MM)

	Guide Clearance
	.0012-.0024" (.03-.061 MM)
	.0020-.0035" (.051-.089 MM)

	Guide OD
	
	

	Valve Seal Type
	POSITIVE
	POSITIVE

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.035-.051" (.889-1.295 MM)
	.035-.051" (.889-1.295 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	'79-4/84:1.875" (2006.6 MM) *
	'79-4/84:1.875" (2006.6 MM) *

	Installed Height
	1.590-1.629" (40.386-41.377 MM)
	1.590-1.629" (40.386-41.377 MM)

	Open Test Press
	
	

	Close Test Press
	61# @ 1.591
	61# @ 1.591

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
Collapse [image: ]
	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	.006" HOT (.152 MM)

	Exhaust Valve Lash
	.010" HOT & AUX (.254 MM)

	Lash Adjustment Method
	AUX VLV ASSMBLY PART #MD009440

	Precup Torque Spec.
	

	Cyl Head Torque
	65-72 FT/LBS COLD, 73-79 FT/LBS HOT
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