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Cylinder Head
Casting
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	Description
	Specifications

	[bookmark: _GoBack]New Thickness/Measured At
	3.6673-3.6712" (93.149-93.248 MM)

	Minimum Thickness
	3.6513" (92.743 MM)

	Warp Spec.
	.008" OVERALL (.203 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	1.3420-1.3437" (34.087-34.13 MM)

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.7200-1.7500" (43.688-44.45 MM)
	1.7200-1.7500" (43.688-44.45 MM)

	Stem Diameter
	.3129-.3134" (7.948-7.96 MM)
	.3118-.3124" (7.92-7.935 MM)

	Total Length
	
	

	Head Diameter
	1.740" (44.196 MM)
	1.450" (36.83 MM)

	Angle
	45°
	45°

	Margin
	.032" MIN. (.813 MM)
	.040" MIN. (1.016 MM)

	Recession
	.040-.067" V/REC (1.016-1.702 MM)
	.040-.067" V/REC (1.016-1.702 MM)

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.634-.642" (16.104-16.307 MM)
	.634-.642" (16.104-16.307 MM)

	Guide Clearance
	.0009-.0022" (.023-.056 MM)
	.0015-.0028" (.038-.071 MM)

	Guide OD
	
	

	Valve Seal Type
	POSITIVE
	POSITIVE

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.063-.077" (1.6-1.956 MM)
	.063-.077" (1.6-1.956 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
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	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	1.895, 1.832MIN (NM)
	1.895, 1.832MIN (NM)

	Installed Height
	1.615" (41.021 MM)
	1.615" (41.021 MM)

	Open Test Press
	
	

	Close Test Press
	48-56# @ 1.615
	48-56# @ 1.615

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
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	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	.008" COLD (.203 MM)

	Exhaust Valve Lash
	.008" COLD (.203 MM)

	Lash Adjustment Method
	ADJUSTING SCREW, 9.4 FT/LBS

	Precup Torque Spec.
	

	Cyl Head Torque
	58-72 FT/LBS
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