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Cylinder Head

	Description
	Specifications

	New Thickness/Measured At
	3.5413-3.5452" (89.949-90.048 MM)

	Minimum Thickness
	3.533" (89.492 MM)

	[bookmark: _GoBack]Warp Spec.
	.006" OVERALL (.152 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	1.1811-1.1821" (30.-30.025 MM)

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.9290-1.9490" (48.997-49.505 MM)
	1.9290-1.9490" (48.997-49.505 MM)

	Stem Diameter
	.2744-.2750" (6.97-6.985 MM)
	.2742-.2748" (6.965-6.98 MM)

	Total Length
	4.4209-4.4367" (112.291-112.692 MM)
	4.4653-4.4811" (113.419-113.82 MM)

	Head Diameter
	
	

	Angle
	45°
	45°

	Margin
	.039" (.991 MM)
	.059" (1.499 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.925-.953" (23.495-24.206 MM)
	.925-.953" (23.495-24.206 MM)

	Guide Clearance
	.0010-.0024" (.025-.061 MM)
	.0012-.0026" (.03-.066 MM)

	Guide OD
	
	

	Valve Seal Type
	POSITIVE
	POSITIVE

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.047-.063" (1.194-1.6 MM)
	.047-.063" (1.194-1.6 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
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	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	1.960-1.970" (49.784-50.038 MM)
	1.960-1.970" (49.784-50.038 MM)

	Installed Height
	1.693" (43.002 MM)
	1.693" (43.002 MM)

	Open Test Press
	
	

	Close Test Press
	44-50# @ 1.693
	44-50# @ 1.693

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
Collapse [image: ]
	Description
	Specifications

	Shaft Diameter
	.8252-.8260" (20.96-20.98 MM)

	Bore Diameter
	.8268-.8281" (21.001-21.034 MM)

	Oil Clearance
	.0008-.0029" (.02-.074 MM)

	Rock Arm Ratio
	


Installation
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	Description
	Specifications

	Intake Valve Lash
	HYD

	Exhaust Valve Lash
	HYD

	Lash Adjustment Method
	NONE

	Precup Torque Spec.
	

	Cyl Head Torque
	LARGE BOLTS: 59-64 FT/LBS, SMALL BOLTS: 12-17 FT/LBS
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