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CYLINDER HEAD
	Description
	Specifications

	[bookmark: _GoBack]New Thickness/Measured At
	5.3150" (135.000 MM)

	Minimum Thickness
	NOT SUPPLIED BY THE OE

	Warp Spec.
	.004" OVERALL (.102 MM)

	Chamber Volume (cc)
	58.2

	Surface Finish
	

	OHC Camshaft Bore Diameter
	OIL CLEARANCE .001-.0024", MAX .0031"

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	1.2191-1.2195" (30.965-30.975 MM)

	Comments
	* GUIDE R&R GRADUALLY HEAT THE HEAD TO 176-212° F (80-100° C) ** REPORTED 1.560"


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.545-1.560" (39.243-39.624 MM) **
	1.545-1.560" (39.243-39.624 MM) **

	Stem Diameter
	.2350-.2356" (5.969-5.984 MM)
	.2348-.2354" (5.964-5.979 MM)

	Total Length
	4.0531" MIN (102.949 MM)
	4.0590" MIN (103.099 MM)

	Head Diameter
	
	

	Angle
	44.5°
	44.5°

	Margin
	.039" (.990 MM), MIN .020 (.5 MM)
	.039" (.990 MM), MIN .020 (.5 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.323-.339" (8.204-8.611 MM) *
	.323-.339" (8.204-8.611 MM) *

	Guide Clearance
	.0010-.0024" (.025-.061 MM), MAX .0031"
	.0012-.0026" (.03-.066 MM), MAX .0039"

	Guide OD
	
	

	Valve Seal Type
	POSITIVE
	POSITIVE

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.039-.055" (.991-1.397 MM)
	.039-.055" (.991-1.397 MM)

	Seat Angle
	30° / 45° / 60°
	30° / 45° / 60°

	Seat Outside Diameter
	CONTACT AREA MIDDLE OF VALVE
	CONTACT AREA MIDDLE OF VALVE

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	1.406" (35.712 MM)
	1.406" (35.712 MM)

	Open Test Press
	
	

	Close Test Press
	39.7-45.9 # @ 1.406
	3.9.7-45.9 # @ 1.406

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
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	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
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	Description
	Specifications

	Intake Valve Lash
	.006-.010" COLD (.152-.254 MM)

	Exhaust Valve Lash
	.010-.014" COLD (.254-.356 MM)

	Lash Adjustment Method
	ADJUSTING SHIMS

	Precup Torque Spec.
	

	Cyl Head Torque
	29 FT/LBS, + 90°, + 90°, BOLTS 4.094" MIN IN THREADS OR REPL

	Camshaft Cap Torque
	12FT/LBS
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