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	Description
	Specifications

	New Thickness/Measured At
	3.169" (80.493 MM) reported

	Minimum Thickness
	

	Warp Spec.
	.004" OVERALL (.102 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	* CASTING # 14066620 = 2.040-2.050" FOR BOTH INTAKE & EXHAUST ** ROCKER RATIO 1.75:1


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.9380-1.9680" (49.225-49.987 MM)*
	1.9380-1.9680" (49.225-49.987 MM)*

	Stem Diameter
	
	

	Total Length
	
	

	Head Diameter
	1.730" (43.942 MM)
	1.500" (38.100 MM)

	Angle
	46°
	46°

	Margin
	.031" (.787 MM)
	.031" (.787 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	
	

	Guide Clearance
	
	

	Guide OD
	
	

	Valve Seal Type
	
	

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.032-.063" (.813-1.6 MM)
	.032-.063" (.813-1.6 MM)

	Seat Angle
	45°
	45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	2.080" (52.832 MM)
	2.080" (52.832 MM)

	Installed Height
	1.660" (42.164 MM)
	1.660" (42.164 MM)

	Open Test Press
	175# @ 1.260
	175# @ 1.260

	Close Test Press
	83# @ 1.656" CHECK CASTING #'S
	83# @ 1.656" CHECK CASTING #'S

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
Collapse [image: ]
	Description
	Specifications

	Shaft Diameter
	RATIO: 1.75:1

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	3/4-1 TRN FRM 0 **

	Exhaust Valve Lash
	3/4-1 TRN FRM 0 **

	Lash Adjustment Method
	ADJUSTING SCREW

	Precup Torque Spec.
	

	Cyl Head Torque
	93 FT/LBS
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