EQ-CH262NC – CH262NO		   [image: ]
Casting
	Description
	Specifications

	New Thickness/Measured At
	3.0650" (77.851 MM)

	Minimum Thickness
	

	[bookmark: _GoBack]Warp Spec.
	.004" OVERALL (.102 MM)

	Chamber Volume (cc)
	

	Surface Finish
	

	OHC Camshaft Bore Diameter
	

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.900" (48.260 MM) reported
	2.000" (50.800 MM) reported

	Stem Diameter
	
	

	Total Length
	
	

	Head Diameter
	
	

	Angle
	45°
	45°

	Margin
	
	

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	V/Seal Height .0394-.0787" (1.001-1.999 MM)
	V/Seal Height .0394-.0787" (1.001-1.999 MM)

	Guide Clearance
	.0010-.0027" (.025-.069 MM)
	.00100.0027" (.025-.069 MM)

	Guide OD
	
	

	Valve Seal Type
	
	

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.040-0.065" (1.016-1.651 MM)
	.065-.098" (1.651-2.489 MM)

	Seat Angle
	46°
	46°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	2.020" (51.300 MM)
	2.020" (51.300 MM)

	Installed Height
	1.670-1.700" (42.920-43.430 MM)
	1.670-1.700" (42.920-43.430 MM)

	Open Test Press
	187-203 #'s @ 1.270"
	187-203 #'s @ 1.270"

	Close Test Press
	76-84 #'s @ 1.700"
	76-84 #'s @ 1.700"

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
Collapse [image: ]
	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	HYD

	Exhaust Valve Lash
	HYD

	Lash Adjustment Method
	None

	Precup Torque Spec.
	

	Cyl Head Torque
	22 FT/LBS + Long bolt 75°, medium bolt 65°, short bolt 55°
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