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Casting
	Description
	Specifications

	New Thickness/Measured At
	4.5850-4.5920" (116.459-116.637 MM)

	Minimum Thickness
	OEM CALLS NEW THICKNESS MINIMUM But .010" has been Safe

	Warp Spec.
	.002" OVERALL (.051 MM)

	Chamber Volume (cc)
	64 CC s

	Surface Finish
	

	OHC Camshaft Bore Diameter
	1.0245-1.0252" (26.022-26.040 MM)

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	* 2005-06 INTAKE HEAD DIAMETER=1.9103-1.9205" & INTAKE VALVE LENGTH=4.4666-4.4965".


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	2.0400-2.0550" (51.816 52.197 MM)
	2.0950-2.1100" (53.213-53.594 MM)

	Stem Diameter
	.2729-.2739" (6.931-6.957 MM)
	.2717-.2728" (6.901-6.929 MM)

	Total Length
	* 4.4539-4.4839" (113.129-113.891 MM)
	4.5244-4.5543" (114.92-115.679 MM)

	Head Diameter
	* 1.8846-1.8949" (47.869-48.13 MM)
	1.4516-1.4618" (36.871-37.13 MM)

	Angle
	45-45.5°
	45-45.5°

	Margin
	
	

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	.525" (13.335 MM)
	.525" (13.335 MM)

	Guide Clearance
	.0008-.0028" (.018-.071 MM)
	.0019-.0039" (.047-.098 MM)

	Guide OD
	
	

	Valve Seal Type
	
	

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.0698-.0928" (1.773-2.357 MM)
	.0673-.0911" (1.709-2.314 MM)

	Seat Angle
	44.5-45°
	44.5-45°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	1.929" (49.000 MM)
	1.929" (49.000 MM)

	Installed Height
	1.580" (40.120 MM)
	1.580" (40.120 MM)

	Open Test Press
	174-196# @ 1.137"
	174-196# @ 1.137"

	Close Test Press
	70-80# @ 1.580"
	70-80# @ 1.580"

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
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	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	.018-.033" (.457-.838 MM) Dry Lash

	Exhaust Valve Lash
	.018-.033" (.457-.838 MM) Dry Lash

	Lash Adjustment Method
	HLA

	Precup Torque Spec.
	

	Cyl Head Torque
	[bookmark: _GoBack]

	Camshaft Cap Torque
	100 INCH/LB
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