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CH364C
Specifications
	INTAKE 	EXHAUST
Port Volume: 	 258 CC  +/- 2cc	87C CC  +/- 2cc
Port Dimension: 	 2.559” +/- .0005 / 1.2515” +/- .0005	1.427” +/- .0005 / 1.5915” +/- .0005
Port Location: 	Stock  	
Valve Head Diameter:	2.165”	1.590”
Valve Seat Angles:	45	45
Valve Guide ID:	.3145” +/- .0005	.3145” +/- .0005
[bookmark: _GoBack]Valve Guide OD:	.500”	.500”
Chamber Volume: 	 69 CC  +/- 2cc
Spark Plug Location: 	 STOCK
Spark Plug Type:	 STOCK
Weight:	 22 LBS
•Highest grade of material used in manufacturing
•Thicker decks for greater strength
•Superior port finishes for increased flow
•Improved flow design to resist cracking
•Redesigned water flow for greater thermal conductivity
•Hardened exhaust seats
•CNC machined guides and seats
•25 point quality check on every head
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