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MONARCH INTERSECTS HIGH-GRADE GOLD ON ITS BEAUFOR PROPERTY, INCLUDING 187.0 G/T AU OVER 0.5 M (1.64 FEET) AND 151.5 G/T AU OVER 0.5 M (1.64 FEET) 

· Corporation intersects multiple high-grade gold intersections from underground and surface exploration drilling.
· Best high-grade results include 187.0 g/t Au over 0.5 m, 151.5 g/t Au over 0.5 m and 147.5 g/t Au over 0.3 m.
· Monarch has initiated Phase 2 of the surface drilling program to follow up on the recent near-surface results.
· The 42,500-metre drilling program is ongoing, with four drills underground and one on surface.

[bookmark: _Hlk25442045]Montreal, Québec, Canada, April 29, 2021 – MONARCH MINING CORPORATION (“Monarch” or the “Corporation”) (TSX: GBAR) (OTCMKTS: GBARF) is pleased to announce additional results from its 2020-2021 42,500-metre exploration diamond drilling program on its wholly-owned Beaufor Mine gold project, located 20 kilometres east of Val-d’Or, Québec. The results include several high-grade assays, including 187.0 g/t Au over 0.5 m, 151.5 g/t Au over 0.5 m and 147.5 g/t Au over 0.3 m, as Monarch continues to test for potential resources in proximity to the historical mine.
The Beaufor Mine initially began commercial production in the early 1930’s and over the years has produced over 1.1 million ounces of gold. The mine is currently on care and maintenance, which has given Monarch an opportunity to drill-test targets throughout the mine area. In June 2020, the Corporation initiated a 42,500-metre diamond drilling program to test two types of targets: the areas around historical high-grade intersections near the existing underground infrastructure, and isolated resource blocks, which are typically defined by a single drill intersection. Both of these “near-mine” targets can often be tested from the existing underground workings, generally by holes less than 200 metres long. Currently, 275 holes are planned or are already being drilled at 25-metre centres. If positive results are received, additional holes will be drilled to allow the zones in question to be converted into reserves and included in a future mine plan.
Assay results have been received for the first 121 holes (14,465 m), representing roughly 34% of the planned metres of drilling. High-grade results previously reported from the program included 783 g/t Au over 0.2 m and 293 g/t Au over 0.5 m (see press release dated October 1, 2020) and 35.87 g/t Au over 9.8 m (see press release dated January 19, 2021). Since the last reported results, the Corporation has drilled 83 additional holes (9,092 m), consisting of 79 exploration holes drilled from underground and 4 holes drilled from the surface. The best results are shown in Table 2 below and illustrated on the attached figures. Several of the holes have multiple intersections due to the stacked nature of the mineralization. The intersection widths reported are core lengths and high-grade intersections have not been capped, as the vein interpretation and statistics have not been finalized for the zones. 
Figure 1: Beaufor property recent assay results (longitudinal view looking N)
Figure 2: Beaufor property recent assay results (sectional view looking NW)

“We are thrilled with the results received to date. Our near-mine exploration drilling program continues to yield high-grade results as we intersect new mineralized zones and extensions of known zones outside the previously defined resource envelope. Monarch’s goal is to significantly increase the near-mine resource so that a minimal amount of new development and capital will be required to put the mine back into production in the short term,” said Jean-Marc Lacoste, President and Chief Executive Officer of Monarch. 
Near-mine exploration drilling is ongoing, with four drill rigs underground and one on surface. The focus remains on high-grade composites that are open along strike and existing resource blocks that contain sufficient room for expansion.
In April, Monarch initiated a Phase 2 surface drill program to follow up on recent positive near-surface results, including 35.87 g/t Au over 9.8 m (see press release dated January 19, 2021). This Phase 2 program consists of approximately 40 short holes totalling 4,000 m with the aim of defining additional resources and subsequent reserves.
Sampling consists of sawing the drill core into equal halves along its main axis and shipping one of the halves to ALS Canada in Val-d’Or and AGAT Laboratories in Mississauga, Ontario, for assaying. The samples are crushed, pulverized and assayed by fire assay, with atomic absorption finish. Samples exceeding 10.0 g/t Au are re-assayed using the gravity method and samples containing visible gold are assayed using the metallic screen method. Monarch uses a comprehensive QA/QC protocol, including the insertion of standards, blanks and duplicates. 

The technical and scientific content of this press release has been reviewed and approved by Christian Tessier, P.Geo., the Corporation’s qualified person under National Instrument 43-101.
About Beaufor
[bookmark: _Hlk70252492]The Beaufor Mine is located within the Bourlamaque Pluton at the eastern contact with the Dubuisson Formation. The Bourlamaque Batholith, a synvolcanic intrusion, is a major geological feature of the Val-d’Or mining camp. It is a quartziferous granodiorite cut by fine-grained dioritic dykes. Gold mineralization occurs in veins associated with shear zones dipping moderately south. Mineralization is associated with quartz-tourmaline-pyrite veins resulting from the filling of shear and extension fractures. Gold-bearing veins show a close association with mafic dykes intruding the granodiorite. A National Instrument 43-101 resource estimate for the Beaufor Mine property was prepared for Monarch Mining in December 2020 by Carl Pelletier, P. Geo., InnovExplo Inc., and John Langton, P. Geo., JPL GeoServices Inc. The mineral resource estimate is listed in the table below.

Table 1: 2020 mineral resource estimate for the Beaufor Mine 
	Category
	Tonnes
	Grade (g/t Au)
	Gold (ounces)

	Measured
	121,000
	5.62
	21,900

	Indicated
	310,100
	7.10
	70,800

	Total M+I
	431,100
	6.68
	92,700

	Inferred
	134,600
	6.96
	30,100



Mineral Resource Estimate notes: 
The independent and qualified person for the 2020 MRE, as defined by NI 43-101, is Carl Pelletier, P.Geo. (InnovExplo Inc.), and the effective date is December 18, 2020.
These mineral resources are not mineral reserves as they do not have demonstrated economic viability. The mineral resource estimates follow CIM Definition Standards and Guidelines.
A capping of 68.5 g/t Au on assays was applied for zones 8, B, M, M1 and Q, and 34.25 g/t for all other zones. The DDH intercepts (min. 2.4 m) were capped at 16.5 g/t. 
The estimate method was polygonal on cross-sections with a minimum width of 2.4 m using a density of 2.75 t/m3 for the 63 mineralized zones.
Measured resource polygons extend 8 m above and below development and up to 10 m laterally. Indicated resource polygons extend up to 20 m from DDH intercepts, along dip and along strike and a minimum of 2 polygons need to be in contact. Inferred resource polygons extend up to 40 m from DDH intercepts, along dip and along strike where a drill spacing ranges from 20 m to 40 m and/or in areas of isolated drill holes where mineralization is known.
The reasonable prospect for an eventual economical extraction is met by having a reasonable minimum width for the polygons, a cut-off grade of 3.20 g/t Au, application of constraining volumes on the blocks (potential underground scenario) below a 30 m crown pillar. The cut-off grades inputs are: a gold price of USD1,612/oz, a CAD:USD exchange rate of 1.34; a mining cost of $100/t for the long hole method and $145/t for the room and pillar method; a processing cost of $50/t; and G&A and environment of $13/t and includes the royalty of 1.0% and a refinery charge of $5/t. The cut-off grades should be re-evaluated in light of future prevailing market conditions (metal prices, exchange rate, mining cost, etc.).
Results are presented in situ. Ounce (troy) = metric tons x grade / 31.10348. The number of tonnes and ounces was rounded to the nearest hundred. Any discrepancies in the totals are due to rounding effects; rounding followed the recommendations as per NI 43-101.
InnovExplo Inc. is not aware of any known environmental, permitting, legal, title-related, taxation, socio-political, marketing or other relevant issue that could materially affect the mineral resource estimate.

About Monarch
Monarch Mining Corporation (TSX: GBAR) is a fully integrated mining company that owns four advanced projects, including the fully permitted past-producing Beaufor Mine, which has produced more than 1 million ounces of gold over the last 30 years. Other advanced assets include the Croinor Gold, McKenzie Break and Swanson properties, all located near Monarch’s wholly owned and fully permitted Beacon 750 tpd mill. Monarch owns 28,725 hectares (287 km2) of mining assets in the prolific Abitibi mining camp that host 588,482 ounces of combined measured and indicated gold resources and 329,393 ounces of combined inferred resources.
Forward-Looking Statements 
The forward-looking statements in this press release involve known and unknown risks, uncertainties and other factors that may cause Monarch’s actual results, performance and achievements to be materially different from the results, performance or achievements expressed or implied therein. Neither TSX nor its Regulation Services Provider (as that term is defined in the policies of the TSX) accepts responsibility for the adequacy or accuracy of this press release.
FOR MORE INFORMATION:
Jean-Marc Lacoste					1-888-994-4465			
President and Chief Executive Officer			jm.lacoste@monarchmining.com		

Mathieu Séguin						1-888-994-4465
Vice President, Corporate Development		m.seguin@monarchmining.com

Elisabeth Tremblay					1-888-994-4465
Senior Geologist – Communications Specialist		e.tremblay@monarchmining.com 

www.monarchmining.com



Table 2: Beaufor Mine significant assay results
	Hole
	From (m)
	To (m)
	Width* (m)
	Au (g/t)

	20-106-158
	0.00
	1.30
	1.30
	7.94

	20-106-158
	14.05
	15.05
	1.00
	8.89

	20-115-105
	6.50
	7.70
	1.20
	8.79

	20-116-123
	98.50
	99.05
	0.55
	14.00

	20-123-92
	57.30
	57.80
	0.50
	67.20

	20-126-80
	18.20
	18.90
	0.70
	7.55

	20-132-56
	73.35
	75.50
	2.15
	3.88

	20-132-57
	49.05
	51.50
	2.45
	2.10

	20-132-57
	60.00
	63.20
	3.20
	1.80

	20-132-58
	46.15
	48.50
	2.35
	20.21

	Incl.
	46.15
	46.45
	0.30
	147.50

	20-133-61
	45.00
	45.50
	0.50
	22.80

	20-133-63
	41.80
	42.30
	0.50
	11.60

	20-133-63
	93.50
	97.50
	4.00
	7.04

	Incl.
	94.30
	95.00
	0.70
	26.10

	20-133-63
	116.60
	120.10
	3.50
	7.90

	Incl.
	116.60
	117.20
	0.60
	29.00

	20-133-64
	107.00
	108.40
	1.40
	5.69

	20-133-66
	68.80
	71.25
	2.45
	3.98

	Incl.
	68.80
	69.30
	0.50
	17.90

	20-133-66
	100.80
	104.55
	3.75
	4.08

	Incl.
	100.80
	101.65
	0.85
	16.00

	20-133-67
	63.50
	66.05
	2.55
	2.61

	20-133-67
	79.50
	85.50
	6.00
	2.66

	20-133-68
	84.30
	87.25
	2.95
	3.48

	20-133-68
	94.30
	97.40
	3.10
	3.20

	Incl.
	94.30
	94.80
	0.50
	17.00

	20-133-73
	82.25
	87.50
	5.25
	1.41

	20-133-73
	90.00
	92.00
	2.00
	2.98

	20-133-73
	117.75
	120.00
	2.25
	3.58

	20-146-42
	23.60
	24.10
	0.50
	65.30

	20-152-19
	8.58
	9.58
	1.00
	94.42

	Incl.
	9.08
	9.58
	0.50
	187.00

	20-152-19
	36.80
	37.80
	1.00
	32.92

	Incl.
	37.30
	37.80
	0.50
	65.10

	20-152-19
	89.05
	90.70
	1.65
	8.91

	Incl.
	89.05
	89.55
	0.50
	26.50

	20-97-68
	3.85
	5.20
	1.35
	57.40

	Incl.
	3.85
	4.35
	0.50
	151.50

	20-97-69
	4.05
	5.70
	1.65
	10.07

	Incl.
	4.05
	4.55
	0.50
	26.70

	20-97-70
	7.70
	8.20
	0.50
	97.90

	BES-20-010
	24.80
	25.30
	0.50
	40.90

	BES-20-010
	59.40
	60.80
	1.40
	5.81

	BES-20-010
	76.30
	80.00
	3.70
	3.64

	BEU-20-10-001
	80.50
	83.20
	2.70
	10.81

	Incl.
	82.50
	83.20
	0.70
	23.90

	BEU-20-15-001A
	143.65
	144.65
	1.00
	7.17

	BEU-20-15-006
	46.10
	48.40
	2.30
	6.59

	BEU-20-15-008
	48.60
	51.00
	2.40
	5.29

	BEU-20-15-008
	89.40
	93.30
	3.90
	2.35

	BEU-20-17-001B
	100.90
	101.90
	1.00
	58.14

	Incl.
	100.90
	101.40
	0.50
	116.00

	BEU-20-17-001B
	136.30
	141.05
	4.75
	7.11

	Incl.
	137.75
	138.50
	0.75
	37.80

	BEU-20-17-001B
	148.35
	152.15
	3.80
	2.67

	BEU-20-17-002
	12.55
	13.15
	0.60
	66.90

	BEU-20-17-002
	94.25
	96.05
	1.80
	21.89

	Incl.
	94.25
	94.95
	0.70
	55.70

	BEU-20-17-005
	13.00
	16.50
	3.50
	1.69

	BEU-20-20-006
	41.30
	41.80
	0.50
	11.50

	BEU-20-20-007
	19.75
	23.15
	3.40
	1.53

	BEU-20-20-008
	22.80
	23.30
	0.50
	10.65

	BEU-21-10-005
	100.95
	103.80
	2.85
	5.57

	BEU-21-30-004
	75.80
	77.70
	1.90
	12.47

	Incl.
	75.80
	76.30
	0.50
	47.20


*The width shown is the core length. True width is unknown at this time.






Table 3: Beaufor Mine drill hole location
	Hole
	Easting
(Mine Grid)
	Northing
(Mine Grid)
	Elevation
(m)
	Az
(deg.)
	Dip
(deg.)
	Length
(m)

	20-103-62
	1849.08
	3158.36
	2358.75
	183.0
	-5.0
	41.1

	20-103-63
	1849.05
	3158.25
	2360.66
	179.0
	47.0
	31.0

	20-106-158
	1956.82
	3306.93
	2517.98
	309.0
	-41.0
	85.2

	20-106-159
	1958.23
	3306.36
	2518.03
	19.0
	-76.0
	51.3

	20-114-167
	2023.42
	3258.38
	2331.61
	39.0
	-5.0
	192.9

	20-114-168
	2023.48
	3258.08
	2331.70
	45.0
	-2.0
	162.0

	20-114-168A
	2023.48
	3258.13
	2331.77
	44.0
	0.0
	224.2

	20-115-105
	2029.77
	3245.89
	2331.88
	188.0
	4.0
	93.7

	20-116-122
	2047.59
	3260.40
	2327.98
	22.0
	-29.0
	145.7

	20-116-123
	2047.23
	3260.22
	2327.74
	15.0
	-39.0
	131.3

	20-116-124
	2048.04
	3260.35
	2327.57
	31.0
	-35.0
	102.8

	20-116-125
	2047.41
	3253.41
	2256.06
	29.0
	-16.0
	28.0

	20-120-190
	2081.72
	3237.95
	2260.30
	24.0
	-31.0
	70.8

	20-123-92
	2144.41
	3305.41
	2319.39
	97.0
	69.0
	63.0

	20-126-79
	2152.55
	3247.65
	2275.90
	71.0
	-18.0
	184.0

	20-126-80
	2152.78
	3247.44
	2275.70
	76.0
	-22.0
	178.6

	20-132-56
	2142.51
	3083.75
	2739.84
	331.0
	-85.0
	82.2

	20-132-57
	2142.78
	3085.13
	2739.78
	12.0
	-44.0
	65.5

	20-132-58
	2143.42
	3085.69
	2740.47
	27.0
	-14.0
	77.0

	20-133-61
	2189.00
	3164.00
	2741.00
	77.0
	-4.0
	90.2

	20-133-62
	2189.87
	3163.79
	2742.02
	94.0
	56.0
	113.4

	20-133-63
	2190.06
	3163.64
	2741.64
	100.0
	42.0
	124.0

	20-133-64
	2189.80
	3163.57
	2742.14
	107.0
	58.0
	127.7

	20-133-65
	2190.13
	3163.19
	2741.44
	117.0
	37.0
	108.0

	20-133-66
	2189.69
	3162.93
	2741.82
	138.0
	51.0
	192.3

	20-133-67
	2188.69
	3163.21
	2742.25
	171.0
	60.0
	157.7

	20-133-68
	2190.03
	3163.49
	2741.76
	108.0
	47.0
	144.7

	20-133-71
	2184.47
	3166.66
	2739.16
	70.0
	-72.0
	148.0

	20-133-73
	2185.91
	3166.42
	2739.26
	78.0
	-21.0
	150.6

	20-133-74
	2185.23
	3166.58
	2739.20
	90.0
	-50.0
	131.7

	20-133-75
	2185.00
	3168.00
	2742.00
	94.0
	-25.0
	155.8

	20-133-76
	2185.00
	3168.00
	2742.00
	96.0
	-35.0
	152.4

	20-146-42
	2330.57
	3172.41
	2598.69
	314.0
	60.0
	75.0

	20-152-19
	2384.25
	3135.53
	2598.82
	160.0
	28.0
	126.8

	20-152-20
	2384.96
	3136.25
	2566.02
	135.0
	38.0
	9.9

	20-152-20A
	2384.90
	3136.15
	2599.04
	135.0
	38.0
	159.1

	20-97-68
	1786.33
	3158.47
	2365.93
	316.0
	-62.0
	167.1

	20-97-69
	1785.84
	3158.66
	2365.85
	322.0
	-49.0
	175.5

	20-97-70
	1785.44
	3159.39
	2366.57
	324.0
	-14.0
	30.9

	20-97-71
	1786.17
	3158.82
	2365.96
	338.0
	-48.0
	149.4

	20-97-72
	1786.46
	3158.63
	2365.82
	344.0
	-62.0
	145.8

	20-97-73
	1787.42
	3159.10
	2366.54
	31.0
	-20.0
	25.8

	BES-20-007
	1849.74
	3782.25
	3047.78
	45.0
	-75.0
	95.0

	BES-20-010
	2480.84
	3420.56
	3065.03
	302.0
	-60.0
	108.0

	BES-20-011
	2480.84
	3420.56
	3065.03
	44.0
	-78.0
	105.0

	BES-20-022
	1545.00
	3105.00
	3049.00
	51.0
	-75.0
	432.0

	BEU-20-10-001
	2117.65
	3201.87
	2739.63
	198.0
	-9.0
	168.5

	BEU-20-15-001
	2472.06
	2993.14
	2598.41
	193.0
	7.0
	106.1

	BEU-20-15-002
	2472.55
	2996.74
	2598.85
	10.0
	19.0
	94.6

	BEU-20-15-003
	2472.71
	2996.86
	2597.60
	13.0
	-17.0
	58.5

	BEU-20-15-004
	2471.58
	2996.80
	2598.28
	22.0
	12.0
	65.6

	BEU-20-15-005
	2422.89
	3021.29
	2596.57
	3.0
	-64.0
	116.6

	BEU-20-15-006
	2362.64
	3051.81
	2596.23
	160.0
	-80.0
	171.0

	BEU-20-15-008
	2361.00
	3052.00
	2599.00
	256.0
	-74.0
	191.8

	BEU-20-17-001A
	1673.77
	3402.22
	2518.96
	267.0
	-36.0
	152.7

	BEU-20-17-001B
	1669.54
	3401.86
	2518.93
	267.0
	-36.0
	162.2

	BEU-20-17-002
	1673.17
	3402.63
	2518.85
	278.0
	-31.0
	142.7

	BEU-20-17-003
	1679.97
	3407.77
	2519.59
	36.0
	-21.0
	64.6

	BEU-20-17-004
	1748.28
	3352.39
	2518.50
	229.0
	-85.0
	35.5

	BEU-20-17-005
	1741.83
	3357.73
	2518.58
	307.0
	-33.0
	39.7

	BEU-20-17-006
	1750.22
	3352.74
	2518.57
	90.0
	-36.0
	39.5

	BEU-20-17-008
	1811.97
	3474.32
	2519.25
	268.0
	14.0
	196.5

	BEU-20-20-001
	1872.19
	3318.87
	2441.98
	324.0
	-30.0
	26.0

	BEU-20-20-002
	1842.53
	3362.22
	2443.95
	218.0
	16.0
	22.0

	BEU-20-20-003
	1866.10
	3378.74
	2444.45
	266.0
	79.0
	22.5

	BEU-20-20-004
	1841.93
	3362.02
	2442.81
	200.0
	-6.0
	26.0

	BEU-20-20-005
	1805.64
	3383.19
	2445.12
	162.0
	42.0
	30.0

	BEU-20-20-006
	1804.63
	3385.41
	2444.74
	29.0
	-44.0
	55.0

	BEU-20-20-007
	1804.70
	3384.16
	2444.85
	201.0
	60.0
	35.0

	BEU-20-20-008
	1804.26
	3383.11
	2444.62
	201.0
	35.0
	35.0

	BEU-20-20-009
	1777.96
	3385.63
	2442.92
	213.0
	-13.0
	50.0

	BEU-20-20-013
	1918.16
	3234.47
	2443.58
	30.0
	-6.0
	126.0

	BEU-20-30-001
	2031.49
	3230.02
	2251.52
	305.0
	-36.0
	233.3

	BEU-21-10-003
	2117.14
	3202.46
	2739.74
	212.0
	-10.0
	196.5

	BEU-21-10-005
	2116.98
	3202.79
	2739.54
	223.0
	-17.0
	144.6

	BEU-21-15-010
	2027.92
	3255.32
	2595.31
	4.0
	-24.0
	139.8

	BEU-21-17-007
	1812.85
	3473.84
	2520.05
	230.0
	31.0
	130.8

	BEU-21-20-010
	1957.53
	3311.32
	2442.66
	200.0
	-22.0
	38.0

	BEU-21-20-012
	2004.42
	3310.28
	2444.76
	314.0
	77.0
	35.0

	BEU-21-30-004
	2051.01
	3223.47
	2248.44
	25.0
	-24.0
	78.1

	BEU-21-30-007
	2118.32
	3234.05
	2240.10
	66.0
	-53.0
	174.0

	BEU-21-30-008
	2120.06
	3266.04
	2235.36
	40.0
	-53.0
	30.5

	BEU-21-30-011
	2156.50
	3382.65
	2221.59
	156.0
	42.0
	46.6







Table 4: Monarch combined gold resources
	
	Tonnes
(metric) 
	Grade 
(g/t Au)
	Ounces

	Croinor Gold1
	
	 
	

	Measured Resources
	80,100
	8.44
	21,700

	Indicated Resources
	724,500
	9.20
	214,300

	Total Measured and Indicated
	804,600
	9.12
	236,000

	Total Inferred
	160,800
	7.42
	38,400

	Beaufor Mine2
	
	 
	

	Measured Resources
	121,000
	5.62
	21,900

	Indicated Resources
	310,100
	7.10
	70,800

	Total Measured and Indicated
	431,100
	6.68
	92,700

	Total Inferred
	134,600
	6.96
	30,100

	McKenzie Break3
	
	 
	

	In-pit
	
	
	

	Total Indicated
	1,441,377
	1.80
	83,305

	Total Inferred
	2,243,562
	1.44
	104,038

	Underground
	
	
	

	Total Indicated
	387,720
	5.03
	62,677

	Total Inferred
	1,083,503
	4.21
	146,555

	Swanson4
	
	 
	

	In-pit
	
	
	

	Total Indicated
	1,864,000
	1.76
	105,400

	Total Inferred
	29,000
	2.46
	2,300

	Underground
	
	
	

	Total Indicated
	91,000
	2.86
	8,400

	Total Inferred
	87,000
	2.87
	8,000

	TOTAL COMBINED5
Measured and Indicated Resources
Inferred Resources
	
	 
	588,482
329,393

	

	1 Source: Monarch Gold prefeasibility study (January 19, 2018) and resource estimate (January 8, 2016). This resource estimate was prepared for Monarch Gold and has not been reviewed by a qualified person for Monarch Mining as required under National Instrument 43-101 and is thus considered as an historical estimate. 
2 Source: NI 43-101 Technical Report and Mineral Resource Estimate for the Beaufor Mine, December 18, 2020, Val-d’Or, Québec, Canada, Carl Pelletier, P. Geo., InnovExplo Inc. and John Langton, P. Geo., JPL GeoServices Inc.
3 Source: NI 43-101 Technical Evaluation Report on the McKenzie Break Property, February 1, 2021, Val-d’Or, Québec, Canada, Alain-Jean Beauregard, P.Geo., Daniel Gaudreault, P.Eng., Geologica Groupe-Conseil Inc., and Merouane Rachidi, P.Geo., Claude Duplessis, P.Eng., GoldMinds GeoServices Inc.
4 Source: NI 43-101 Technical Report and Mineral Resource Estimate for the Swanson Project, January 22, 2021, Val-d’Or, Québec, Canada, Christine Beausoleil, P. Geo. and Alain Carrier, P. Geo., InnovExplo Inc.
5 Numbers may not add up due to rounding.
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