IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-02-19T10:58:25"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140606_1530(x64) - Exporter 2015.0.2014.0606 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "jelena.kadric" of Organization (no name given)
  Owner history of Person "jelena.kadric" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "0702A5" | names: "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR:0702A5:287738" | material: materials ("Fabric - Mermet - M-Screen Ultimetal - 0702A5", "Fabric - Mermet - M-Screen Ultimetal - Verso A5", "Aluminum - Mermet") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Other, Phasing

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR: 0702A5" (IFCLABEL)
    Family and Type = "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR: 0702A5" (IFCLABEL)
    Height Control = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule Level = "Level: Level 0" (IFCLABEL)
    Symbol Control = FALSE (IFCBOOLEAN)
    Type = "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR: 0702A5" (IFCLABEL)
    Type Id = "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR: 0702A5" (IFCLABEL)
    Width Control = 800. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Windows_Blinds_Mermet_M-Screen-Ultimetal_FR" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "E2010320" (IFCTEXT)
    Assembly Description = "Window Treatments - Shades" (IFCTEXT)
    Description = "Tissu ajouré de fils de verre enduit PVC ignifugé métallisé 1 face LowE pour protection solaire int" (IFCTEXT)
    Keynote = "14.04" (IFCTEXT)
    Manufacturer = "MERMET" (IFCTEXT)
    Model = "M-Screen-Ultimetal" (IFCTEXT)
    OmniClass Number = "23.30.60.14.21" (IFCTEXT)
    OmniClass Title = "Shades" (IFCTEXT)
    Product Guid = "dbff6d9e-47c8-4aa3-acf8-af5342fccbee" (IFCTEXT)
    Product data url = "https://www.bimobject.com/mermet/product/m-screen-ultimetal" (IFCTEXT)
    Type Name = "0702A5" (IFCTEXT)
    URL = "http://www.sunscreen-mermet.fr/" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "0702A5" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "MERMET" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Dimension Overconstraint = TRUE (IFCBOOLEAN)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.67280683668331 (IFCAREAMEASURE) [SQUARE_METRE]
    Hauteur = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00141492035700227 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Marque du store = "" (IFCTEXT)
    Modèle du store = "" (IFCTEXT)
  Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Autres informations = "http://www.sunscreen-mermet.fr/" (IFCTEXT)
    Certification NF = FALSE (IFCBOOLEAN)
    Clarté = "Clair" (IFCTEXT)
    Classe pour l'intimité de nuit = "2 (effet modéré)" (IFCTEXT)
    Classe pour l'utilisation de la lumière naturelle = "1 (peu d'effet)" (IFCTEXT)
    Classe pour le contact visuel avec l'extérieur = "2 (effet modéré)" (IFCTEXT)
    Classe pour le contrôle de l'éblouissement = "3 (bon effet)" (IFCTEXT)
    Code de la toile ou de la lame chez le fournisseur = "M-Screen Ultimetal" (IFCTEXT)
    Code du coloris du produit chez le fournisseur = "0702" (IFCTEXT)
    Coefficient d'ouverture (Co) = "0.3" (IFCTEXT)
    Coloris du côté face au rayonnement = "Métallisé" (IFCTEXT)
    Commentaires = "Tissu métallisé sur 1 face" (IFCTEXT)
    Description de la toile ou de la lame chez le fournisseur = "Tissu ajouré de fils de verre enduit PVC, métallisé sur 1 face pour protection solaire intérieure" (IFCTEXT)
    Description du produit = "Tissu sans PVC pour stores intérieurs" (IFCTEXT)
    Données thermiques lumineuses ou énergétiques fournies = "Oui" (IFCTEXT)
    Facteur de réflexion lumineuse de la face opposée au rayonnement (rho' lum) = "0.52" (IFCTEXT)
    Facteur de réflexion lumineuse de la face orientée vers le rayonnement (rho lum) = "0.83" (IFCTEXT)
    Facteur de réflexion solaire de la face opposée au rayonnement incident (rho' sol) = "0.48" (IFCTEXT)
    Facteur de réflexion solaire de la face orientée vers le rayonnement incident (rho sol) = "0.83" (IFCTEXT)
    Facteur de transmission du rayonnement thermique (tau th) = "0.04" (IFCTEXT)
    Facteur de transmission globale (tau lum ou tau vnh) = "0.04" (IFCTEXT)
    Facteur de transmission solaire (tau sol) = "0.04" (IFCTEXT)
    Facteur de transmission transmis sous forme diffuse (tau vn-diff) = "0.01" (IFCTEXT)
    Facteur de transmission transmis sous forme direct (tau vn-h) (équivalent au Co) = "0.03" (IFCTEXT)
    Fiche environnementale = "Oui" (IFCTEXT)
    Nom Gamme = "SCREEN Low E" (IFCTEXT)
    Position possible par rapport au vitrage = "Entre vitrages|Intérieure" (IFCTEXT)
    Référence commerciale = "M-Screen Ultimetal 0702" (IFCTEXT)
    Si toile bi-face clarté de l'autre face = "Clair" (IFCTEXT)
    Si toile bi-face coloris dominant de l'autre face = "Gris" (IFCTEXT)
    Type de fiche environnementale = "FDES" (IFCTEXT)
    Type de protection = "Toile" (IFCTEXT)
    URL : Image ou schéma du produit = "https://www.sunscreen-mermet.fr/gammes/m-screen-ultimetal.html" (IFCTEXT)
    Émissivité effective de la face orientée vers l'extérieur = "0.05" (IFCTEXT)
    Émissivité effective de la face orientée vers l'intérieur = "0.89" (IFCTEXT)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Edition number = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Coloris (Face Arrière) = "Fabric - Mermet - M-Screen Ultimetal - Verso A5" (IFCLABEL)
    Coloris (Face Avant) = "Fabric - Mermet - M-Screen Ultimetal - 0702A5" (IFCLABEL)
    Material main = "Fiber Glass" (IFCTEXT)
    Material secondary = "Vinyl" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)