| OpendTect 8.0

Loading...
Searching...
No Matches
Classes
uiSeis

Seismic Data User Interface. More...

## Classes
class | uiSeisFileMan::BrowserDef
class | uiSeisPreStackMan::BrowserDef
class | uiMultCompSel::MCompDlg
class | uiSeis2DMultiLineSel::Setup
class | uiVelocityDesc::Setup
class | uiSynthSeis::Setup
class | uiSeisWaveletSel::Setup
class | uiSeisSel::Setup
class | uiSeisBrowser::Setup
class | uiSeisTransfer::Setup
class | uiBaseSynthSeis
class | uiBatchTime2DepthSetup
class | Vel::uiBatchVolumeConversion
class | uiCBVSPS3DOpts
class | uiCBVSVolOpts
class | uiClusterProc
class | uiDepth2Time
class | uiElasticModelProvider
class | uiElasticPropSelDlg
class | uiElasticPropSelGrp
class | uiFKSpectrum
class | uiFreqTaperDlg
class | uiFreqTaperGrp
class | uiFreqTaperSel
class | uiFuncTaperDisp
class | uiGISExport2DLines
class | uiMergeSeis
class | uiMultCompDlg
| dialog to select (multiple) component(s) of stored data More...
class | uiMultCompSel
| CompoundParSel to capture and sum up the user-selected components. More...
class | uiMultiZSeisSubSel
class | uiPreStackCopyDlg
| Dialog for copying PS data stores. More...
class | uiPreStackDataPackSelDlg
class | uiPreStackMergeDlg
| : setup a dialog where the user can select a set of Prestack volumes and merge them into one. The priority order decides which volume to use in case of an overlap. More...
class | uiPreStackOutputGroup
| Group for output when copying PS data stores. More...
class | uiPreStackSel
class | uiSeis2DFileMan
class | uiSeis2DFrom3D
class | uiSeis2DLineChoose
class | uiSeis2DLineNameSel
class | uiSeis2DLineSel
class | uiSeis2DMultiLineSel
class | uiSeis2DSubSel
class | uiSeis2DTo3D
| Dialog for 2D to 3D interpolation. More...
class | uiSeis2DTo3DInterPol
| Dialog for 2D to 3D interpolation. More...
class | uiSeis3DSubSel
class | uiSeisBayesClass
| 'Server' for Seismic Bayesian Inversion. More...
class | uiSeisBrowser
class | uiSeisCopy2DDataSet
| UI for copying 2d Datasets. More...
class | uiSeisCopyCube
| UI for copying cubes. More...
class | uiSeisDirectFileDataDlg
class | uiSeisDump2DGeom
class | uiSeisExpCubePositionsDlg
class | uiSeisFileMan
class | uiSeisFmtScale
class | uiSeisImpCBVSFromOtherSurveyDlg
class | uiSeisImportCBVS
| Imports or links to a CBVS file. More...
class | uiSeisIOObjInfo
class | uiSeisIOSimple
class | uiSeisMMProc
class | uiSeisMultiCubePS
class | uiSeisPartServer
| Seismic User Interface Part Server. More...
class | uiSeisPosProvGroup
| UI for SeisPosProvider. More...
class | uiSeisPreLoadedDataSel
class | uiSeisPreLoadMgr
| Manager for pre-loading Seismic Data. More...
class | uiSeisPreLoadSel
class | uiSeisPreStackMan
class | uiSeisRandTo2DBase
class | uiSeisRandTo2DLineDlg
class | uiSeisSel
class | uiSeisSelDlg
class | uiSeisSingleTraceDisplay
class | uiSeisSubSel
class | uiSeisTransfer
class | uiSeisTrcBufViewer
class | uiSeisWaveletSel
| 'Immediate' Wavelet selector, with optionally 'Manage' and/or 'Extract' buttons More...
class | uiSeisWvltCopy
class | uiSeisWvltCreate
class | uiSeisWvltExp
class | uiSeisWvltGen
class | uiSeisWvltImp
class | uiSeisWvltMan
class | uiSeisWvltMerge
class | uiSeisWvltRotDlg
class | uiSeisWvltSliderDlg
class | uiSeisWvltTaperDlg
class | uiElasticPropSelGrp::uiSelInpGrp
class | uiStaticsDesc
class | uiSteerCubeSel
class | uiSynthSeis
| Interface for selecting all parameters to run a Seis::RaySynthGenerator. More...
class | uiSynthSeisAdvancedGrp
| Group for the advanced synthetic generation parameters interface. More...
class | uiSynthSeisSel
class | uiTime2Depth
class | uiTrcPositionDlg
class | uiVelModelZAxisTransform
class | uiVelocityDesc
class | uiVelocityDescDlg
class | uiVelSel
| Field that selects a velocity volume, and edit it's properties/velocity tag. More...
class | uiWaveletDispProp
class | uiWaveletDispPropDlg
class | uiWaveletExtraction
class | uiWaveletMatchDlg
class | uiWaveletSel
class | uiSeisWvltMerge::WvltMathFunction

## Detailed Description

Seismic Data User Interface.

Most of the tools in this module enable import and export of seismic data into/from the OpendTect data store. The merge and manage tools manipulate seismic data already in the data store.

A standalone 'application' is the uiSeisMMProc class, which handles the distribution of processing on multiple machines.

Generated at
for the OpendTect seismic interpretation project. Copyright (C): dGB Beheer B.V. 1995-2025