<map id="VTILayer" name="VTILayer">
<area shape="rect" id="Node000001" title=" " alt="" coords="15,225,90,251"/>
<area shape="rect" id="Node000005" href="$classHTILayer.html" title=" " alt="" coords="15,299,91,324"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="55,264,55,298,50,298,50,264"/>
<area shape="rect" id="Node000002" href="$classElasticLayer.html" title="Elastic Impedance layer implementation: AI + SVel." alt="" coords="5,152,100,177"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="55,191,55,225,50,225,50,191"/>
<area shape="rect" id="Node000003" href="$classAILayer.html" title="Acoustic Impedance layer implementation." alt="" coords="19,79,86,104"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="55,118,55,152,50,152,50,118"/>
<area shape="rect" id="Node000004" href="$classRefLayer.html" title="Base class for all Acoustic and Elastic impedance layers This object uses SI values exclusively for a..." alt="" coords="15,5,90,31"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="55,44,55,78,50,78,50,44"/>
</map>
