

Epic™

The Epic™ from Little Giant Ladders® is a multi-position ladder in its ultimate form. Adjust your ladder to meet the needs of your project, so you can work more efficiently than ever. This tough-as-nails ladder is equipped with a variety of features that set this ladder apart from the rest.

**Multi-Position Ladder**

This multi-position ladder converts to multiple configurations with the press of a button. Seamlessly set up the Epic as a stepladder, extension ladder, 90-degree ladder, staircase ladder, or trestle-and-plank scaffolding\*. Whether you use it in the home or on the job, the Epic is durable and versatile enough to meet the task.

**Safety Rails**

This ladder features extendable safety rails that can be placed vertically or horizontally on the ladder. When placed vertically in the walkthrough position, the rails extend above the top of the ladder, giving you a sturdy handhold. This feature is ideal when climbing to the roof of the house because it gives you a stabilizing surface to move from the ladder to the roof with ease and back down again.

Additionally, the non-marring safety rails can be placed horizontally in the stand-off position, so you can set up your ladder around windows, spanning a distance of up to 7 feet. In its horizontal stand-off position, you can place hanging hooks on the rails, where you can hang items up to 15 lbs., like paint buckets, water or other supplies that you would like to have within arm’s reach.

**Other Benefits**

Other benefits of the ladder include Tip & Glide™ wheels that improve ladder mobility during transportation. It is uncommon to work on a perfectly level surface, and with the Rachet™ leg levelers, you can easily adjust your ladder to safely meet any uneven ground with ease. Integrated dual-position accessory ports connect to the Little Giant AirDeck®\*. The dual-position feature allows you to use certain accessories vertically or horizontally. The Epic is the kind of ladder that will soon become your new go-to tool for all of your projects.

**Specs**

The aluminum multi-position Epic ladder meets or exceeds all OSHA and ANSI standards and is rated to hold 300 lbs. and can hold up to 300 lbs. on both sides when used in the stepladder configuration.

\*Accessory not included

| **SPECIFICATIONS** | | |
| --- | --- | --- |
| Product Category | **Epic** | |
| Extension Lock | **Rapid Lock** | |
| Country Assembled | **China** | |
| Marketing Language | **English / Spanish** | |
| Duty Rating | **Type IA - Extra Heavy Duty** | |
| Feet | **Standard non-marring (snap-on)** | |
| Hinge Lock | **Plastic / Triple Locking Hinge** | |
| Material | **Aluminum** | |
| Load Capacity | **300 lbs.** | |
| Spreader System | **Hinge Lock** | |
| Ladder Type | **Telescoping - Articulated** | |
| Warranty | **Limited Lifetime** | |
| Size | **11' - 19'** | **3.35 m - 5.79 m** |
| Inside Clear Width | **1 ft.** | **32 cm** |
| Storage Height | **5 ft. 7 in.** | **1.70 m** |
| Storage Width At Base | **2 ft. 4 in.** | **71 cm** |
| Storage Depth | **9 in.** | **23 cm** |
| Inner Rung Depth | **1 in.** | **4 cm** |
| Outer Rung Depth | **1 in.** | **3 cm** |
| Double Rung Depth | **3 in.** | **8 cm** |
| Top Width | **1 ft. 6 in.** | **46 cm** |
| Product Weight | **46 lbs.** | **20.86 kg** |

| **FEATURES** | | |
| --- | --- | --- |
| Scaffolding Position | **Yes** | |
| Tip-N-Glide Wheels | **Yes** | |
| 90° Position | **Yes** | |
| **SHIPPING** | | |
| Freight Class | **250 - Ladders and/or Accessories** | |
| Ship Length | **68"** | **5' 8"** |
| Ship Width | **28"** | **2' 4"** |
| Ship Height | **9"** | **9"** |
| Ship Weight | **58.4 lbs.** | |
| HTS Code | **7616.99.5190** | |

| **STEP LADDER** | | |
| --- | --- | --- |
| Stepladder Size | **5' 6" - 9' 6"** | **1.68 m - 2.90 m** |
| Highest Standing Level Max | **7 ft. 7 in.** | **2.31 m** |
| Highest Standing Level Min | **3 ft. 11 in.** | **1.19 m** |
| Maximum Footprint | **6 ft. 4 in.** | **1.94 m** |
| Minimum Footprint | **3 ft. 11 in.** | **1.21 m** |
| Max Reach | **14 ft. 1 in.** | **4.29 m** |

| **SINGLE / EXTENSION** | | |
| --- | --- | --- |
| Extension Total Length Of Sections | **21 ft. 2 in.** | **6.45 m** |
| Extension Max Reach | **22 ft.** | **6.71 m** |
| Single / Extension Highest Standing Level Max | **15 ft. 6 in.** | **4.72 m** |
| Single / Extension Highest Standing Level Min | **7 ft. 10 in.** | **2.39 m** |
| Single / Extension Max Working Length | **18 ft. 11 in.** | **5.77 m** |
| Single / Extension Min Working Length | **10 ft. 11 in.** | **3.33 m** |