{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":5,"n_cols":11,"rows_kept":5,"merged":[[1,0,1,11]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES "]
[]
[{"$nulls":10},"CONSTRUCTION OF EXTENSION BUILDING AT ADH.  DHIGURAH HEALTH CENTER."]

{"sheet":"SUMMARY","index":1,"n_rows":16,"n_cols":5,"rows_kept":16,"merged":[[1,0,1,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITIES"]
["CONSTRUCTION OF EXTENSION BUILDING AT ADH.  DHIGURAH HEALTH CENTER."]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01"]
[2,null,"DOORS AND WINDOWS","Bill no. 06"]
[3,null,"PAINTING","Bill no. 09"]
[4,null,"ELECTRICAL INSTALLATIONS","Bill no. 10"]
[5,null,"HYDRAULICS & DRAINAGE","Bill no. 11"]
[6,null,"TENDERER'S ADJUSTMENTS","Bill no. 13"]
[null,null,"Sub total"]
[null,null,"GST 8%"]
[]
[null,null,"GRAND TOTAL carried to form of bid"]

{"sheet":"BoQ","index":2,"n_rows":165,"n_cols":8,"rows_kept":165,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,7,5,7]],"flags":["formulas_cached_only"]}
["BILL OF QUANTITIES"]
["COMPLETION OF PENDING WORKS OF ADH.  DHIGURAH HEALTH CENTER EXTENSION BUILDING."]
[]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[1.5,"INSPECTION TRIPS"]
[{"v":1,"d":"(1)"},"Arrange inspection trip to PMU team. Each inspection trip takes 2 days.\nContractor has to arrange following for trips;\n(a) Speed boat transfer from Male city/Adh. Dhigurah /Male city. Type of Speed boat must be Gulf craft, Touring 36 or Equivalent.\n(c) Accommodations (2 Air-condition room) per trip.","Item",{"v":2,"d":"2.00"}]
[]
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL N0: 02"]
[null,"DOORS AND WINDOWS"]
[]
[2.1,"Window Curtains"]
[null,"Supply and installation of Curtains for following windows, quality of Curtains should be sun protected high quality, Rates should be complete installation of curtain with railing and ect.."]
[{"v":1,"d":"(1)"},"W1 windows , size of finished curtain should be 2.9m height, X1.3meter width.","No",{"v":5,"d":"5.00"}]
[{"v":2,"d":"(2)"},"W2 windows , size of finished curtain should be 2.9m height, X1.8 meter width.","No",{"v":7,"d":"7.00"}]
[{"v":2,"d":"(2)"},"W3 windows , size of finished curtain should be 2.9m height, X1.1 meter width.","No",{"v":2,"d":"2.00"}]
[]
[2.2,"BED SIDE CURTAINS"]
[null,"Supply and complete installation of top quality Hospital grade bed side curtain including railing/Track. Length of rail/track is 6870mm, and height of curtain would be 2.8 meter."]
[{"v":1,"d":"(1)"},"General ward","Item",{"v":6,"d":"6.00"}]
[]
[2.3,"Registration counter"]
[{"v":1,"d":"(1)"},"Design and Fabrication of Registration counter as per drawings, Fabrication of counter to be timber and appropriate thick plywood with PVC  fomica.","No",{"v":1,"d":"1.00"}]
[]
[null,"BILL N0: 02 -  DOORS AND WINDOWS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 3"]
[null,"PAINTING"]
[]
[3.1,"General"," "]
[null,"Exterior wall shall be of 1 coat of oil based textured paint and 2 coats of Kansani weather bond paint ( oil based ) over 1 coat of oil based sealer ( white) or equivalent (according to technical specifications or approved drawings). Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window and including soffits and sides of beams. "]
[null,"Interior wall shall be of 2-3 coats over 1 coat of water based sealer. Rates includes Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint, Kansani or equivalent as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window and including soffits and sides of beams."]
[]
[null,"Exterior & Exterior Ceiling  (interior and exterior) shall be of 2 coats of (wood paint over 1 coat of wood primer, Kansani or equivalent. Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for the provision and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and or masking floors fittings and similar work removing and replacing door window furniture. "]
[null,"All painting work shall be carried in accordance with the Specifications"]
[]
[3.2,"Wall painting"]
[]
["3.2.1","Internal Painting 1 coat of paints, Emulsion paint putty finish system."]
[{"v":1,"d":"(1)"},"Final coat of both side of Partition walls,","m²",{"v":226,"d":"226.00"}]
[]
[]
[]
[]
[]
[null,"BILL No: 3 - PAINTING"]
[null,"TOTAL OF BILL No: 3 - Carried over to summary"]
[null,"BILL No: 4"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[4.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each Light/ light fixture and its switch is measured as one  point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[]
[4.2,"Mains connection"]
[{"v":1,"d":"(1)"},"Main connection: Rates shall include for screws, nails, bolts ,nuts, standard cable, fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories. Rates shall including for electrical conduits, fittings, equipment and similar items. Three - PHASE CABLE WIRING TO D-BOARD:  All necessary work in trench shall include for excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers warning tape and disposal of surplus soil supply and laying of the cable in according to Maldives electricity bureau. ( 16mm2 4-Core Cable, Approved by respective Authorities, GI pipe, warning tape), contractor has to measure cable length from site. ","no",{"v":1,"d":"1.00"}]
[]
[4.3,"Lighting / Fan"]
[{"v":1,"d":"(1)"},"Ceiling diffusing embedded down light 200mm dia with 21W LED  bulb,  (Philips), Cool day light, (not crystal light or not Stellar bright) Total lumen 2300. or equivalent, For Portico area.","no",{"v":6,"d":"6.00"}]
[{"v":4,"d":"(4)"},"LED Emergency light ( 2 hours Battery charge)","no",{"v":6,"d":"6.00"}]
[" ",null,null," "]
[4.4,"Light switches "]
[null,"(a) All light switches shall be \"Legrand\" or equivalent. Each light should be control by one switch."]
[{"v":1,"d":"(1)"},"Three gang switch  at Portico area","no",{"v":12,"d":"12.00"}]
[]
[4.5,"Telephone Network"]
[{"v":1,"d":"(1)"},"Supply and complete installation of IP Telephone","No",{"v":10,"d":"10.00"}]
[]
[4.6,"Lightening Protection System"]
[{"v":1,"d":"(1)"},"Design, supply, and Complete installation of Erco, Eritech or equivalent lightening Protection System to cover the whole building as per local regulations (Rate shall include for all fixing of the system and down conductor to earthing) Coverage of lightning protection should be minimum 100 Meter Radius. Pric also include to install Marine grade SS post.","Item",{"v":1,"d":"1.00"}]
[]
[4.7,"SOLAR PV SYSTEM"]
[{"v":1,"d":"(1)"},"Design supply and complete installation on 10KW Solar PV system. Rates includes to complete the system and connect to the grid with net metering as per specification. ( junction box specs, Solar AC&DC cable specs, solar bracket specs, inverter specs & solar panel specs).","Item",{"v":1,"d":"1.00"}]
[4.8,"Fire Fighting"]
[{"v":1,"d":"(1)"},"CO2 Extinguisher","Item",{"v":3,"d":"3.00"}]
[{"v":2,"d":"(2)"},"H2O Extinguisher","Item",{"v":3,"d":"3.00"}]
[]
[4.9,"Supplying and installation of Furniture and IT Equipments"]
[null,"Supply and Complete installation of following items."]
[{"v":1,"d":"(1)"},"Office Table with drawer, 1200mm ( table should be solid wood).","No",{"v":6,"d":"6.00"}]
[{"v":2,"d":"(2)"},"Office Table with drawer, 1500mm ( table should be solid wood).","No",{"v":2,"d":"2.00"}]
[{"v":3,"d":"(3)"},"Secretary chair , high back.","No",{"v":8,"d":"8.00"}]
[{"v":4,"d":"(4)"},"Secretary chair , Low back.","No",{"v":10,"d":"10.00"}]
[{"v":5,"d":"(5)"},"Meeting room chair , thickness of tubes must be minimum 1.2mm\nMaterial: Iron/Aluminum\nSurface treatment: Spray painting finished.\nSeat and back: Hight-density sponge, minimum 2.5\" thick seat cushion ","No",{"v":30,"d":"30.00"}]
[{"v":6,"d":"(6)"},"Folding Meeting Table, 1400X600mm, \nSpecifications: Lockable castorsm Aluminum components\nFeature: Chrome with polished aluminum feet, Easy tilt mechanism for compact storage, \nTable surface: Scratch resistant, Natural Ash.","No",{"v":6,"d":"6.00"}]
[{"v":7,"d":"(7)"},"Supply and installation of 4 seater Airport Bench set, Armrest/Leg/bracket: Die-casting molding of high strength aluminum alloy. \nSeat: Numerical control hydraulic molding of high quality cold rolling steel plate. \nSponge: Cold consolidation and foam-forming of high density and super soft PU. \nBeam: metal tube with a diamond shape. \nCoating: Electrostatic coating after Rust-proof treatment, electroplated polishing.  ","No",{"v":12,"d":"12.00"}]
[{"v":8,"d":"(8)"},"Supply and complete installation of Computer system as per specifications","No",{"v":6,"d":"6.00"}]
[{"v":9,"d":"(9)"},"Supply and complete installation of 75\" QLED TV, LG, sony, Samsung at meting room. Any cast or chrome cast must support.","No",{"v":1,"d":"1.00"}]
[{"v":10,"d":"(10)"},"Supplying of Canon Monochrome Multi-Functional Device, image RUNNER 2725/ 2725i, (A4 & A3 sze) 3 in 1 printer or equivalent.","No",{"v":1,"d":"1.00"}]
[{"v":11,"d":"(11)"},"Supplying of Surface Pro 9, 12th Gen Intel® Core™ i7, 16GB RAM, 512GB SSD,Colour: Graphite, Microsoft Extended Hardware Service - 4 year, Surface Pro Signature Keyboard with Slim Pen 2 for Business - Black, Microsoft Surface 127W Power Supply for Business and Microsoft Arc Touch Mouse For PMU use.","No",{"v":2,"d":"2.00"}]
[]
[null,"BILL No: 4 - ELECTRICAL INSTALLATIONS"]
[null,"TOTAL OF BILL No: 4 - Carried over to summary"]
[]
[null,"BILL No: 5"]
[null,"HYDRAULICS & DRAINAGE"]
[]
[5.1,"Hydraulics"]
["5.1.1","General"]
[null,"(a)  Rates shall include for excavation, laying pipes and backfilling trenches, maintaining faces of drainpipe trenches and pits, backfilling, disposal of surplus soil, bends, junctions, reducers, expansion joints brackets, joints, straps, hangers, screws, nails and fixing complete, and all joints and other incidental material, All Pipes and fittings area high pressure uPVC  pipes"]
[null,"fixing complete, including cutting and forming holes; excavating, laying pipes and backfilling trenches."]
[null,"(b) All pipe work shall be uPVC."]
[]
[5.2,"Drainage"]
["5.2.1","General"]
[null,"(a) Rates shall include for: excavation, maintaining faces of drain pipe trenches and pits, backfilling, disposal of surplus spoil; bends, junctions, reducers, expansion joints and all joints and other incidental materials."]
[null,"(b) All pipe work shall be UPVC"]
[{"v":1,"d":"(1)"},"Constructing  Concrete Inspection Chamber of required size with all provisions to connect pipelines as per drawing.","Item",{"v":4,"d":"4.00"}]
[]
[5.3,"Pipe work"]
[]
[{"v":1,"d":"(1)"},"Completion of pipe works and Connect Waste disposal pipe 75mm dia to Sewer network installed at existing system.","Item",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Completion of pipe works and Connect Sewers pipe 100mm dia UPVC to   Sewer network installed at existing system. Rates includes to install inspection chamber as per consultants instructions.","Item",{"v":1,"d":"1.00"}]
[]
[null,"BILL No: 5 - HYDRAULICS & DRAINAGE"]
[null,"TOTAL OF BILL No: 5 - Carried over to summary"]
[]
[null,"BILL No:6"]
[null,"TENDERER'S ADJUSTMENTS"]
[]
[6.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[6.2,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"DOORS AND WINDOWS, Bill no. 06"]
[{"v":3,"d":"(3)"},"PAINTING, Bill no. 09"]
[{"v":4,"d":"(4)"},"ELECTRICAL INSTALLATIONS, Bill no. 11"]
[{"v":5,"d":"(5)"},"HYDRAULICS & DRAINAGE, Bill no. 10"]
[{"v":6,"d":"(6)"},"TENDERER'S ADJUSTMENTS,  Bill no. 13"]
[null,"ADDITIONS TOTAL"]
[]
[6.3,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"DOORS AND WINDOWS, Bill no. 06"]
[{"v":3,"d":"(3)"},"PAINTING, Bill no. 09"]
[{"v":4,"d":"(4)"},"ELECTRICAL INSTALLATIONS, Bill no. 11"]
[{"v":5,"d":"(5)"},"HYDRAULICS & DRAINAGE, Bill no. 10"]
[{"v":6,"d":"(6)"},"TENDERER'S ADJUSTMENTS,  Bill no. 13"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 6 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 6 - Carried over to summary"]