{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[1,0,1,11],[6,5,6,9]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES"]
[]
[{"$nulls":10},"Civil Works at the Mental Health Department, Orange Hiya Third Floor"]
[]
[{"$nulls":10},0]

{"sheet":"SUMMARY","index":1,"n_rows":21,"n_cols":5,"rows_kept":21,"merged":[[1,0,1,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITY"]
["Civil Works at the Mental Health Department, Orange Hiya Third Floor"]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01",0]
[2,null,"ALUMINIUM FRAME GLASS PARTITION WORKS","Bill no. 02",0]
[3,null,"CEILING","Bill no. 03",0]
[4,null,"DOORS","Bill no. 04",0]
[5,null,"ELECTRICAL INSTALLATIONS","Bill no. 05",0]
[6,null,"NETWORKING WORKS","Bill no. 06",0]
[7,null,"AIR CONDITIONING WORKS","Bill no. 07",0]
[8,null,"SUPPLY OF FURNITURES","Bill no. 08",0]
[9,null,"REPAIRS & OTHER WORKS","Bill no. 09",0]
[10,null,"TENDERER'S ADJUSTMENTS","Bill no. 10",0]
[null,null,"Sub total",null,0]
[null,null,"GST 8%",null,0]
[]
[]
[null,null,"GRAND TOTAL carried to form of bid",null,0]

{"sheet":"BoQ","index":2,"n_rows":262,"n_cols":8,"rows_kept":262,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,7,5,7]],"flags":["formulas_cached_only"]}
[" BILL OF QUANTITIES"]
["Civil Works at the Mental Health Department, Orange Hiya Third Floor"]
[]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"," "]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[1.2,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","Item",{"v":1,"d":"1.00"},null,null,0,0]
[]
[null,"BILL No: 01 PRELIMINARIES",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"ALUMINIUM FRAME GLASS PARTITION WORKS"]
[]
[2.1,"General"]
[null,"(a) Rates shall include for all materials, fittings, tools, accessories, labor, and other expenses to complete the entire work."]
[null,"(b) Rates shall include for design, supply, and installation."]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position."]
[null,"(d) All materials must be submitted to and approved by the project manager before installation."]
[]
[2.2,"Aluminium Framed Glass Partition Walls"]
[null,"(a) Specification of the glass partitions/panels shall be as follows;\n-Single-glazed, 6mm thick glass:\n   *Frosted glass panels (up to 1100mm from floor height)\n   *Crystal-clear glass panels (between 1100mm and 3000mm from floor height)\n-The edges of the glass panels shall be polished to remove any sharp corners/burrs."]
[null,"(b) Specification of the aluminium frames shall be as follows;\n-The aluminium framing shall be fabricated from aluminium alloy 6063 T5 extruded sections.\n-The frame shall be made of 2\" x 1.5\" aluminium sections with 1.2mm thickness all around.\n-Vertical members shall be at max distance of 1200mm centre-to-centre. \n-Horizontal members shall be at 1100mm from the floor level and 3000mm from the floor level centre-to-centre.\n-Aluminium cleats/brackets shall be provided at the junctions for securing the frames firmly.\n-The joints between aluminium members shall be mechanically joined using cleats and self tapping screws.\n-The frames shall be aligned in perfect plane & right angle to ensure flawless installation of glass.\n-Rubber/PVC beading gaskets shall be provided all around the glass to prevent any damage during transportation or installation.\n-The exposed aluminium surface shall be anodized in natural matt finish or powder coated (black color) as per approval."]
[null,"(c) The contractor shall provide Project Manager with a drawing of the walls before commencing the work, which should show the horizontal and vertical aluminium frames along with the dimensions. Also, the approval of the Project Manager shall be obtained for the drawings before initiating the work."]
[{"v":1,"d":"(1)"},"Design, supply and installation of aluminium framed glass partitions:\n-Director General (DG) Room (Height = 3000mm)","m²",24.63,null,null,0,0]
[{"v":2,"d":"(2)"},"Design, supply and installation of aluminium framed glass partitions:\n-Deputy Director General (DDG) Room (Height = 3000mm)","m²",9.14,null,null,0,0]
[null,"BILL No: 02 - ALUMINIUM FRAME GLASS PARTITION WORKS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"CEILING"]
[]
[3.1,"Interior Ceiling"]
[null,"(a) Rates shall include for all materials, fittings, tools, accessories, labor, and other expenses to complete the entire work."]
[null,"(b) Rates shall include for design, supply, and installation."]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position."]
[null,"(d) All materials must be submitted to and approved by the project manager before installation."]
[null,"(e) The false ceiling shall be provided using mineral fiber ceiling tiles of size 600mm x 600mm x 15mm."]
[null,"(f) The ceiling tiles shall have Humidity Resistance (RH) of 95%,  Light Reflectance ≥ 85%, Thermal Conductivity k = 0.052 - 0.057 W/mK, and Fire Performance as per ASTM E84 Class A."]
[null,"(g) The ceiling tiles shall be supported on hot dipped galvanized steel grid system with main runners at every 1200mm and cross tees at 600mm centre to centre."]
[null,"(h) The grid shall be suspended (hanged) from the roof slab using adjustable hangers of 2mm diameter GI wire at every 900mm c/c."]
[null,"(i) Perimeter trim channels having width of 20mm x 27mm shall be fixed along the perimeter of the ceiling."]
[null,"(j) The junctions between ceiling tiles shall be finished smoothly with no uneven gaps. Acoustic fleece shall be provided above the tiles."]
[null,"(k) The false ceiling system shall be non-combustible as per fire codes and standards."]
[{"v":1,"d":"(1)"},"Design, supply and installation of false ceilings:\n-Director General (DG) Room","m²",16.83,null,null,0,0]
[{"v":2,"d":"(2)"},"Design, supply and installation of false ceilings:\n-Deputy Director General (DDG) Room","m²",12.06,null,null,0,0]
[null,"BILL No: 03 - CEILING",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL N0: 04"]
[null,"DOORS"]
[]
[4.1,"General"]
[null,"(a) Rates shall include for all materials, fittings, tools, accessories, labor, and other expenses to complete the entire work."]
[null,"(b) Rates shall include for design, supply, and installation."]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position."]
[null,"(d) All materials must be submitted to and approved by the project manager before installation."]
[null,"(e) The door shall be made of 8mm thick clear tempered glass fixed in aluminium frame of 2\" x 1.5\" sections."]
[null,"(f) The aluminium frame shall have brushed finish. Horizontal members shall be provided at top and bottom of the door."]
[null,"(g) A lever-handle stainless steel door lock shall be fixed that could be locked from both sides."]
[null,"(h) A hydraulic door closer shall be fixed that could be adjustable."]
[null,"(i) Door stoppers shall be provided on the head to prevent the handles hitting the wall."]
[null,"(j) The contractor shall provide Project Manager with a drawing of the doors before commencing the work, which should show the horizontal and vertical aluminium frames along with the dimensions. Also, the approval of the Project Manager shall be obtained for the drawings before initiating the work."]
[]
[4.2,"Aluminium Framed Glass Door"]
[{"v":1,"d":"(1)"},"Design, supply & installation of aluminium framed glass door including all the hardware/fittings:\n-Director General (DG) Room - Single Door, 800mm x 2100mm (L x H)","no",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"Design, supply & installation of aluminium framed glass door including all the hardware/fittings:\n-Deputy Director General (DDG) Room - Single Door, 800mm x 2100mm (L x H)","no",{"v":1,"d":"1.00"},null,null,0,0]
[]
[null,"BILL N0: 04 -  DOORS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 04 - Carried over to summary"]
[null,"BILL No: 5"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[5.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing, or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each light / light fixture and its switch is measured as one  point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[]
[5.2,"Electrical Boards"]
[{"v":1,"d":"(1)"},"Three-phase electrical distribution board (surface-mounted):  Supply, installation & connection of D-Board.  Rates shall include all required brackets and other electrical appliance as per Maldivian Regulations. All the light circuits should be in one DB and sockets to be in another DB.","no",{"v":2,"d":"2.00"},null,null,0,0]
[]
[5.3,"Electrical wiring"]
[null,"Three-phase electrical wiring with copper conductor cable in conduits and in casing on soffits of slab as specified to: Each switch must control one light."]
[{"v":1,"d":"(1)"},"Wiring with 2.5 mm² cable to 2X13amp power points","points",{"v":26,"d":"26.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"Wiring with 2.5 mm² cable to 3X13amp power points (for each workstation, DG & DDG table)","points",{"v":42,"d":"42.00"},null,null,0,0]
[{"v":3,"d":"(3)"},"Wiring with 6 mm² cable to 1X15amp power points for Acs","points",{"v":4,"d":"4.00"},null,null,0,0]
[{"v":4,"d":"(4)"},"Wiring with 2.5 mm² cable to lights in Director General (DG) & Deputy Director General (DDG) Room","points",{"v":6,"d":"6.00"},null,null,0,0]
[]
[5.4,"Lighting"]
[null,"(a) Rates shall include for supply and installation/fixing of lights including the materials and accessories required to complete installation/fixing."]
[{"v":1,"d":"(1)"},"Ceiling LED light Square 600x600mm, color temp: 5000-6000K, luminous flux: 2400 - 3000.\nFor Director General (DG) Room and Deputy Director General (DDG) Room","no",{"v":6,"d":"6.00"},null,null,0,0]
[" ",null,null," "]
[5.5,"Socket outlets"]
[null,"(a) All socket outlets shall be \"Legrand\" or equivalent.",{"$nulls":5},0]
[{"v":1,"d":"(1)"},"2x13Amp wall Socket outlet,  ","points",{"v":26,"d":"26.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"3x13Amp wall Socket outlet (for each workstation & DG room table)","points",{"v":42,"d":"42.00"},null,null,0,0]
[{"v":3,"d":"(3)"},"1x15Amp wall Socket outlet for ACs,","points",{"v":4,"d":"4.00"},null,null,0,0]
[]
[5.6,"Light switches "]
[null,"(a) All light switches shall be \"Legrand\" or equivalent. Each light shall be controlled by one switch."]
[{"v":1,"d":"(1)"},"Two gang switch ","no",{"v":3,"d":"3.00"},null,null,0,0]
[]
[5.7,"Fire Fighting"]
[null,"Rates shall include for; supply and wall-mounting of extinguisher cylinders "]
[{"v":1,"d":"(1)"},"ABC Powder Extinguisher - 6KG Cylinder","Item",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"H2O Extinguisher - 9L Cylinder","Item",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":3,"d":"(3)"},"CO2 Extinguisher - 2KG Cylinder","Item",{"v":1,"d":"1.00"},null,null,0,0]
[]
[null,"BILL No: 5 - ELECTRICAL INSTALLATIONS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 5 - Carried over to summary"]
[null,"BILL No: 6"]
[null,"NETWORKING WORKS"]
[]
[6.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing, or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Rates shall include for supply and complete installation "]
[]
[6.2,"Computer Network"]
[null,"(a) Design, supply, and complete installation of computer networking, including CAT6 cabling, sockets and double layer switches for all the workstations ,  Allow for the provision of a completed and detailed set of shop drawings "]
[null,"(b) Rates shall include for all materials, items, fittings, accessories, and labour."]
[null,"(c) A sample of each material shall be presented to the client."]
[null,"(d) Before commencing the work, contractor shall take the exact measurements."]
[null,"(e) Cat6 cables must be used for internal connections from distribution racks to workstations"]
[null,"(f) Uplink cables to all distribution racks must be distinguished with color or type or label."]
[null,"(g) All cables in cable tray must be bundled with Velcro or easy-remove & reuse clips/ties"]
[null,"(h) All cables must be labelled at both ends."]
[null,"(i) All cables must be with cable boots on both ends."]
[null,"(j) Patch cables to workstations must be protected by floor casing (where applicable)"]
[]
[{"v":1,"d":"(1)"},"Completion of  Data Network points for workstations, faceplate must be \"Schneider\" Zencelo series or equivalent. Rate shall include for; CAT6 cabling work from the network rack (network cabinet) to the workstations (shown in drawing). The  network rack (network cabinet) is located in the \"Public Health Inspection\" block.","No",{"v":19,"d":"19.00"},null,null,0,0]
[]
[null,"BILL No: 6 - NETWORKING WORKS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 6 - Carried over to summary"]
[null,"BILL No: 7"]
[null,"AIR CONDITIONING WORKS"]
[7.1,"General"]
[null,"(a) Rates shall include for detail design, supply and complete installation of A/C units pipework, insulation, fixings, electrical wiring, drain pipes, etc."]
[null,"(b) The Contractor shall provide detailed and complete set of shop drawings."]
[null,"(c) The contractor shall submit shop drawings of AC. The capacity shall be determined by the contractor. "]
[null,"(d) Rate shall include complete installation of indoor units and outdoor units."]
[]
[7.2,"Air Condition Units"]
[null,"(a) Design, supply, and complete installation of indoor and outdoor units.  All AC units shall be DAIKIN, LG, VOLTAS or near-equivalent (INVERTER TYPE). "]
[null,"(b) The whole of the liquid and suction refrigerant lines including all fittings, valves etc. shall be insulated with 25mm thick insulation for all copper sizes. Insulation shall be closed cell elastomeric nitrile rubber."]
[null,"(c) Protection of exposed Refrigerant Pipe Insulation:\nTo protect nitrile rubber of exposed piping from degrading due to ultra violet rays & atmospheric conditions, it shall be covered by polychelid coating with at least two coats of resin and hardener (Make-Polybond / Paramount Polytreat). Fiberglass tape shall be helically wound & painted with two coats of resin with hardener to give smooth & plain finish. "]
[null,"(d) The proposed outdoor or outdoor set specifications should detail Energy Efficiency Ratio (EER) kw/kw not less than 4.5kw"]
[null,"(e) The outdoor units shall be factory-assembled with weather-proof casing, constructed from Heavy Gauge Mild Steel Panels and coated with anti-corrosive Epoxy resin finish. The units should be completely factory wired and tested and shall be fitted with all necessary controls and switch gear."]
[null,"(f) The proposed indoor units should have an indoor Sound Pressure Level below 30dB (A) "]
[null,"(g) All outdoor units need to have aluminum fins with 105+2 μm thickness, with special anti-corrosive coating of 1.3 ± 0. 35 μm thickness and an outside Hydrophilic layer coating of 0.35 ± 0. 07 μm thickness."]
[null,"(h) All outdoor units shall be equipped with high efficiency optimized heat exchangers with variable heat exchanger circuits"]
[null,"AC to be installed in the following rooms, all the indoor unit should be spilt type. "]
[]
[7.3,"Air Condition works"]
[{"v":1,"d":"(1)"},"12,000 BTU  spilt-type ceiling cassette air conditioner (with wireless remot) DAIKIN, LG, VOLTAS or near-equivalent  - in Director General (DG) Room & Deputy Director General (DDG) Room","Item",{"v":2,"d":"2.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"36,000 BTU  spilt-type ceiling cassette air conditioner (with wireless remote) DAIKIN, LG, VOLTAS or near-equivalent - in the Staff Area","Item",{"v":2,"d":"2.00"},null,null,0,0]
[]
[null,"BILL No: 7 -AIR CONDITIONING WORKS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 7 - Carried over to summary"]
[null,"BILL No: 08"]
[null,"SUPPLY OF FURNITURE"]
[8.1,"General"]
[null,"(a) Rates shall include for supply, complete installation/assemble, and arrangement of furnitures in the Mental Health Department, Orange Hiya third floor."]
[null,"(b) Contractor shall obtain approval of the Project Manager for each type of furniture prior to supply, installation/assemble, and arrangement. Also, contractor shall provide a catalogue (with photos)."]
[null,"(c) Contractor shall supply, install/assemble, and arrange the following furnitures;"]
[{"v":1,"d":"(1)"},"Low-Back Office Chair\nThe low-back office chair shall be of the below specifications;\n-Backrest Height: In Between 400mm and 500mm\n-Seat & Backrest Material: PU High-Density Molded Seat and Backrest\n-Base Material: Metal\n-Base Design: Swivel Chair Base with 5 Wheels (Tilt-Style Chair)\n-Finishing / Color: Black\n-Other Features: Swivel & Tilt, Adjustable Height, Arm Rest, Ergonomic.","No",{"v":14,"d":"14.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"Rectangular Office-Table with Table Divider\nOffice table with two lockable drawers (1200mm Length x 700mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging.  Table should be seperated with a desk divider attached/fixed on the table.  The tables that require divider are shown in the annexed drawing with red lines. The color of the table and divider shall be shades of brown, gray, black, and yellow.","No",{"v":10,"d":"10.00"},null,null,0,0]
[{"v":3,"d":"(3)"},"Medium-Back Office Chair\nThe medium-back office chair shall be of the below specifications;\n-Backrest Height: In Between 500mm and 600mm\n-Seat & Backrest Material: PU High-Density Molded Seat and Backrest\n-Base Material: Metal\n-Base Design: Swivel Chair Base with 5 Wheels (Tilt-Style Chair)\n-Finishing / Color: Black\n-Other Features: Swivel & Tilt, Adjustable Height, Arm Rest, Ergonomic.","No",{"v":10,"d":"10.00"},null,null,0,0]
[{"v":4,"d":"(4)"},"Rectangular Office-Table\nOffice table with three lockable drawers (1500mm Length x 750mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging. The color of the table shall be shades of brown, gray, black, and yellow.","No",{"v":3,"d":"3.00"},null,null,0,0]
[{"v":5,"d":"(5)"},"High-Back Office Chair\nThe high-back office chair shall be of the below specifications;\n-Backrest Height: In Between 600mm and 700mm\n-Seat & Backrest Material: PU High-Density Molded Seat and Backrest\n-Base Material: Metal\n-Base Design: Swivel Chair Base with 5 Wheels (Tilt-Style Chair)\n-Finishing / Color: Black\n-Other Features: Swivel & Tilt, Adjustable Height, Arm Rest, Ergonomic.","No",{"v":2,"d":"2.00"},null,null,0,0]
[{"v":6,"d":"(6)"},"L-Shaped Executive-Table for DG Room\nExecutive office table with three lockable drawers. The dimensions of the main table (front side) shall be (1500mm Length x 750mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging. The color of the table shall be shades of brown, gray, black, and yellow. Also, a side table of appropriate dimensions shall be provided along with the main table.","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":7,"d":"(7)"},"Executive Office Chair\nThe executive office chair shall be of the below specifications;\n-Backrest Height: In Between 700mm and 800mm\n-Seat & Backrest Material: PU High-Density Molded Seat and Backrest\n-Base Material: Metal\n-Base Design: Swivel Chair Base with 5 Wheels (Tilt-Style Chair)\n-Finishing / Color: Black (Executive Style)\n-Other Features: Swivel & Tilt, Adjustable Height, Arm Rest, Ergonomic.","No",{"v":2,"d":"2.00"},null,null,0,0]
[{"v":8,"d":"(8)"},"Wooden Round Meeting Table \nThe table shall have a diameter of  3ft and the tabletop shall be of 25mm Melamine top with 2mm ABS Edging. The color of the table shall be shades of brown, gray, black, and yellow.","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":9,"d":"(9)"},"Wooden Round Meeting Table for DG Room\nThe table shall have a diameter of  2.5ft and the tabletop shall be of 25mm Melamine top with 2mm ABS Edging. The color of the table shall be shades of brown, gray, black, and yellow.","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":10,"d":"(10)"},"Wooden Filing Cabinet  with Glass Door (Lockable)\nNumber of shelves in each filing rack: 5\nHeight of each shelf: minimum 15inch \nThe color of the table shall be shades of brown or gray.","No",{"v":5,"d":"5.00"},null,null,0,0]
[null,"BILL No: 08 - SUPPLY OF FURNITURES",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 08 - Carried over to summary"]
[null,"BILL No: 9"]
[null,"REPAIRS & OTHER WORKS"]
[9.1,"General"]
[null,"(a) Rates shall include for materials, accessories, tools, labours, etc. required for supply and complete installation."]
[]
[9.2,"Changing Door Locks"]
[{"v":1,"d":"(1)"},"Removal of existing lever-handle door lock of the main entrance door at the Mental Health Department.","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"Installation of new lever-handle door lock at the Mental Health Department. The lock shall meet the below specification and the brand shall be Yale or equivalent;\nMaterial: Stainless Steel\nHandle Type: Lever\nFinish Type: Chrome\nLock Cylinder Type: Single cylinder (key-to-knob)","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"$nulls":6},0,0]
[9.3,"Renovation of Toilets ",{"$nulls":4},0,0]
[{"v":1,"d":"(1)"},"Removal of existing muslim showers and installation of new PVC muslim showers. The brand shall be either Cotto, Grohe, or near-equivalent.","No",{"v":2,"d":"2.00"},null,null,0,0]
[{"v":2,"d":"(2)"},"Replacing the existing toilets with new toilets. The new toilet shall meet the below specification and the brand shall be Cotto or equivalent;\nBowl shape: Elongated\nColor: White\nSeat type: Slow-close / soft-close\nFlush type: Dual-flush","No",{"v":2,"d":"2.00"},null,null,0,0]
[{"v":3,"d":"(3)"},"Replacing the existing wash basin with new wash basin. The new wash basin shall meet the below specification and the brand shall be Cotto or equivalent;\nProduct type: Pedestal-stand washbasin\nMount type: Pedestal\nBasin shape: Round\nMaterial: Ceramic\nColor: White","No",{"v":1,"d":"1.00"},null,null,0,0]
[{"$nulls":6},0,0]
[9.4,"Parquet Flooring for the Director General (DG) Room and the Deputy Director General (DDG) Room",{"$nulls":4},0,0]
[null,"(a) The flooring shall be pre-finished engineered wooden parquet flooring planks.",{"$nulls":4},0,0]
[null,"(b) The wooden top layer shall be made of chopped beech wood fibers merged with resins for durability.",{"$nulls":4},0,0]
[null,"(c) The parquet planks shall be laid on a base of polyethylene foam underlay for leveling and sound insulation.",{"$nulls":4},0,0]
[null,"(d) The planks shall have tongue and groove mechanism for easy installation. The planks shall be installed using adhesive as per manufacturer's instructions.",{"$nulls":4},0,0]
[null,"(e) The flooring shall be finished smoothly with no uneven joints between planks.",{"$nulls":4},0,0]
[null,"(f) Wooden skirting board shall be installed along the perimeter walls over the flooring using adhesive and screws.",{"$nulls":4},0,0]
[{"v":1,"d":"(1)"},"Supply & installation of parquet flooring along with skirting boards for the DG room.","m²",16.83,null,null,0,0]
[{"v":2,"d":"(2)"},"Supply & installation of parquet flooring along with skirting boards for the DDG room.","m²",12.06,null,null,0,0]
[{"$nulls":6},0,0]
[9.5,"Drywall Partition Works",{"$nulls":4},0,0]
[null,"(a) Rates shall include for: all fabrication work, marking, drilling for bolts including those securing timbers, steel plates, bolts, nuts and any type of washer, riveted work, counter sinking and tapping for bolts or machine screws.",{"$nulls":4},0,0]
[null,"(b) Rate shall include for: timber priming and all painting.",{"$nulls":4},0,0]
[null,"(c) Rates shall include for painting of two coats of anti-bacterial interior matte paint and finishing.",{"$nulls":4},0,0]
[null,"(d) Rates shall include for fabrication and erection of temporary supports and fixing into position.",{"$nulls":4},0,0]
[null,"(e) All dry wall partition framing shall be of 600x600mm spaced both ways, using 50x50mm timber frame with 12mm thick Gymsum board on both sides. Rates shall include sealing all seams (fix mesh tape at all joints prior to application of putty), and sanding and leveling including all other necessary works.",{"$nulls":4},0,0]
[null,"(f) All timber used in frame shall be free of rots and knots. All the joints must be fixed rigidly.",{"$nulls":4},0,0]
[{"v":1,"d":"(1)"},"Drywall partition in the DG Room to cover and seal the wall at the toilets side.","m²",12.75,null,null,0,0]
[{"v":2,"d":"(2)"},"Drywall partition in the DDG Room to cover and seal the wall at the toilets side.","m²",9.14,null,null,0,0]
[{"$nulls":6},0,0]
[null,"BILL No: 9 - REPAIRS & OTHER WORKS",{"$nulls":5},0]
[null,"TOTAL OF BILL No: 9 - Carried over to summary"]
[null,"BILL No:10"]
[null,"TENDERER'S ADJUSTMENTS"]
[10.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[10.2,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"ALUMINIUM FRAME GLASS PARTITION WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"CEILING, Bill no. 03"]
[{"v":4,"d":"(4)"},"DOORS, Bill no. 04"]
[{"v":5,"d":"(5)"},"ELECTRICAL INSTALLATIONS, Bill no. 05"]
[{"v":6,"d":"(6)"},"NETWORKING WORKS, Bill no. 06"]
[{"v":7,"d":"(7)"},"AIR CONDITIONING WORKS, Bill no. 07"]
[{"v":8,"d":"(8)"},"SUPPLY OF FURNITURES, Bill no. 08"]
[{"v":9,"d":"(9)"},"REPAIRS & OTHER WORKS, Bill no. 09"]
[null,"ADDITIONS TOTAL"]
[]
[10.3,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"ALUMINIUM FRAME GLASS PARTITION WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"CEILING, Bill no. 03"]
[{"v":4,"d":"(4)"},"DOORS, Bill no. 04"]
[{"v":5,"d":"(5)"},"ELECTRICAL INSTALLATIONS, Bill no. 05"]
[{"v":6,"d":"(6)"},"NETWORKING WORKS, Bill no. 06"]
[{"v":7,"d":"(7)"},"AIR CONDITIONING WORKS, Bill no. 07"]
[{"v":8,"d":"(8)"},"SUPPLY OF FURNITURES, Bill no. 08"]
[{"v":9,"d":"(9)"},"REPAIRS & OTHER WORKS, Bill no. 09"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 10 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 10 - Carried over to summary"]