{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["BOQ"," summary ","cover"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOQ","index":0,"n_rows":493,"n_cols":6,"rows_kept":493,"merged":[[0,0,0,1],[1,1,1,4],[499,1,499,2],[500,1,500,2]],"flags":["formulas_cached_only"]}
[]
[null,"BILL OF QUANTITIES"]
[]
["Item","Description","Qty","Unit","Rate","Amount"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[null,"Abbreviations"]
[null,"m - metre"]
[null,"Nos - numbers"]
[null,"m³ - cubic metre"]
[null,"m² - square metre"]
[null,"Lm - Linear metre"]
[null,"t - tonnes"]
[null,"incl - including"]
[null,"mm - millimetre"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanised Iron"]
[null,"DN - Drawing number from drawings "]
[null,"SN - Sheet number from drawings "]
[]
[]
[1.1,"SITE MANAGEMENT COST"]
[null,"Allow for all on and off site management cost including cost of certified site engineer,foreman and assistants, temporary services, telephone, fax,hoardings, guards and similler.",{"v":1,"d":"1.00"},"item"]
[]
[]
[]
[null,"BILL No: 01 - PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"EARTH WORKS"]
[]
[2.1,"EXCAVATION"]
[null,"Note: Excavation quantities are measured to the faces of concrete members. Rates shall include for all additional excavation required to place the formwork/shuttering and dewatering the trenches for the required days. "]
[]
[{"v":1,"d":"(1)"},"Excavation for foundation beams",5.74,"m³"]
[]
[]
[2.2,"WATER PROOFING"]
[null,"Heavy duty polyethylene  sheet damp proof membrane (1000 gauge) laid on blinding layer.  "]
[null,"Note: Rates shall include for: dressing around and sealing to avoid all penetrations"]
[]
[{"v":1,"d":"(1)"},"Damp proof membrane under foundation beams",{"v":7.8,"d":"7.80"},"m2"]
[{"v":2,"d":"(2)"},"Damp proof membrane under ground slab",{"v":53,"d":"53.00"},"m2"]
[]
[{"v":3,"d":"(3)"},"Apply 2 coats of Brush Bond or similar on all concrete surfaces below ground level in accordance with manufacturer's instructions",{"v":23,"d":"23.00"},"m2"]
[]
[]
[2.3,"EARTH  FILLING"]
[null,"Rates shall include for levelling, grading, trimming and compacting."]
[{"v":1,"d":"(1)"},"Back filling",{"v":3.4000000000000004,"d":"3.40"},"m³"]
[{"v":2,"d":"(2)"},"200mm thk sand layer",{"v":10.600000000000001,"d":"10.60"},"m³"]
[]
[2.4,"CLEANING UPON COMPLETION"]
[{"v":1,"d":"(1)"},"Cleaning the site upon completion of all works",{"v":1,"d":"1.00"},"item"]
[]
[null,"BILL No: 01 - EARTH WORKS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"CONCRETE WORKS"]
[]
[null,"(a) Rates shall include for: provision to place in position; casting of all required items and finishing after removal of formwork and  additional concrete required to conform to structural and excavated tolerances "]
[null,"(b) Rates shall include supply of all formwork item including form oil, timber, plywood, nails etc."]
[null,"(c) Mix ratio for  reinforced concrete shall be 1:2:3 and lean concrete shall be 1:3:6 by volume"]
[null,"(d)RHEOMAC 707\" or equivalent concrete admixture shall be added to all concrete elements as per manufacturers instruction and specification."]
[]
[]
[3.1,"LEAN CONCRETE",null,0]
[null,"Note: Quantity is measured to the edges of concrete members. Rates shall be inclusive of any additional concrete required to place the formwork.",null,0]
[]
[{"v":1,"d":"(1)"},"50mm thick lean screed to bottom of  foundation beams at 1:5 ratio",{"v":7.8,"d":"7.80"},"m2"]
[]
[]
[3.2,"REINFORCED CONCRETE",null,0]
[" ","In-situ reinforced concrete to:",null,0]
["3.2.1","Foundation level",null,0]
[{"v":1,"d":"(1)"}," Foundation beams",2.34,"m³"]
["3.2.2","Ground Floor"]
[{"v":1,"d":"(1)"},"Columns ",{"v":0.8,"d":"0.80"},"m³"]
[{"v":2,"d":"(2)"},"Ground floor slab 75mm thick",{"v":3.9749999999999996,"d":"3.98"},"m³"]
[{"v":3,"d":"(3)"},"Concrete beds",{"v":0.3,"d":"0.30"},"m³"]
[{"v":4,"d":"(4)"},"Lintel and sill beams (150mmX150mm)on all doors and windows ",{"v":1,"d":"1.00"},"item"]
[]
["3.2.3","Roof"]
[{"v":1,"d":"(1)"},"Attached beams",1.75,"m³"]
[]
[3.3," FORMWORK"]
[null,"(a) Rates shall include for: all necessary boarding, supports, erecting, framing, temporary cambering, cutting, perforations for reinforcing bars, bolts, straps, ties, hangers, pipes and removal of formwork."]
[]
["3.3.1","Foundation level",null,0]
[{"v":1,"d":"(1)"}," Foundation beams",{"v":23,"d":"23.00"},"m2"]
[]
["3.3.2","Ground Floor"]
[{"v":1,"d":"(1)"},"Columns ",{"v":21.8,"d":"21.80"},"m2"]
[{"v":2,"d":"(2)"},"Concrete beds",{"v":3.1,"d":"3.10"},"m2"]
[{"v":3,"d":"(3)"},"Lintel and sill beams (150mmX150mm)on all doors and windows ",{"v":1,"d":"1.00"},"item"]
[]
["3.3.3","Roof"]
[{"v":1,"d":"(1)"},"Attached beams",{"v":28,"d":"28.00"},"m2"]
[3.4,"REINFORCEMENT",null,0]
[null,"(a) Rates shall include for: cleaning, fabrication, placing, the provision for all necessary temporary fixings and supports including tie wire and chair supports, laps and wastage",null,0]
[null,"(b) All reinforcing bars except 6mm dia bars shall be high strength deformed bars",null,0]
[null,"(c) The exact length exclusive of laps are given. The rates shall take into account laps and any wastage."]
[]
["3.4.1","Foundation"]
[{"v":1,"d":"(1)"},"12 mm dia. bars in  foundation beams",{"v":134,"d":"134.00"},"kg"]
[{"v":2,"d":"(2)"},"6 mm dia. bars in foundation beams",{"v":63,"d":"63.00"},"kg"]
[]
["3.4.2","Ground Floor"]
[{"v":1,"d":"(1)"},"10mm dia. bars in columns",{"v":95,"d":"95.00"},"kg"]
[{"v":2,"d":"(2)"},"6mm dia. bars in columns",{"v":40,"d":"40.00"},"kg"]
[{"v":3,"d":"(3)"},"10mm dia. bars in concrete bed",{"v":27,"d":"27.00"},"kg"]
[{"v":4,"d":"(4)"},"6 mm dia. bars in ground slab @ 300mm c/c",{"v":71,"d":"71.00"},"kg"]
[{"v":5,"d":"(5)"},"10 & R6 bars in  lintels and sill beams",{"v":1,"d":"1.00"},"item"]
[]
["3.4.3","Roof"]
[{"v":1,"d":"(1)"},"12mm dia. bars in beams",{"v":134,"d":"134.00"},"kg"]
[{"v":2,"d":"(2)"},"6mm dia. bars in beams",{"v":57,"d":"57.00"},"kg"]
{"$rows_empty":8}
[null,"BILL No: 03 - CONCRETE"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No: 04"]
[null,"MASONRY AND PLASTERING"]
[null,"Note: Rates shall include for: blocks, cutting or leaving holes and openings as recesses, building in pipes, conduits, sleeves and similar as required for all trades; leaving surfaces rough or raking out joints for plastering and flashing, bedding  frames. Blocks should be mechanical or machine compacted blocks with mix ratio 1:5"]
[null,"(a) Mix ratio for Plastering & masonry shall be 1:4.with river sand OPC cement"]
[4.1,"HOLLOW BLOCK WORK 100 MM THK"]
[{"v":1,"d":"(1)"},"External wall",{"v":89,"d":"89.00"},"m²"]
[{"v":2,"d":"(2)"},"Bed side wall",{"v":3.6,"d":"3.60"},"m²"]
[4.2,"HOLLOW BLOCK WORK 100MM THK"]
[{"v":1,"d":"(1)"},"Internal wall",{"v":31,"d":"31.00"},"m²"]
[]
[4.3,"PLASTERING"]
[null,"15mm thk for interior, 20mm thk for exterior plastering on walls and concrete surfaces."]
[]
[{"v":1,"d":"(1)"},"Ground floor"]
[null,"Interior",{"v":151,"d":"151.00"},"m²"]
[null,"Exterior",{"v":89,"d":"89.00"},"m²"]
[]
[]
[]
[4.4,"FLOOR SCREED"]
[null,"38mm thk,1:4 cement sand screeding on the floor to receive floor paint as  described"]
[]
[{"v":1,"d":"(1)"},"Internal floor and steps",{"v":53,"d":"53.00"},"m²"]
[]
[]
[]
[null,"BILL No: 04 - MASONRY AND PLASTERING"]
[null,"TOTAL OF BILL No: 04 - Carried over to summary"]
[null,"BILL No: 05"]
[null,"METAL WORKS/WOOD WORKS"]
[]
[null,"Note: (a) Rates shall include for: all fabrication work, welding, marking, drilling for bolts including those securing timbers, steel plates, bolts, nuts and any type of washer, riveted work, counter sinking and tapping for bolts or machine screws.",null,0]
[null,"(b) Rates shall include for all painting and finishing.",null,0]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position"]
[null,"(d) Rates shall include for the application of one coat redoxide to all welded joints and application of single coat aluminium paint on all GI pipes."]
[]
[]
[5.1,"COUNTERS/SHELVES"]
[{"v":1,"d":"(1)"},"Sink  counter with  homogeneous polished tiles finish on top .Rates  shall include, concete ,formwork ,water connection and completion all necessary works.",{"v":1,"d":"1.00"},"item"]
[]
[]
[{"v":2,"d":"(2)"},"Wooden kafan rack with  6 shelves 600mm X600mm made using 25mm thk mdf board and completion of all necessary works",{"v":1,"d":"1.00"},"item"]
[]
[]
[]
[]
[]
[]
[null,"BILL No: 05 - METAL/WOOD WORKS"]
[null,"TOTAL OF BILL No: 05 - Carried over to summary"]
[null,"BILL No: 06"]
[null,"CEILING"]
[6.1,"SUSPENDED CEILING"]
[]
[null,"6 mm thick fiber cement board for weather exposed area or toilets and eves & 9mm thick gypsum ceiling board for internal,  suspended ceiling systems Rates shall include finishing  with  steel frames for internal and external shall be wooden frames at 600mm X 600mm grid."]
[]
[{"v":1,"d":"(1)"},"External( toilet,eaves and external exposed area )",{"v":37,"d":"37.00"},"m²"]
[{"v":2,"d":"(2)"},"Internal  ceiling",{"v":40,"d":"40.00"},"m²"]
{"$rows_empty":24}
[null,"BILL N0: 06 - CEILINGS"]
[null,"TOTAL OF BILL No: 06 - Carried over to summary"]
[null,"BILL N0: 07"]
[null,"DOORS AND WINDOWS"]
[null,"Notes: (a) Rates shall include for locks, latches, closures, push plates, pull handles, bolts, kick plates, hinges and all door & window hardware."]
[null,"(b) Rates shall include for door frames, mullions, transoms, trims, glazing, tinting, timber panels, boarding, framing, lining, fastenings and all fixings"]
[null,"(c) Rates shall include for finishing"]
[]
[null,"All aluminium doors should be white powder coated finish . Door panel should be filled with rockwool as described "]
[null,"Rates shall include masonry and plastering for relocation doors and windows as per proposed plans"]
[]
[7.1," DOORS AND WINDOWS"]
[]
[{"v":1,"d":"(1)"},"D1 ( Aluminium door )",{"v":2,"d":"2.00"},"nos"]
[{"v":2,"d":"(2)"},"D2 ( Aluminium door )",{"v":1,"d":"1.00"},"nos"]
[{"v":3,"d":"(3)"},"D3 ( Aluminium door )",{"v":1,"d":"1.00"},"nos"]
[{"v":4,"d":"(4)"},"D4 ( Aluminium door )",{"v":1,"d":"1.00"},"nos"]
[{"v":5,"d":"(5)"},"W1 ( Aluminium window )",{"v":1,"d":"1.00"},"nos"]
[{"v":6,"d":"(6)"},"W2 ( Aluminium window )",{"v":1,"d":"1.00"},"nos"]
[{"v":7,"d":"(7)"},"W3 ( Aluminium window )",{"v":3,"d":"3.00"},"nos"]
[{"v":8,"d":"(8)"},"V1 ( Aluminium ventilator )",{"v":1,"d":"1.00"},"nos"]
[]
[]
[7.2," VERTICLE BLINDS"]
[]
[null,"Supply and installation of verticle blinds on all external doors and windows as described"]
[]
[{"v":1,"d":"(1)"},"W1",{"v":1,"d":"1.00"},"nos"]
[{"v":2,"d":"(2)"},"W2",{"v":1,"d":"1.00"},"nos"]
[]
[]
[]
[]
[null,"BILL N0: 07 -DOORS AND WINDOWS"]
[null,"TOTAL OF BILL No: 07 - Carried over to summary"]
[null,"BILL N0: 08"]
[null,"FINISHES"]
[]
[null,"Note: Rates for tiling shall include for: fixing, bedding, grouting, pointing, finishing and any other similar works to ensure the required finish.Allow for tile adhesive for wall and floor tiling "]
[null," ",null,0]
[8.1,"FLOOR/WALL  FINISHES",null,0]
[]
[{"v":1,"d":"(1)"},"600x600mm matt Porcelain tiles on hall and store  floor ",{"v":21,"d":"21.00"},"m²"]
[]
[{"v":2,"d":"(2)"},"300x300mm matt Hormogenous tiles on shower floor",{"v":18.2,"d":"18.20"},"m²"]
[]
[{"v":3,"d":"(3)"},"300x300mm matt Hormogenous tiles on toilet floor",{"v":2.7,"d":"2.70"},"m²"]
[]
[{"v":4,"d":"(4)"},"300x300mm matt Hormogenous tiles on outdoor entrance floor",{"v":7.1,"d":"7.10"},"m²"]
[]
[{"v":5,"d":"(5)"},"300x450mm  Ceramic tiles on shower wall @ 1.5m",{"v":21,"d":"21.00"},"m²"]
[]
[{"v":6,"d":"(6)"},"300x450mm  Ceramic tiles on toilet wall @ 2.5m",{"v":14,"d":"14.00"},"m²"]
[]
[]
["8.1.1","Tile skirting"]
[null,"Tiles skirting between wall and floor as specified"]
[]
[{"v":1,"d":"(1)"},"Internal walls",{"v":43,"d":"43.00"},"m"]
[]
[8.2,"PLASTERBOARD CONICE/TIMBER BORDER"]
[null,"Supply and installation of plasteredboard  cornice for internal and external should be  75mm x 25mm wooden border  to all edges between walls and ceiling soffits."]
[]
[{"v":1,"d":"(1)"},"Ground floor"]
[null,"Interior",{"v":37.2,"d":"37.20"},"m"]
[null,"Exterior",{"v":5.6,"d":"5.60"},"m"]
[]
[]
[null,"BILL No: 08 - FINISHES"]
[null,"TOTAL OF BILL No: 08 - Carried over to summary"]
[null,"BILL No: 09"]
[null,"HYDRAULICS & DRAINAGE"]
[]
[9.1,"HYDRAULICS "]
[null,"Preamble notes"]
[null,"a) Rates shall include for sockets, running joints, connectors, elbows, junctions, valves, reducers, expansion joints, backnuts and similar, incidental fittings, clips saddles, brackets, straps, hangers, screws, nails and fixing complete, including cuttin"]
[]
[" ","(b) All pipe work and fittings shall be high pressure PVC"]
[null,"(c) Rate shall include for supply and fixing of all pipes"]
[]
["9.1.1","Internal Plumbing"]
[{"v":1,"d":"(1)"},"Internal plumbing to all toilets, washrooms, pantries and work area sinks  incl. supply and laying of pipes.",{"v":1,"d":"1.00"},"item"]
["9.1.2","External Plumbing "]
[{"v":1,"d":"(1)"},"Waste water and sewage connection from all the toilets & lab inc. supply and laying of pipes.",{"v":1,"d":"1.00"},"item"]
[]
[{"v":2,"d":"(2)"},"Waste water and solid waste  connection to Public junction box or Septic tank inc. supply and laying of pipes.",{"v":1,"d":"1.00"},"item"]
[]
["9.1.3","Sanitary Fixtures & Accessories"]
[null,"Sanitary fixtures complete including brackets, stop valves, fittings etc. All sanitary fittings shall be of 'Rapetti' brand or equivalent and all fixtures shall be of 'Duravit' brand or equivalent."]
[]
[]
[{"v":1,"d":"(1)"},"WC suites incl. Flush tank and fittings with well water connection",{"v":1,"d":"1.00"},"nos"]
[{"v":2,"d":"(2)"},"Wash Basins incl. taps and fittings ",{"v":1,"d":"1.00"},"nos"]
[{"v":3,"d":"(3)"},"Water tap",{"v":1,"d":"1.00"},"nos"]
[{"v":4,"d":"(4)"},"Mirror",{"v":1,"d":"1.00"},"nos"]
[{"v":5,"d":"(5)"},"Soap tray",{"v":1,"d":"1.00"},"nos"]
[{"v":6,"d":"(6)"},"Floor drain",{"v":3,"d":"3.00"},"nos"]
[{"v":7,"d":"(7)"},"Paper holder",{"v":2,"d":"2.00"},"nos"]
[{"v":8,"d":"(8)"},"Soap bottole holder",{"v":1,"d":"1.00"},"nos"]
[{"v":9,"d":"(9)"},"movable shower",{"v":1,"d":"1.00"},"nos"]
[{"v":10,"d":"(10)"},"SS sink",{"v":1,"d":"1.00"},"nos"]
[]
[]
[]
[]
[]
[]
["9.1.4","Water Supply"]
[null,"Connecting to pipe work of existing network of supply water.",{"v":1,"d":"1.00"},"item"]
[]
[]
[]
[9.2," DRAINAGE AND WELL SYSTEM"]
[null,"(a) Rates shall include for: excavation, maintaining faces of drain pipe trenches and pits, backfilling, disposal of surplus spoil; bends, junctions, reducers, expansion joints and all joints and other incidental materials."]
[null,"(b) All pipework shall be uPVC"]
[]
["9.2.1","Pipe work"]
[{"v":1,"d":"(1)"},"Allow for supply and installation of  pipework including all the necessary accessories & fittings.",{"v":1,"d":"1.00"},"item"]
["9.2.2","Inspection chambers"]
[{"v":1,"d":"(1)"},"Inspection chambers complete as shown on the drawings incl all pipe connections and similar",{"v":1,"d":"1.00"},"item"]
[]
["9.2.3","Septic tank and Soak pit"]
[{"v":1,"d":"(1)"},"Instalation of all pipe connections to the new sewarage septic tank",{"v":1,"d":"1.00"},"item"]
[]
[]
["9.2.4","Rainwater discharge pipe"]
[{"v":1,"d":"(1)"},"ø 75mm PVC Rainwater down pipe from roof to the sewarage septic tank.",{"v":1,"d":"1.00"},"item"]
{"$rows_empty":36}
[null,"BILL No: 09 - HYDRAULIC AND DRAINAGE"]
[null,"TOTAL OF BILL No: 09 - Carried over to summary"]
[null,"BILL No: 10"]
[null,"PAINTING"]
[null,"Note: (a) Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door window furniture"]
[null,"(b) All painting work shall be carried in accordance with the Specifications",null,0]
[10.1,"WALLS / CONCRETE SURFACES",null,0]
[" ","Nippon or equivalent emulsion paint finish on cement plastered walls and concrete surfaces. Exterior walls should be  weather proof paint.Allow for 1-coats of Alkali Resisting primer on all plastered surface including 1-coat of putty finish before paint on all internal surfaces as described",null," "]
[]
[{"v":1,"d":"(1)"},"Ground floor"]
[null,"Interior",{"v":151,"d":"151.00"},"m²"]
[null,"Exterior",{"v":89,"d":"89.00"},"m²"]
[]
[]
[10.2,"CEILING SURFACES"]
[null,"Nippon or equivalent paint finish on soffits of concrete slab and staircase including application of putty, grinding and sanding as specified"]
[]
[{"v":1,"d":"(1)"},"Ground floor"]
[null,"Interior",{"v":40,"d":"40.00"},"m²"]
[null,"Exterior",{"v":37,"d":"37.00"},"m²"]
{"$rows_empty":10}
[null,"BILL No: 10 - PAINTING"]
[null,"TOTAL OF BILL No: 10 - Carried over to summary"]
[null,"BILL No: 11"]
[null,"ELECTRICAL & SPECIFIC INSTALLATIONS"]
[]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories",null,0]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates for electrical conduits, fittings, equipment and similar items shall include for: all fixings to various building surfaces"]
[null,"(d) Light end and switch end of wiring together measured as one point"]
[null,"(e) A point wiring for power points is measured as one point for each socket outlet; other end of wire is not included in the quantity."]
[null,"(f) Rates shall include for supply and complete installation "]
[null,"(g) Single phase power supply."]
[]
[11.1,"ELECTRICAL BOARDS"]
[null,"Complete installation, including for all connections, earthing, painting, testing and similar of:"]
[null,"Single phase main panel board with connections from the mains including meter, cut-off fuse and other accessories to be located in the panel room at ground floor to electrical engineers specification"]
[]
[]
[]
[]
[{"v":3,"d":"(3)"},"Installation of 6sqmm 2 core  main cable from  existing control panel to proposed building building with GI condute ( approximate length 20m)",{"v":1,"d":"1.00"},"item"]
[]
[]
[11.2,"ELECTRICAL WIRING",null,0]
[null,"Electrical wiring with copper conductor cable in conduits in walls and concrete  as per government regulations including necessary D-boards at each level.",null,0]
[{"v":1,"d":"(1)"},"Wiring to Lighting ",{"v":22,"d":"22.00"},"points"]
[{"v":2,"d":"(2)"},"Wiring to Power outlets and fans",{"v":14,"d":"14.00"},"points"]
[{"v":3,"d":"(3)"},"Wiring to D/B",{"v":1,"d":"1.00"},"item"]
[]
[11.3,"LIGHTING, POWER POINTS & FANS",null,0]
[null,"All lights shall be 'Philips' brand or equivalent, all switches, sockets etc. shall be 'Legrand' brand or equivalent, Air condition system shall be Hitachi or equivalent"]
[]
[{"v":1,"d":"(1)"},"Emergency led light one hour non maintained",{"v":4,"d":"4.00"},"nos"]
[{"v":2,"d":"(2)"},"Ceiling recessed led light",{"v":14,"d":"14.00"},"nos"]
[{"v":3,"d":"(3)"},"1x4' Tube led light",{"v":1,"d":"1.00"},"nos"]
[{"v":4,"d":"(4)"},"Wall mounted  light ",{"v":2,"d":"2.00"},"nos"]
[{"v":5,"d":"(5)"},"Wall mounted  light (weather proof)",{"v":5,"d":"5.00"},"nos"]
[{"v":6,"d":"(6)"},"Ceiling fan with dimmer",{"v":4,"d":"4.00"},"nos"]
[{"v":7,"d":"(7)"},"13 Amp Double Socket outlet",{"v":1,"d":"1.00"},"nos"]
[{"v":8,"d":"(8)"},"13 Amp Double Socket outlet(Weatherproof)",{"v":2,"d":"2.00"},"nos"]
[{"v":9,"d":"(9)"},"13 Amp Single Socket outlet",{"v":6,"d":"6.00"},"nos"]
[{"v":10,"d":"(10)"},"15 Amp Single Socket outlet",{"v":1,"d":"1.00"},"nos"]
[{"v":11,"d":"(11)"},"1 Gang Switch",{"v":1,"d":"1.00"},"nos"]
[{"v":12,"d":"(12)"},"2 Gang Switch",{"v":2,"d":"2.00"},"nos"]
[{"v":13,"d":"(13)"},"3 Gang Switch",{"v":1,"d":"1.00"},"nos"]
[{"v":14,"d":"(14)"},"4 Gang Switch",{"v":1,"d":"1.00"},"nos"]
[{"v":15,"d":"(15)"},"5 Gang Switch",{"v":2,"d":"2.00"},"nos"]
[]
[11.4,"FIRE ALARM & FIGHTING SYSTEM"]
[null,"Provide & install fire fighting equipment inclusive of all necessary connection as per local regulations as described Fire system shall be Apollo brand or equivalent"]
[{"v":1,"d":"(1)"},"CO2 Extinguisher(2kg)",{"v":2,"d":"2.00"},"nos"]
[{"v":2,"d":"(2)"},"Water Extinguisher(9ltr )",{"v":2,"d":"2.00"},"nos"]
[]
[null,"BILL No: 11 - ELECTRICAL"]
[null,"TOTAL OF BILL No: 11- Carried over to summary"]
[null,"BILL No: 12"]
[null,"ROOF TRUSS AND COVER"]
[]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories",null,0]
[]
[12.1,"ROOF FRAMES",null,0]
[" ","Build up timber frames rest on wood plate anchored in roof beam in adherence with the drawing.",null," "]
[]
[{"v":1,"d":"(1)"},"Ridge beam 50 x 150mm",{"v":2.6,"d":"2.60"},"m"]
[{"v":2,"d":"(2)"},"Wooden hip rafters 50 x 150mm  ",{"v":25,"d":"25.00"},"m"]
[{"v":3,"d":"(3)"},"Wooden rafters 50 x 150mm  @900mm c/c",{"v":71,"d":"71.00"},"m"]
[{"v":4,"d":"(4)"},"Wooden battens 38 x 38mm wood purlins @450mm, fully anchored to rafters.",{"v":102,"d":"102.00"},"m"]
[{"v":5,"d":"(5)"},"Wooden fascia board 25 x 250mm",{"v":37,"d":"37.00"},"m"]
[{"v":6,"d":"(6)"},"Painting of the above inclusive of wood treatment.",{"v":1,"d":"1.00"},"item"]
[]
[12.2,"ROOF COVER AND ACCESSORIES"]
[null,"Corrugated  roofing sheets, fixed in accordance to manufacturer's instruction, inclusive of all necessary accessories"]
[]
[{"v":1,"d":"(1)"},"lysaght roofing sheets",{"v":83,"d":"83.00"},"m²"]
[{"v":2,"d":"(2)"},"50mm thk rockwool insulation",{"v":83,"d":"83.00"},"m²"]
[{"v":3,"d":"(3)"},"PVC mesh",{"v":83,"d":"83.00"},"m²"]
[{"v":4,"d":"(4)"},"Lysaght ridge cap",{"v":27.6,"d":"27.60"},"m"]
{"$rows_empty":10}
[null,"BILL No: 12 - ROOF  TRUSS AND COVER "]
[null,"TOTAL OF BILL No: 12 - Carried over to summary"]

{"sheet":" summary ","index":1,"n_rows":44,"n_cols":4,"rows_kept":44,"merged":[[0,1,0,4],[2,4,2,5],[4,4,4,5],[6,4,6,5],[8,4,8,5],[10,4,10,5],[12,4,12,5],[14,4,14,5],[16,4,16,5],[18,4,18,5],[20,4,20,5],[22,4,22,5],[24,4,24,5],[25,4,25,5],[26,4,26,5],[27,4,27,5],[28,4,28,5],[29,4,29,5],[30,4,30,5],[31,4,31,5],[36,4,36,5],[37,4,37,5],[38,4,38,5],[39,4,39,5],[41,4,41,5],[43,4,43,5],[46,1,46,2],[47,1,47,2]],"flags":["formulas_cached_only"]}
[null,"BILL OF QUANTITIES"]
[null,"SUMMARY"]
[]
[{"v":1,"d":"1.0"},"PRELIMINARIES"]
[]
[{"v":2,"d":"2.0"},"EARTH WORKS",null,0]
[]
[{"v":3,"d":"3.0"},"CONCRETE",null,0]
[]
[{"v":4,"d":"4.0"},"MASONRY AND PLASTERING",null,0]
[]
[{"v":5,"d":"5.0"},"METAL/WOOD WORKS"]
[]
[{"v":6,"d":"6.0"},"CEILING WOKS"]
[]
[{"v":7,"d":"7.0"},"DOORS AND WINDOWS"]
[]
[{"v":8,"d":"8.0"},"FINISHES"]
[]
[{"v":9,"d":"9.0"},"HYDRAULICS & DRAINAGE"]
[]
[{"v":10,"d":"10.0"},"PAINTING"]
[]
[{"v":11,"d":"11.0"},"ELECTRICAL & SPECIFIC INSTALLATIONS"]
[]
[{"v":12,"d":"12.0"},"ROOF TRUSS AND COVER"]
{"$rows_empty":10}
[" "," ",null,0]
[null," SUB TOTAL "]
[null," GST  6%"]
[null," GRAND TOTAL"]
[]
[null,"DURATION IN DAYS"]
[]
[null,"VALIDITY PERIOD IN DAYS"]

{"sheet":"cover","index":2,"n_rows":31,"n_cols":2,"rows_kept":31,"merged":[[6,0,6,5],[7,0,7,5],[8,0,8,5],[9,0,9,5],[10,0,10,5],[11,0,11,5],[12,0,12,5],[13,1,13,4],[15,1,15,4],[16,0,16,5],[17,0,17,5],[18,0,18,5],[19,0,19,5],[20,0,20,5],[22,0,22,5],[23,0,23,5],[25,0,25,5],[27,0,27,5],[28,0,28,5],[29,0,29,5]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[]
["BILL OF QUANTITIES"]
[]
[]
["PROJECT TITILE"]
[]
["PROPOSED  SINGLE STOREY  BUILDING"]
[]
[]
[]
[null,"MALE' "]
[]
["REPUBLIC OF MALDIVES"]
[]
[]
["2017-05-15"]
[]
[]
[]
["Quantity Surveyor"]
["Name: M.Shareef                                                 "]
[]
["Email: m.shareef90@gmail.com"]
["ContactNo: +960 7993433"]
["Email: mohamed.shareef@fenaka.com.mv"]
["BSc (Hons) Quantity Surveying and Construction Management"]