{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["COVER SHEET","BoQ"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[1,0,1,11]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES "]
[]
[{"$nulls":10},"AEH WALK WAY REPAIR & RENOVATION (ISO)"]
[]
[{"$nulls":10},"S. HITHADHOO"]

{"sheet":"BoQ","index":1,"n_rows":90,"n_cols":8,"rows_kept":90,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,7,5,7]],"flags":["formulas_cached_only"]}
["BILL OF QUANTITIES"]
["AEH WALK WAY REPAIR & RENOVATION (ISO)"]
["S. HITHADHOO"]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 1"]
[null,"ROOFING"]
[]
[1.1,"General"]
[null,"(a) Rates shall include for: fair edges, dressing over angel fillets, turning into grooves, all other labours, circular edges, nails, screws and other fixings and laps."]
[null,"(b) Rates shall include to apply Wood preservative to  all the surface of timbers (Roof structure)."]
[]
[1.2,"Roof Coverings"]
[{"v":1,"d":"(1)"},"Roofing sheets: Blue scope steel international limited MSP- Aqua marine or equivalent for Main building and connection area.","m²",{"v":35.2,"d":"35.20"}]
[]
[1.3,"Capping and Flashings"]
[{"v":1,"d":"(1)"},"Ridge Capping:  Blue scope steel international limited MSP- Aqua marine or equivalent","m",9.75]
[{"v":2,"d":"(2)"},"Flasing: Blue scope steel international limited MSP- Aqua marine or equivalent","m",7.11]
[1.4,"Gutter"]
[null,"(a) MSP Colorbond flat sheet gutter including framing, and supports, straps, brackets, clips, stop ends, overflow, downpipe outlets, mesh flashings and all fixings and fastenings."]
[{"v":1,"d":"(1)"},"GUTTER: Blue scope steel international MSP- Aqua marine or equivalent ","m",19.51]
[]
[1.5,"Down Pipes"]
[{"v":1,"d":"(1)"},"50mm dia uPVC down pipes including bends,  straps, brackets, clips, roof drain strainer and all fixings.","m",{"v":18,"d":"18.00"}]
[]
[]
[1.6,"Roof Structure"]
[{"v":1,"d":"(1)"},"(a) Rates shall include for: all labour in framing, notching and fitting around projections, pipes, light fittings, hatches, grilles and similar and complete with cleats, packers, wedges and similar and all nails and screws."]
[]
[{"v":1,"d":"(1)"},"50 X 150mm timber rafters ","m",{"v":42,"d":"42.0"}]
[{"v":2,"d":"(2)"},"50 X 50mm timber purling ","m",{"v":58,"d":"58.0"}]
[{"v":3,"d":"(3)"},"50 X 150mm timber beam","m",{"v":29,"d":"29.0"}]
[{"v":4,"d":"(4)"},"Timber fascia board 25 X 250mm","m",{"v":19.51,"d":"19.5"}]
[]
[]
[]
[null,"BILL No: 2"]
[null,"CEILINGS"]
[]
[2.1,"Exterior Ceilings"]
[null,"Exterior ceiling consist of 4 mm thick Cement plaster board suspended ceiling, including framing beading nails and screws. Grid of the frame to be 600 X 600 with timber supports to roof structure at every 1200 mm on the main entrance ceiling & 600X900 mm at eaves of roof ceiling, timber framing and supports shall  50 x 50mm size shall be seasoned red meranti timber"]
[]
[{"v":1,"d":"(1)"},"Exterior Ceiling ","m²",28.42]
[]
[null,"BILL No: 3"]
[null,"PAINTING"]
[]
[]
[null,"Exterior & Exterior Ceiling  (interior and exterior) shall be of 2 coats of (bodelac 9000) high gloss wood paint over 1 coat of wood primer (bodelac 9000 undercoat) or equivalent. Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for the provision and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and or masking pavement bricks and walkway tiles."]
[null,"All painting work shall be carried in accordance with the Specifications"]
[3.1,"Ceiling painting"]
[{"v":1,"d":"(1)"}," Exterior Ceiling painting","m²",28.42]
[{"v":2,"d":"(2)"},"Panting Colums","Item",{"v":1,"d":"1.00"}]
[]
[]
[]
[]
[null,"BILL No: 4"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[4.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each Light/ light fixture and its switch is measured as one one point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[]
[]
[]
[4.2,"Electrical wiring"]
[null,"Three phase Electrical wiring with copper conductor cable in conduits in walls and in casing on soffits of slab as specified to:"]
[{"v":1,"d":"(1)"},"Wiring with 2.5 mm² cable to lights ","points",{"v":10,"d":"10.00"}]
[]
[4.3,"Lighting "]
[{"v":1,"d":"(1)"},"Ceiling Recessed Led Down Light 250mm dia, 13W LED  ,  ","no",{"v":10,"d":"10.00"}]
[]
[]
[null,"BILL No: 11 - ELECTRICAL INSTALLATIONS"]
[null,"TOTAL OF BILL No: 11 - Carried over to summary"]
[]
[]
[null,"BILL No: 5"]
[null,"RENOVATION WORKS"]
[]
[12.1,"General"]
[null,"(a) Rates shall include for completion of works as per drawings. "]
[]
[12.2,"Clading"]
[{"v":1,"d":"(1)"},"Remove & Re-fix aluminum composite panels PVC cladding system , as per specified in the  drawing.","Item",{"v":1,"d":"1.00"}]