{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[1,0,1,11],[6,5,6,9]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES"]
[]
[{"$nulls":10},"Partition Works at Fifth Floor Meeting Room and IT DDG Room Area"]
[]
[{"$nulls":10},0]

{"sheet":"SUMMARY","index":1,"n_rows":16,"n_cols":5,"rows_kept":16,"merged":[[1,0,1,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITY"]
["Partition Works at Fifth Floor Meeting Room and IT DDG Room Area"]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01",0]
[2,null,"ALUMINIUM FRAME GLASS PARTITION WORKS","Bill no. 02",0]
[3,null,"DOORS","Bill no. 03",0]
[4,null,"DRY WALL PARTITION WORKS","Bill no. 04",0]
[5,null,"TENDERER'S ADJUSTMENTS","Bill no. 05",0]
[null,null,"Sub total",null,0]
[null,null,"GST 8%",null,0]
[]
[]
[null,null,"GRAND TOTAL carried to form of bid",null,0]

{"sheet":"BoQ","index":2,"n_rows":104,"n_cols":8,"rows_kept":104,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,7,5,7]],"flags":["formulas_cached_only"]}
[" BILL OF QUANTITIES"]
["Partition Works at Fifth Floor Meeting Room and IT DDG Room Area"]
[]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"," "]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[1.2,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","Item",{"v":1,"d":"1.00"}]
[]
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"ALUMINIUM FRAME GLASS PARTITION WORKS"]
[]
[2.1,"General"]
[null,"(a) Rate shall include supply, fabrication, delivery, installation, transport, labour, scaffolding (if required), sealant works, finishing, and all necessary accessories."]
[null,"(b) Rates shall include for design, supply, and installation."]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position."]
[null,"(d) All materials must be submitted to and approved by the project manager before installation."]
[null,"(e) Contractor shall verify all site dimensions prior to fabrication."]
[]
[2.2,"Aluminium Framed Glass Partition Walls"]
[null,"(a) Specification of the glass partitions/panels shall be as follows;\n-6mm thick glass, single-glazed:\n   *Frost sticker to be applied on crystal-clear glass panels up to 1100mm from finished floor level (FFL).\n   *Crystal-clear glass panels from 1100mm to 2470mm height.\n-All exposed edges of glass panels shall be polished to remove sharp corners and burrs."]
[null,"(b) Specification of the aluminium frames shall be as follows;\n-The aluminium framing shall be fabricated from aluminium alloy 6063 T5 extruded sections.\n-The frame shall be made of 2\" x 1.5\" aluminium sections with 1.2mm thickness all around.\n-Vertical members shall be at max distance of 1200mm (preferable) centre-to-centre. \n-Horizontal members shall be at 1100mm (preferable) from finished floor level and at ceiling level (full height ~2470mm).\n-Aluminium cleats/brackets shall be provided at the junctions for securing the frames firmly.\n-The joints between aluminium members shall be mechanically joined using cleats and self tapping screws.\n-The frames shall be aligned in perfect plane & right angle to ensure flawless installation of glass.\n-Rubber/PVC beading gaskets shall be provided all around the glass to prevent any damage during transportation or installation.\n-The exposed aluminium surface shall be anodized in natural matt finish or powder coated (black color) as per approval."]
[null,"(c) The contractor shall provide Project Manager with a drawing of the walls before commencing the work, which should show the horizontal and vertical aluminium frames along with the dimensions. Also, the approval of the Project Manager shall be obtained for the drawings before initiating the work."]
[{"v":1,"d":"(1)"},"Design, supply and installation of aluminium-framed single-glazed 6mm thick glass partitions:\n-Meeting Room (Height = ~2470mm)","sqft",{"v":95,"d":"95.00"}]
[{"v":2,"d":"(2)"},"Design, supply and installation of aluminium-framed single-glazed 6mm thick glass partitions:\n-IT Deputy Director General (DDG) Room - One Side (Height = ~2470mm) ","sqft",{"v":91.8,"d":"91.80"}]
[{"v":3,"d":"(3)"},"Design, supply and installation of aluminium-framed single-glazed 6mm thick glass partitions:\n-IT Deputy Director General (DDG) Room - Second Side (Height = ~2470mm)","sqft",12.75]
[null,"BILL No: 02 - ALUMINIUM FRAME GLASS PARTITION WORKS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL N0: 03"]
[null,"DOORS"]
[]
[3.1,"General"]
[null,"(a) Rates shall include for all materials, fittings, tools, accessories, labor, and other expenses to complete the entire work."]
[null,"(b) Rates shall include for design, supply, and installation."]
[null,"(c) Rates shall include for fabrication and erection of temporary supports and fixing into position."]
[null,"(d) All materials must be submitted to and approved by the project manager before installation."]
[null,"(e) The door shall be made of 6mm thick clear glass fixed in aluminium frame of 2\" x 1.5\" sections."]
[null,"(f) The aluminium frame shall have brushed finish. Horizontal members shall be provided at top and bottom of the door."]
[null,"(g) A lever-handle stainless steel door lock shall be fixed that could be locked from both sides."]
[null,"(h) A hydraulic door closer shall be fixed that could be adjustable."]
[null,"(i) Door stoppers shall be provided on the head to prevent the handles hitting the wall."]
[null,"(j) The contractor shall provide Project Manager with a drawing of the doors before commencing the work, which should show the horizontal and vertical aluminium frames along with the dimensions. Also, the approval of the Project Manager shall be obtained for the drawings before initiating the work."]
[]
[3.2,"Aluminium Framed Glass Door"]
[{"v":1,"d":"(1)"},"Design, supply & installation of aluminium framed glass door including all the hardware/fittings:\n-Meeting Room - Single Door, ~800mm x 2100mm (L x H)","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Design, supply & installation of aluminium framed glass door including all the hardware/fittings:\n-IT Deputy Director General (DDG) Room - Single Door, ~800mm x 2100mm (L x H)","no",{"v":1,"d":"1.00"}]
[]
[null,"BILL N0: 03 -  DOORS"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No: 4"]
[null,"DRY WALL PARTITION WORKS"]
[]
[4.1,"General"]
[null,"(a) Contractor shall verify site dimensions before fabrication."]
[null,"(b) All materials to be new and free from defects."]
[null,"(e) Rates shall include for supply and complete installation (with own materials and labor)"]
[]
[4.2,"Dry wall partition work"]
[null,"Timber Framing:-\n(a) Timber shall be seasoned and treated against termite and moisture attack.\n(b) Vertical studs minimum size: 2” × 3” treated timber.\n(c) Vertical studs spacing: Maximum 400mm (preferable) centre-to-centre.\n(d) Horizontal members to be provided:\n           -At top and bottom plates.\n           -At mid-height level.\n(e) Reinforced double horizontal member at proposed TV mounting height.\n(f) Additional internal 18mm plywood backing board to be fixed at TV mounting location for secure anchoring of bracket.\n(g) Frame shall be securely anchored to floor, adjoining wall and ceiling.\n(h) Partition shall be capable of supporting minimum 60kg point load at TV mounting location."]
[null,"Board Cladding (Front Side Only):-\n(a) 12mm gypsum board or 12mm plywood (as approved).\n(b) Only visible front side to be clad.\n(c) Back side to remain open (timber framing exposed).\n(d) Proper screw fixing at recommended spacing.\n(e) Joints aligned and surface prepared ready for painting\n(f) Application of putty, sanding, and paint works to be done by contractor"]
[{"v":1,"d":"(1)"},"Supply & construction of timber-framed drywall partition (with paint works) for TV mounting","sqft",{"v":64.4,"d":"64.40"}]
[]
[null,"BILL No: 4 - DRY WALL PARTITION WORKS"]
[null,"TOTAL OF BILL No: 4 - Carried over to summary"]
[null,"BILL No:5"]
[null,"TENDERER'S ADJUSTMENTS"]
[5.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[5.2,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"ALUMINIUM FRAME GLASS PARTITION WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"DOORS, Bill no. 03"]
[{"v":4,"d":"(4)"},"DRY WALL PARTITION WORKS, Bill no. 04"]
[null,"ADDITIONS TOTAL"]
[]
[5.3,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"ALUMINIUM FRAME GLASS PARTITION WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"DOORS, Bill no. 03"]
[{"v":4,"d":"(4)"},"DRY WALL PARTITION WORKS, Bill no. 04"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 5 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 5 - Carried over to summary"]