{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":5,"n_cols":11,"rows_kept":5,"merged":[[1,0,1,11]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES "]
[]
[{"$nulls":10},"REMAINING WORKS OF K. HIMMAFUSHI HEALTH CENTER"]

{"sheet":"SUMMARY","index":1,"n_rows":23,"n_cols":5,"rows_kept":23,"merged":[[1,0,1,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITIES"]
["REMAINING WORKS OF K. HIMMAFUSHI HEALTH CENTER"]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01"]
[2,null,"GROUND  WORKS","Bill no. 02"]
[3,null,"CONCRETE","Bill no. 03"]
[4,null,"MASONRY AND PLASTERING","Bill no. 04"]
[5,null,"ROOFING","Bill no. 05"]
[6,null,"DOORS AND WINDOWS","Bill no. 06"]
[7,null,"TILING","Bill no. 07"]
[8,null,"CEILINGS","Bill no. 08"]
[9,null,"PAINTING","Bill no. 09"]
[10,null,"ELECTRICAL INSTALLATIONS","Bill no. 10"]
[11,null,"HYDRAULICS & DRAINAGE","Bill no. 11"]
[12,null,"TENDERER'S ADJUSTMENTS","Bill no. 12"]
[13,null,"AIR CONDITIONING WORKS","Bill no. 13"]
[null,null,"Sub total"]
[null,null,"GST 6%"]
[]
[null,null,"GRAND TOTAL carried to form of bid"]

{"sheet":"BoQ","index":2,"n_rows":446,"n_cols":8,"rows_kept":446,"merged":[[5,0,5,7],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,7,8,7]],"flags":["formulas_cached_only"]}
["BILL OF QUANTITIES"]
["REMAINING WORKS OF K. HIMMAFUSHI HEALTH CENTER"]
["K. HIMMAFUSHI ISLAND"]
[]
[]
["BILL OF QUANTITIES"]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"," "]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[]
[1.2,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","Item",{"v":1,"d":"1.00"}]
[]
[1.3,"INSPECTION TRIPS"]
[{"v":1,"d":"(1)"},"Arrange inspection trip to PMU team.\nContractor has to arrange following for trips;\n(a) Speed boat ticket from Male' city/K. Himmafushi/Male' City.\n(b) Accommodations (2 Air-condition room) per trip for 2 nights at guest house.","Item",{"v":4,"d":"4.00"}]
[]
[]
[]
[]
[]
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"GROUND  WORKS"]
[]
[2.1,"General"]
[null,"(a) Rates shall include for: leveling, grading, trimming, compacting to faces of excavation, keep sides plumb, backfilling, consolidating and disposing surplus soil."]
[]
[2.2,"Site Clearing"]
[{"v":1,"d":"(1)"},"Includes clearing of all trees and bushes complete with stems, roots, Flooring, and the reimbursement fees if applicable. The contractor is to advised to survey the construction site and ensure that all necessary works for site clearing are included and on completion of works.\nRates must include diverting all the pipes laid underground within the new building area (Sewer, wastewater, freshwater line and inspection chambers).Also, reallocate all AC outdoor units installed with the new building area.","Item",{"v":1,"d":"1.00"}]
[]
[]
[2.3,"Damp Proof Membrane"]
[null,"Cutting and laying in position heavy duty polythene sheets of gauge 500 (not less than 1.5mm thick). Rates shall include for: dressing around and sealing to all penetrations. Apply slurry type waterproofing to all surfaces of concrete below ground level in accordance with manufacturer's instructions."]
[{"v":2,"d":"(2)"},"Damp proof membrane below floor slab, Detanl room and Ramp area","m²",12.17]
[]
[]
[null,"BILL No: 02 - GROUND WORKS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"CONCRETE"]
[3.1,"General"]
[null,"Rates shall include for cleaning, fabrication, placing, the provision for all necessary temporary fixings and supports including tie wire and other supports, laps and wastage, all reinforcement bars except 6 mm dia bars shall be of deformed high strength bars. 6 mm bar shall be round mild steel bars. Binding wire shall be of 1.6 mm or 1.4 mm soft iron wire.\nReinforcement bars shall be cleaned before use i.e. should be free from rust, oil, din, or other coatings that reduces bonds, all reinforced bars and binding wires shall be stored under cover of at least 450 mm above the ground, cutting and bending according to approved manner & the approved working drawing, placing and fixing in position and binding should be as per the approved working drawing, laps in the bars shall be staggered, concrete cover for reinforcement shall not less than 50 mm for substructure, 40 mm for columns & side beams  and not more than 30 mm for slab and beam bottoms.  \nDesalinated water shall be used for all purposes, ground water shall not be used."]
[]
[3.2,"Reinforced Concrete"]
[null,"In-situ reinforced concrete to:"]
[null,"*Add water proofing compound / admixture to concrete mix for walls GL and Roof Slabs"]
[]
["3.2.1","Ground Floor"]
[{"v":1,"d":"(1)"},"RCC Ground Slab 100 mm thick,  (Dental room, Toilet area and ramp area)","m³",3.15]
[]
[3.3,"Reinforcement"]
[null,"GENERAL : Rates shall include for cleaning, fabrication, placing, the provision for all necessary temporary fixings and supports including tie wire and other supports, laps and wastage, all reinforcement bars except 6 mm dia bars shall be of deformed high strength bars. 6 mm bar shall be round mild steel bars. Binding wire shall be of 1.6 mm or 1.4 mm soft iron wire.\nReinforcement bars shall be cleaned before use i.e. should be free from rust, oil, din, or other coatings that reduces bonds, all reinforced bars and binding wires shall be stored under cover of at least 450 mm above the ground, cutting and bending according to approved manner & the approved working drawing, placing and fixing in position and binding should be as per the approved working drawing, laps in the bars shall be staggered, concrete cover for reinforcement shall not less than 50 mm for substructure, 40 mm for columns & side beams  and not more than 30 mm for slab and beam bottoms. "]
[null,"(b) All reinforcing bars shall be high strength bars."]
[]
["3.3.1","Floor Slab"]
[{"v":1,"d":"(1)"},"10 mm dia bars @300 C/C, For ground slab including ramp area","bars",{"v":38,"d":"38.00"}]
[]
[3.4,"OTHER CONCRETE WORKS"]
[]
[{"v":1,"d":"(1)"},"Fabrication of Concrete sink cupboard at at proposed Laboratory, 7.125 Meter length and 600mm width as per Drawings, Rates includes, concrete works tiling of  all surfaces,installation of two ceramic laboratory sink 620x480x255mm, (Cotto or equivalent)with an wall mount elbow operated faucet. And Rates shall also include connecting fresh water, waste water related to this item. Also, rates shallinclude fixing the timber door panel and shelves with PVC role fomica on allsurfaces.  Granite sheet to be laid on top of the Sink cupboard. 12mm thick plywood to use for door panels of the cupboard with both side Formica,","Item",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Fabrication of Concrete sink cupboard at at Room 1, 3.828 Meter length and 600mm width as per Drawings, Rates includes, concrete works tiling of  all surfaces,installation of ceramic laboratory sink 620x480x255mm, (Cotto or equivalent)with an wall mount elbow operated faucet. And Rates shall also include connecting fresh water, waste water related to this item. Also, rates shallinclude fixing the timber door panel and shelves with PVC role fomica on allsurfaces.  Granite sheet to be laid on top of the Sink cupboard. 12mm thick plywood to use for door panels of the cupboard with both side Formica,","Item",{"v":1,"d":"1.00"}]
[]
[]
[null,"BILL No: 03 - CONCRETE WORKS"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No: 04"]
[null,"MASONRY AND PLASTERING"]
[]
[4.1,"General"]
[null,"Rates shall include for: cleaning out cavities, forming rebated reveals and pointing and cleaning down to reveals where necessary; fractional size blocks, all necessary machine cutting, cutting or forming chases or edges of \nfloor slabs, cutting or leaving holes and openings as recesses for and building in pipes, conduits, sleeves and similar as required for all trades; leaving surfaces rough or raking out joints for plastering and flashings, bedding\nframes or plates, building in joists, bearers or similar, temporary supports to openings, templates, reinforcement in walls and for all necessary making good.\nBedding mortar (mixing ratio 1:4 i.e. cement: manufactured sand) shall be of OPC & fine aggregate shall be imported river sand shall be approved in grading & clean from any harmful substance.\nMasonry work shall be done with approved Machine compact cement blocks (300X150X150) with no defects. Lay in line and length as per approved working drawing\nBlock making (mixing ratio 1:5 i.e. cement: Local sand) shall be of OPC & free form salt."]
[null,"floor slabs, cutting or leaving holes and openings as recesses for and building in pipes, conduits, sleeves and similar as required for all trades; leaving surfaces rough or raking out joints for plastering and flashings, bedding "]
[null,"Rates shall include for: 25mm groove lines on external surfaces as shown on the drawing."]
[]
[4.2,"Cement block work"]
[null,"External and external walls"]
["4.2.1","200mm wide machine compress Hollow blocks, laid on and incl. 1:5 Cement Mortar, tie rods, compression gap filler, nylon / plastic mesh as specified."]
[{"v":1,"d":"(1)"},"Ground Floor (internal walls)","m²",46.74,null,null,0,0]
[]
[4.3,"Plastering"]
[]
[null,"GENERAL: Interior and Exterior:  Plaster All masonry wall have smooth finishing of 18 mm thick cement plastering with mix ratio 1:4 (i.e. cement: River Sand), plastering material shall be of OPC & fine aggregate shall be imported river sand shall be approved in grading & clean from any harmful substance. Plastic net should be provided wherever concrete surface and masonry meets, and cracks are unacceptable. Regular curing up to 7 days must be done, edges of doors, windows and ventilators included."]
[]
["4.3.1","25mm thick cement plastering (2 coat) on external walls and 18mm thick cement plastering on internal walls and concrete surfaces with 1:4 Cement mortar mix as specified incl. wire mesh at joints of concrete surfaces and walls (first, second coats)."]
[{"v":1,"d":"(1)"},"Ground floor ( new walls and old walls).","m²",{"v":128,"d":"128.00"}]
[]
[4.4,"Cement Screed Finish"]
["4.4.1","50mm thick Cement screeding on the"]
[null,"concrete floor with 1:4 cement mortar"]
[null,"mix incl. trowel finish; General Areas"]
[{"v":1,"d":"(1)"},"Ground Floor","m²",{"v":165,"d":"165.00"}]
[]
[4.5,"Dry wall partition"]
[null,"125mm thick dry wall partition, Timber frame with 9mm thick Shera board on bothside, Rates includes to fabricate the timber frame as per consultants instructions as well as puttying and Anti bacterial and washable paint on both side and etc. 100X50mm vertical member at 600mm c/c and 100X50mm Horizontal member at 600mm c/c. Rates also includes to apply Solignum wood presavative for all the surfaces of timber frame."]
[{"v":1,"d":"(1)"},"Partition wall , up to the ceiling. ","m²",{"v":62,"d":"62.00"}]
[]
[]
[]
[]
[null,"BILL No: 04 - MASONRY AND PLASTERING"]
[null,"TOTAL OF BILL No: 04 - Carried over to summary"]
[null,"BILL No: 05"]
[null,"ROOFING"]
[]
[5.1,"General"]
[null,"(a) Rates shall include for: fair edges, dressing over angel fillets, turning into grooves, all other labors, circular edges, nails, screws and other fixings and laps."]
[null,"(b) Rates shall include to apply Wood preservative to  all the surface of timbers (Roof structure)."]
[null,"(b) Rates shall include to remove existing end cap, fascia board and necessary roofing sheets and necessary works to connect new roof to existing roof. "]
[]
[]
[]
[5.2,"Gutter"]
[null,"(a) MSP Color bond flat sheet gutter 200X200mm, Total coated thickness minimum 0.47mm thick,  including framing, and supports, straps, brackets, clips, stop ends, overflow, downpipe outlets, mesh flashings and all fixings and fastenings."]
[{"v":1,"d":"(1)"},"GUTTER: Blue scope steel international MSP- Aqua marine or equivalent ","m",{"v":25,"d":"25.00"}]
[]
[5.5,"Down Pipes",{"$nulls":4},0,0]
[{"v":1,"d":"(1)"},"75 mm dia uPVC down pipes including bends, junctions, straps, brackets, clips, roof drain strainer and all fixings.","m",{"v":30.6,"d":"30.60"},null,null,0,0]
[{"$nulls":6},0,0]
[]
[5.7,"Roof Structure"]
[null,"(a) Rates shall include for: all labour in framing, notching and fitting around projections, pipes, light fittings, hatches, grilles and similar and complete with cleats, packers, wedges and similar and all nails and screws.\n(b) Rates includes to applying solignam wood preservative oil to all the surface of roof structure.\n(c) Rates include to fixing galvanized bolt with washers and nuts as show on the drawings."]
[{"v":1,"d":"(1)"},"Fascia board 18 X 250mm (Shera board to be used)","m",{"v":43,"d":"43.00"}]
[{"v":2,"d":"(2)"},"Aligh the roof structure","item",{"v":1,"d":"1.00"}]
[]
[5.8,"Supplying and installation of Furniture"]
[null,"Supply and Complete installation of Furniture's."]
[{"v":1,"d":"(1)"},"Office Table with partition, 1200mm ( table should be solid wood).","No",{"v":4,"d":"4.00"}]
[{"v":2,"d":"(2)"},"Secretary chair , high back.","No",{"v":8,"d":"8.00"}]
[{"v":4,"d":"(4)"},"Secretary chair , Low back.","No",{"v":8,"d":"8.00"}]
[{"v":5,"d":"(5)"},"Supply and installation of 3 seater Airport Bench set, Armrest/Leg/bracket: Die-casting molding of high strength aluminum alloy. \nSeat: Numerical control hydraulic molding of high quality cold rolling steel plate. \nSponge: Cold consolidation and foam-forming of high density and super soft PU. \nBeam: metal tube with a diamond shape. \nCoating: Electrostatic coating after Rust-proof treatment, electroplated polishing.  ","No",{"v":8,"d":"8.00"}]
[]
[5.9,"Casing of Column"]
[{"v":1,"d":"(1)"},"Boxing of existing column at center of Office area as per drawing, ","Item",{"v":2,"d":"2.00"},null,null,0,0]
[]
[]
[null,"BILL No: 05 - ROOFING"]
[null,"TOTAL OF BILL No: 05 - Carried over to summary"]
[null,"BILL N0: 06"]
[null,"DOORS AND WINDOWS"]
[]
[6.1,"General"]
[null,"Timber doors, Fabricate the doorframes and door panel to specified size using recommended timber fix same and other fittings such as locks etc. wood Paint specified and shown in approved working drawings and installation should be as per technical specifications.\nRates shall include for locks (i.e. security lock & dead lock), latches, closures, push plates, pull handles, bolts, kick plates hinges, screws, washer and all door and window hardware and these materials should be of ss steel according to drawing and of superior quality."]
[null,"Aluminum Doors and windows, Fabricate and fix in position the aluminum doors and window frame  - aluminum doors and window (white powder coated, 60-80 micron, 1.5mm profile thickness) using recommended material with specified fixtures as shown in approved working drawings and installation should be as per technical specifications. Rates shall include for locks, latches, closures, push plates, pull handles, bolts, kick plates hinges, screws, washer and all door and window hardware and these materials should be of ss steel according to drawing and of superior quality."]
[null,"(a) All door and window frames and panels shall be as specified in the drawing and timber boarder to be fixed all timber doors."]
[null,"(b) All glazing shall be 6mm  Tinted."]
[null,"(Profiles to be chosen by client, profile thickness mush me minimun 2.5mm thick)."]
[]
[]
[6.2,"Door / Windows units"]
[]
[{"v":1,"d":"(1)"},"D1A,  Minimum 80 Micron Aluminum, Dark sandy grey powder coated Door 2150X1800mm with panels as per drawings. ","no",{"v":2,"d":"2.00"}]
[{"v":2,"d":"(2)"},"D2, Minimum 80 Micron Aluminum, Dark sandy grey powder coated Door 2150X1000mm with panels as per drawings. ","no",{"v":3,"d":"3.00"}]
[{"v":3,"d":"(3)"},"D3, Minimum 80 Micron Aluminum, Dark sandy grey powder coated Door 2150X1350mm with panels as per drawings. ","no",{"v":2,"d":"2.00"}]
[{"v":4,"d":"(4)"},"D4, Minimum 80 Micron Aluminum, Dark sandy grey powder coated Door 2150X1000mm with panels as per drawings. ","no",{"v":1,"d":"1.00"}]
[{"v":5,"d":"(5)"},"W1, Aluminum 60-80 Micron, white powder coated window 1700x1300mm with panels as per drawings ","no",{"v":10,"d":"10.00"}]
[]
[6.3,"Registration counter"]
[{"v":1,"d":"(1)"},"Design and Fabrication of Registration counter, length of Counter would be 3 meter with 3 drawer  Fabrication of counter to be timber and appropriate thick plywood with PVC  fomica.","Item",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Design and Fabrication of  lab counter, length of Counter would be 1 meter with 3 drawer  Fabrication of counter to be timber and appropriate thick plywood with PVC  fomica.","Item",{"v":1,"d":"1.00"}]
[]
[6.4,"BED SIDE CURTAINS"]
[null,"Supply and complete installation of top quality Hospital grade bed side curtain including railing/Track. Length of rail/track is 6870mm, and height of curtain would be 2.4 meter. Please check the ceiling height before ordering curtains."]
[{"v":1,"d":"(1)"},"General ward and OPD rooms","Item",{"v":6,"d":"6.00"}]
[]
[6.5,"Vertical Blinds"]
[null,"Supply and installation of Vertical Blinds for following windows, quality of vertical blinds should be high quality sun protected , Rates should be complete installation of Vertical blinds with railing and ect.."]
[{"v":1,"d":"(1)"},"W1 windows , size of finished blinds should be 1.0m height, X1.4meter width.","No",{"v":10,"d":"10.00"}]
[]
[]
[null,"BILL N0: 06 -  DOORS AND WINDOWS"]
[null,"TOTAL OF BILL No: 06 - Carried over to summary"]
[null,"BILL N0: 07"]
[null,"TILING"]
[]
[7.1,"General"]
[null,"Prepare surface for approved bedding tiles with reach bedding materials as per the technical specifications & approved working drawings, fix tiles with ct grout in a precise manner to maintain correct alignment, applying tile grout and wiping any excess grout to ensure the required standards of finished works.\nRates shall include for: fixing, bedding, grouting, and pointing materials; making good around pipes, sanitary fixtures, and similar; cleaning down and polishing any other similar works to ensure the required finish.\nAll tiles shall be Full body homogeneous tiles or equivalent."]
[]
[7.2,"Floor finish"]
[]
["7.2.1","600x600 skid resistant full body homogeneous mat finish floor tiles, "]
[{"v":1,"d":"(1)"},"General area flooor tilling,","m²",{"v":159,"d":"159.00"}]
[{"v":2,"d":"(2)"},"Toilet area floor tilling. With Water proofing membrane, approved by the Client.","m²",{"v":7.2,"d":"7.20"}]
[{"v":3,"d":"(3)"},"Ramp area and front steps (office entrance)","m²",{"v":13.9,"d":"13.90"}]
[{"v":4,"d":"(4)"},"Tile Skirting 150mm high for all walls.","Item",{"v":1,"d":"1.00"}]
[]
[7.3,"Wall finish"]
["7.3.1","300x600 mm full body homogeneous wall tile,"]
[{"v":1,"d":"(1)"},"Public Toilet,  2.4 meter from floor finish level, With Water proofing membrane, approved by the Client.","m²",{"v":24.5,"d":"24.50"}]
[{"v":2,"d":"(2)"},"Laboratory,  2.4 meter from floor finish level, With Water proofing membrane, approved by the Client.","m²",{"v":56.2,"d":"56.20"}]
[]
[null,"BILL No: 7 - TILING"]
[null,"TOTAL OF BILL No: 7 - Carried over to summary"]
[null,"BILL No: 8"]
[null,"CEILINGS"]
[]
[8.1,"Interior Ceilings"]
[null,"Interior ceiling consist of  50X50mm Timber frame  @ 1200mm c/c vertical and 600mm c/c horizontal rame with 6mm thick Gypsum board suspended ceiling, including framing beading nails and screws as per manufactures instruction."]
[null,"Interior ceiling consist of  50X50mm Timber frame  @ 1200mm c/c vertical and 600mm c/c horizontal rame with 6mm thick Gypsum board suspended ceiling, including framing beading nails and screws as per manufactures instruction."]
[{"v":1,"d":"(1)"},"Ground floor","m²",{"v":166,"d":"166.00"}]
[]
[8.2,"Exterior Ceilings"]
[null,"Exterior ceiling consist of 6mm thick Shera board suspended ceiling, including framing beading nails and screws. Grid of the frame to be 600 X 600 with timber supports to roof structure at every 1200 mm on the main entrance ceiling & 600X900 mm at eaves of roof ceiling, timber framing and supports shall  50 x 50mm size shall be seasoned red meranti timber as per given drawing."]
[{"v":1,"d":"(1)"},"Ground floor","m²",{"v":39.6,"d":"39.60"}]
[]
[]
[]
[null,"BILL N0: 8 CEILINGS"]
[null,"TOTAL OF BILL No:8 - Carried over to summary"]
[null,"BILL No: 09"]
[null,"PAINTING"]
[]
[9.1,"General"," "]
[null,"Exterior wall shall be of 1 coat of oil based textured paint and 2 coats of Kansani weather bond paint ( oil based ) over 1 coat of oil based sealer ( white) or equivalent (according to technical specifications or approved drawings). Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window and including soffits and sides of beams. "]
[null,"Interior wall shall be of 2-3 coats over 1 coat of water based sealer. Rates includes Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window and including soffits and sides of beams."]
[]
[null,"Exterior & Exterior Ceiling  (interior and exterior) shall be of 2 coats of (wood paint over 1 coat of wood primer or equivalent. Erection of scaffolding, preparing working platforms, applying sealer and two coats of paint as specified in the working drawings. Removal of scaffolding if any after completion of work. Rates shall include for the provision and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and or masking floors fittings and similar work removing and replacing door window furniture. "]
[null,"All painting work shall be carried in accordance with the Specifications"]
[]
[9.2,"Wall painting"]
[null,"For Masonary walls."]
["9.2.1","External painting 1 coat of wall sealer, 1 coat texture compound & 2 coats of paints ( all coats to be oil based and external paint)."]
[null,"Internal Painting 1 coat of wall sealer & 2 coats of paints, Emulsion paint putty finish system on plastered and concrete surfaces of internal walls. "]
[{"v":1,"d":"(1)"},"Ground floor interior and exterior painting as spection above, ","m²",{"v":553,"d":"553.00"}]
[null,"Partition walls"]
[]
[null,"For Partition walls."]
[{"v":2,"d":"(2)"},"Internal Painting 1 coat of wall sealer & 2 coats of paints, Emulsion paint putty finish system on plastered and concrete surfaces of internal walls. ","m²",{"v":125,"d":"125.00"}]
[]
[]
[9.3,"Interior Ceiling painting"]
["9.3.1","Emulsion paint putty finish on concrete slab and beams, plywood / cement fiber board of all internal surfaces. 1 coat of primer & 2 coats of paints."]
[{"v":1,"d":"(1)"},"Emulsion putty paint finish","m²",{"v":166,"d":"166.00"}]
[]
[9.4,"Exterior ceiling painting"]
[{"v":1,"d":"(1)"},"Exterior Ceiling painting  as per specification given.","m²",{"v":39.6,"d":"39.60"}]
[]
[]
[]
[null,"BILL No: 9 - PAINTING"]
[null,"TOTAL OF BILL No: 9 - Carried over to summary"]
[null,"BILL No: 10"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[10.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each Light/ light fixture and its switch is measured as one  point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[]
[10.2,"Mains connection"]
[{"v":1,"d":"(1)"},"Main connection: Rates shall include screws, nails, bolts, nuts, standard cable, fixing or supporting clips, brackets, straps, rivets, plugs, and all incidental accessories. Rates shall include electrical conduits, fittings, equipment, and similar items. Three - PHASE CABLE WIRING TO D-BOARD:  All necessary work in trench shall include excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers warning tape, and disposal of surplus soil supply and laying of the cable in according to Maldives electricity bureau. (16mm2 4-Core Cable, approved by respective Authorities, GI pipe, warning tape), the contractor has to measure cable length from the site. The main cable must be connected to the existing health center. The contractor must inspect the site and Upgrade the Main distribution board if necessary to connect the Health center as well as the extension Building as per Fenaka requirements.","no",{"v":1,"d":"1.00"}]
[]
[10.3,"Electrical Boards"]
[{"v":1,"d":"(1)"},"Three phase electrical distribution board (wall embedded):  Supply and installation of   D-Board .  Rates Shall include all required Brackets and other electrical appliance as per drawings and Maldivian Regulations,All the light circuit should be one DB Sockets to be one DB.","no",{"v":2,"d":"2.00"}]
[]
[10.4,"Electrical wiring"]
[null,"Three phase Electrical wiring with copper conductor cable (Kelani or Equivalent) in conduits in walls and in casing on soffits of slab as specified to:"]
[{"v":1,"d":"(1)"},"Wiring with 2.5 mm² cable to 1X13amp Power points","points",{"v":54,"d":"54.00"}]
[{"v":2,"d":"(2)"},"Wiring with 6 mm² cable to 1X15amp Power points","points",{"v":5,"d":"5.00"}]
[{"v":3,"d":"(3)"},"Wiring with 6 mm² cable to 1X15amp Power points for Acs","points",{"v":7,"d":"7.00"}]
[{"v":4,"d":"(4)"},"Wiring with 2.5 mm² cable to lights and fan","points",{"v":58,"d":"58.00"}]
[]
[10.5,"Lighting / Fan"]
[{"v":1,"d":"(1)"},"Ceiling diffusing embedded down light 200mm dia with 21W LED,  (Philips), Cool day light, (not crystal light or not Stellar bright) Total lumen 1400. or equivalent,","no",{"v":34,"d":"34.00"}]
[{"v":2,"d":"(2)"},"Whether proof wall mount light with  13W LED,  (Philips), Cool day light, Total lumen 1400, for Portico area","no",{"v":6,"d":"6.00"}]
[{"v":3,"d":"(3)"},"LED Emergency light ( 2 hours Battery charge)","no",{"v":8,"d":"8.00"}]
[{"v":4,"d":"(4)"},"Supply and complete installation of KDK 300X300mm heavy duty extast fan with exaust pipe of public toilet.","Item",{"v":1,"d":"1.00"}]
[" ",null,null," "]
[10.6,"Socket outlets"]
[null,"(a) All socket outlets shall be \"Legrand\" or equivalent."]
[{"v":1,"d":"(1)"},"1x13Amp wall Socket outlet,  ","no",{"v":54,"d":"54.00"}]
[{"v":2,"d":"(2)"},"1x15Amp wall Socket outlet,  ","no",{"v":5,"d":"5.00"}]
[{"v":3,"d":"(3)"},"1x15Amp wall Socket outlet for Acs,","no",{"v":7,"d":"7.00"}]
[]
[10.7,"Light switches "]
[null,"(a) All light switches shall be \"Legrand\" or equivalent. Each light should be control by one switch."]
[]
[{"v":1,"d":"(1)"},"One gang switch ","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Two gang switch ","no",{"v":4,"d":"4.00"}]
[{"v":3,"d":"(3)"},"Tthree gang switch ","no",{"v":2,"d":"2.00"}]
[{"v":4,"d":"(4)"},"Four gang switch ","no",{"v":5,"d":"5.00"}]
[{"v":5,"d":"(5)"},"Out door photo cell switch","no",{"v":2,"d":"2.00"}]
[]
[10.8,"Computer Network"]
[null,"Design, Supply and Complete Installation of computer networking, including CAT6 Cabling, Sockets and double layer switches,  Allow for the provision of a completed and detailed set of shop drawings "]
[{"v":1,"d":"(1)"},"Completion of  Data Network points including face plate, face plate must be \"Legrand\" or equivalent.","No",{"v":8,"d":"8.00"}]
[{"v":3,"d":"(3)"},"Supply and complete installation of 24 port, Double layer Manageable network switch D-Link or equivalent and connect to the Health Center network.","No",{"v":1,"d":"1.00"}]
[{"v":4,"d":"(4)"},"Supply and complete installation of Computer system as per specifications","No",{"v":4,"d":"4.00"}]
[{"v":5,"d":"(5)"},"Supply and complete installation of 65\" QLED TV, LG or Equivalent at meting room. Any cast or chrome cast must support.","No",{"v":2,"d":"2.00"}]
[{"v":6,"d":"(6)"},"Suuplying of Canon Black and white print , A4 and A5 size","No",{"v":4,"d":"4.00"}]
[]
[10.9,"Telephone Network"]
[null,"Design and supply and complete installation of Telephone network (Including cabling and sockets) and connect to existing PABX. Cat6 cable to be used for laying telephone network."]
[{"v":1,"d":"(1)"},"Completion of Telephone outlet points , rates includes to connect existing telephone network. including face plate, face plate must be \"Legrand\" or equivalent.","No",{"v":8,"d":"8.00"}]
[{"v":2,"d":"(2)"},"Supply and complete installation of IP PABX, minimum 25 lines, including console.","Item",{"v":1,"d":"1.00"}]
[{"v":3,"d":"(3)"},"Supply and complete installation of Telephone","No",{"v":12,"d":"12.00"}]
[]
[{"v":10.1,"d":"10.10"},"Earthing"]
[null,"Earth pit with resistance less than 2 ohms, 3/4 earth rods must be used and must have clamps at the end, Earth pit should be covered junction with cover.\n"]
[{"v":1,"d":"(1)"},"Completion of  earth pit with earthing cable and completion of earthing as per the above requirements.","Item",{"v":1,"d":"1.00"}]
[]
[10.11,"Fire Fighting"]
[{"v":1,"d":"(1)"},"CO2 Extinguisher","Item",{"v":4,"d":"4.00"}]
[{"v":2,"d":"(2)"},"H2O Extinguisher","Item",{"v":4,"d":"4.00"}]
[]
[]
[]
[null,"BILL No: 10 - ELECTRICAL INSTALLATIONS"]
[null,"TOTAL OF BILL No: 10 - Carried over to summary"]
[]
[null,"BILL No: 11"]
[null,"HYDRAULICS & DRAINAGE"]
[]
[11.1,"Hydraulics"]
["11.1.1","General"]
[null,"(a)  Rates shall include for excavation, laying pipes and backfilling trenches, maintaining faces of drainpipe trenches and pits, backfilling, disposal of surplus soil, bends, junctions, reducers, expansion joints brackets, joints, straps, hangers, screws, nails and fixing complete, and all joints and other incidental material, All Pipes and fittings area high pressure uPVC  pipes"]
[null,"fixing complete, including cutting and forming holes; excavating, laying pipes and backfilling trenches."]
[null,"(b) All pipe work shall be uPVC."]
[]
["11.1.2","Fresh water supply pipe work"]
[{"v":1,"d":"(1)"},"Completion of pipe works and Connect ground water supply pipe work to Fresh water network installed at hospital.","Item",{"v":1,"d":"1.00"}]
[]
["11.1.3","Ground water supply pipe work"]
[{"v":1,"d":"(1)"},"Completion of pipe works and Connect ground water supply pipe work.","Item",{"v":1,"d":"1.00"}]
[]
["11.1.4","Sanitary fixtures & accessories"]
[null,"Sanitary fixtures & Accessories: Sanitary fixtures complete including brackets, flush pipes, valves, overflows, plugs and washers, as specified."]
[{"v":1,"d":"(1)"},"Water closet (American standard, Neo Modern,  Anti bacterial type) or equivalent, (dual top flush)","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Wash basin with pedestal (American Standard) or equivalent","no",{"v":3,"d":"3.00"}]
[{"v":3,"d":"(3)"},"Water tap for wash basin , ( Cotto) or equivalent","no",{"v":3,"d":"3.00"}]
[{"v":4,"d":"(4)"},"Muslim Shower with Stop valve, ( Cotto) or equivalent","no",{"v":1,"d":"1.00"}]
[{"v":5,"d":"(5)"},"Floor waste with SS gully trap ( toilet and laundry area)","no",{"v":1,"d":"1.00"}]
[{"v":6,"d":"(6)"},"Stop Valves, ( Cotto) or equivalent","no",{"v":6,"d":"6.00"}]
[{"v":7,"d":"(7)"},"Wall cabinet ( Mirror and towel bar only) Cotto and equivalent","no",{"v":1,"d":"1.00"}]
[{"v":8,"d":"(8)"},"Water tap for Gardening , ( Cotto) or equivalent","no",{"v":2,"d":"2.00"}]
[]
[11.2,"Drainage"]
["11.2.1","General"]
[null,"(a) Rates shall include for: excavation, maintaining faces of drain pipe trenches and pits, backfilling, disposal of surplus spoil; bends, junctions, reducers, expansion joints and all joints and other incidental materials."]
[null,"(b) All pipe work shall be UPVC"]
[{"v":1,"d":"(1)"},"Constructing  Concrete Inspection Chamber of required size with all provisions to connect pipelines as per drawing.","Item",{"v":2,"d":"2.00"}]
[]
[11.3,"Pipe work"]
[]
[{"v":1,"d":"(1)"},"Completion of pipe works and Connect Waste disposal pipe 75mm dia to Sewer network installed at existing system.","Item",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Completion of pipe works and Connect Sewers pipe 100mm dia UPVC to   Sewer network installed at existing system. Rates includes to install inspection chamber as per consultants instructions.","Item",{"v":1,"d":"1.00"}]
[]
[]
[]
[null,"BILL No: 11 - HYDRAULICS & DRAINAGE"]
[null,"TOTAL OF BILL No: 11 - Carried over to summary"]
[]
[null,"BILL No: 12"]
[null,"AIR CONDITIONING WORKS"]
[]
[12.1,"General"]
[null,"(a) Rates shall include for detail design, supply and complete installation of  A/C units pipework, insulation, fixings, electrical wiring, drain pipes etc."]
[null,"(b) The Contractor shall provide detailed and complete set of shop drawings"]
[null,"c) The contractor shall subbmit shop drawings of AC  and Exhaust System. The capacity shall be determined by the contractor. "]
[null,"d) Rate shall include complete installation of indoor units and outdoor units."]
[]
[12.2,"Air Condition"]
["12.2.1","Design, supply and complete installation of indoor and out door unit, \nAll AC unit is DAIKIN or equivalent (INVERTER TYPE). "]
[null,"The whole of the liquid and suction refrigerant lines including all fittings, valves etc. shall be insulated with 25mm thick insulation for all copper sizes. Insulation shall be closed cell elastomeric nitrile rubber."]
[null,"Protection of exposed Refrigerant Pipe Insulation:\nTo protect nitrile rubber of exposed piping from degrading due ultra violet rays & atmospheric conditions, it shall be covered polychelid coating with at least two coats of resin and hardener (Make-Polybond /Paramount Polytreat). Fiberglass tape shall be helically wound & painted with two coats of resin with hardener to give smooth & plain finish. "]
[null,"The proposed outdoor or outdoor set specifications should detail Energy Efficiency Ratio (EER) kw/kw not less than 4.5kw"]
[null,"The Outdoor Unit Shall be Factory assembled with Weather Proof casing, constructed from Heavy Gauge Mild Steel Panels and coated with Anti Corrosive Epoxy resin finish. The unit should be completely factory wired and tested and shall be fitted with all necessary controls and switch gear."]
[null,"All outdoor units needs to have aluminum fins with 105+2 μm thickness, with special Anti corrosive coating of 1.3 ± 0. 35 μm thickness and an outside Hydrophilic layer coating of 0.35 ± 0. 07 μm thickness."]
[null,"All outdoor units shall be equipped with high efficiency optimized heat exchangers with variable heat exchanger circuits"]
[null,"All the outdoor unit must be fixed back side of the Building."]
[]
[null,"AC to be install Following rooms, all the indoor unit should be spilt type. "]
[]
[12.3,"Air Condition works"]
[{"v":1,"d":"(1)"},"Consultation room-1 &2, 12,000 BTU  spilt type Wall mount air conditioner, DAIKIN or equivalent.","Item",{"v":2,"d":"2.00"}]
[{"v":2,"d":"(2)"},"Laboratory, 36,000 BTU  spilt type Wall mount air conditioner, DAIKIN or equivalent.","Item",{"v":1,"d":"1.00"}]
[{"v":3,"d":"(3)"},"Room 1, 24,000 BTU  spilt type Wall mount air conditioner, DAIKIN or equivalent.","Item",{"v":1,"d":"1.00"}]
[{"v":4,"d":"(4)"},"Sample collection area , 9,000 BTU  spilt type Wall mount air conditioner, DAIKIN or equivalent.","Item",{"v":1,"d":"1.00"}]
[{"v":5,"d":"(5)"},"Waiting area , 48,000 BTU  spilt type Wall mount air conditioner, DAIKIN or equivalent.","Item",{"v":2,"d":"2.00"}]
[{"v":6,"d":"(6)"},"Ward area, 48,000 BTU  Multi spilt type Ceiling cassette air conditioner (with wired remote) DAIKIN or equivalent. Rates also include electrical wiring and other necessary works required to complete the task.","Item",{"v":1,"d":"1.00"}]
[]
[12.4,"Air Curtain"]
[null,"Supply and Complete installation of Air curtain."]
[{"v":1,"d":"(1)"},"Supply and Complete installation on KDK (10ESK )  air curtain, 900mm length at  Exit door.","Item",{"v":2,"d":"2.00"}]
[]
[null,"BILL No: 12 -AIR CONDITIONING WORKS"]
[null,"TOTAL OF BILL No: 12 - Carried over to summary"]
[]
[null,"BILL No:13"]
[null,"TENDERER'S ADJUSTMENTS"]
[]
[13.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[13.1,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"GROUND  WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"CONCRETE, Bill no. 03"]
[{"v":4,"d":"(4)"},"MASONRY AND PLASTERING, Bill no. 04"]
[{"v":5,"d":"(5)"},"METAL WORKS, Bill no. 05"]
[{"v":6,"d":"(6)"},"DOORS AND WINDOWS, Bill no. 06"]
[{"v":7,"d":"(7)"},"TILING, Bill no. 07"]
[{"v":8,"d":"(8)"},"CEILINGS, Bill no. 08"]
[{"v":9,"d":"(9)"},"PAINTING, Bill no. 09"]
[{"v":10,"d":"(10)"},"ELECTRICAL INSTALLATIONS, Bill no. 10"]
[{"v":11,"d":"(11)"},"HYDRAULICS & DRAINAGE, Bill no. 11"]
[{"v":12,"d":"(12)"},"TENDERER'S ADJUSTMENTS,  Bill no. 12"]
[{"v":13,"d":"(13)"},"AIR CONDITIONING WORKS,  Bill no. 13"]
[null,"ADDITIONS TOTAL"]
[]
[13.2,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"GROUND  WORKS, Bill no. 02"]
[{"v":3,"d":"(3)"},"CONCRETE, Bill no. 03"]
[{"v":4,"d":"(4)"},"MASONRY AND PLASTERING, Bill no. 04"]
[{"v":5,"d":"(5)"},"METAL WORKS, Bill no. 05"]
[{"v":6,"d":"(6)"},"DOORS AND WINDOWS, Bill no. 06"]
[{"v":7,"d":"(7)"},"TILING, Bill no. 07"]
[{"v":8,"d":"(8)"},"CEILINGS, Bill no. 08"]
[{"v":9,"d":"(9)"},"PAINTING, Bill no. 09"]
[{"v":10,"d":"(10)"},"ELECTRICAL INSTALLATIONS, Bill no. 10"]
[{"v":11,"d":"(11)"},"HYDRAULICS & DRAINAGE, Bill no. 11"]
[{"v":12,"d":"(12)"},"TENDERER'S ADJUSTMENTS,  Bill no. 12"]
[{"v":13,"d":"(13)"},"AIR CONDITIONING WORKS,  Bill no. 13"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 13 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 13 - Carried over to summary"]