{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER PAGE","summary1","BOQ"],"not_rendered":{"external_links":1,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER PAGE","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"merged":[[5,1,5,5],[7,1,7,5],[9,1,9,5],[10,1,10,5],[14,1,14,5]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"BILL OF QUANTITIES"]
[]
[null,"PROPOSED SINGLE STOREY COURT BUILDING AT F. FEEALI"]
[]
[null,"CLIENT: DEPARMENT OF JUDICIAL ADMINISTRATION "]
[]
[]
[]
[]
[null,"March 2024"]

{"sheet":"summary1","index":1,"n_rows":38,"n_cols":4,"rows_kept":38,"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITIES"]
["Proposed Single storey court building at F. Feeali"]
[]
["Bill No",null,"Description","Amount"]
[1,null,"PRELIMINARIES"]
[2,null,"CONCRETE"]
[3,null,"MASONRY AND PLASTERING"]
[4,null,"WOOD & METAL WORKS"]
[5,null,"ROOFING"]
[6,null,"DOORS AND WINDOWS"]
[7,null,"CEILINGS"]
[8,null,"PAINTING"]
[9,null,"FINISHES"]
[10,null,"FIRE FIGHTING SYSTEM"]
[11,null,"HYDRAULICS & DRAINAGE"]
[12,null,"ELECTRICAL INSTALLATIONS"]
[13,null,"CCTV SYSTEM (SECURITY SYSTEM)"]
[14,null,"AIR CONDITION SYSTEM "]
[15,null,"FURNITURE "]
[16,null,"COURT ROOM FURNITURE "]
[17,null,"TENDERER'S ADJUSTMENTS"]
[]
[null,null,"GRAND TOTAL carried to form of bid"]
[null,null,"BOUNDARY WALL"]
[1,null,"PRELIMINARIES"]
[2,null,"GROUND WORKS"]
[3,null,"CONCRETE"]
[4,null,"MASONRY AND PLASTERING"]
[5,null,"METAL"]
[7,null,"PAINTING"]
[9,null,"ELECTRICAL INSTALLATIONS"]
[10,null,"TENDER'S ADJUSTMENT"]
[]
[null,null,"GRAND TOTAL carried to form of bid",0]
[null,null,"Total",0]
[null,null,"GST 6%",0]
[null,null,"Project Total",0]

{"sheet":"BOQ","index":2,"n_rows":895,"n_cols":6,"rows_kept":895,"merged":[[596,0,596,5]],"flags":["formulas_cached_only"]}
["Item","Description","Unit","Qty","Rate","Amount"]
[]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"]
[null,"m - metre"]
[null,"No - numbers"]
[null,"m³ - cubic metre"]
[null,"m² - square metre"]
[null,"Lm - Linear metre"]
[null,"t - tonnes"]
[null,"incl - including"]
[null,"mm - millimetre"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanised Iron"]
[]
[1.2,"Site Management Costs"]
[{"v":1,"d":"(1)"},"Allow for all on and off site management cost including costs of foreman and assistants, temporary services, telephone, fax, hoardings and similar.","item",{"v":1,"d":"1.00"}]
[]
[1.3,"Sign Board"]
[{"v":1,"d":"(1)"},"Allow for sign board.","no",{"v":1,"d":"1.00"}]
[]
[1.4,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","item",{"v":1,"d":"1.00"}]
{"$rows_empty":15}
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"CONCRETE"]
[]
[2.1,"General"]
[null,"(a) Rates shall include for: placing in position; making good after removal of formwork and casting in all required items; additional concrete required to conform to structural and excavated tolerances."]
[null,"(b) Mix ratio for  reinforced concrete shall be 1:2:3 and lean concrete shall be 1:2:6 by volume."]
[null,"(c ) Use plasticiser in all concrete works."]
[]
[2.2,"Reinforced Concrete"]
[" ","In-situ reinforced concrete to:"]
["2.2.1","Roof level"]
[{"v":1,"d":"(1)"},"Stifener Column","m³",{"v":0.3,"d":"0.30"}]
[{"v":2,"d":"(2)"},"127 x 100 sill beams and Lintel","nos",{"v":7,"d":"7.00"}]
[]
[2.3,"Formwork"]
[null,"(a) Rates shall include for: all necessary boarding, supports, erecting, framing, temporary cambering, cutting, perforations for reinforcing bars, bolts, straps, ties, hangers, pipes and removal of formwork."]
["2.3.1","Roof level"]
[{"v":1,"d":"(1)"},"Stiffener Column","m²",{"v":10,"d":"10.00"}]
[{"v":2,"d":"(2)"},"127 x 100 sill beams and Lintel","nos",{"v":7,"d":"7.00"}]
[]
[2.4,"Reinforcement"]
[null,"(a) Rates shall include for: cleaning, fabrication, placing, the provision for all necessary temporary fixings, and supports including tie wire and chair supports, laps, distribution bars and wastage."]
[null,"(b) All reinforcing bars shall be high strength bars."]
["2.4.1","Sill Beams"]
[null,"10 mm dia. bars in 150 x 100  sill Beams","nos",{"v":7,"d":"7.00"}]
[null,"6 mm dia. bars in 150 x 100 sill Beams ","nos",{"v":7,"d":"7.00"}]
[]
["2.4.2","Roof Level"]
[{"v":1,"d":"(1)"},"10 mm dia. bars in Stiffener Column","kg",{"v":24,"d":"24.00"}]
[{"v":2,"d":"(2)"},"6 mm dia. bars in Stiffener Column","kg",{"v":18.2,"d":"18.20"}]
[]
[2.5,"Other concrete works"]
[null,"(a) Rates shall include for:  concrete, formwork, reinforcement & finish as specified and shown on the drawings."]
[]
["2.5.1","Concrete works"]
[null,"Plumbing and Sweage disposal units, refer plumbing details drawings"]
[{"v":1,"d":"(1)"},"Reinforced concrete Ground water well 1200mm dia. ","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Inspection Chamber (600x600)","no",{"v":6,"d":"6.00"}]
["2.6.2","R.C Flag Post"]
[{"v":1,"d":"(1)"},"RC Flag post footing including 8 anchor bolts as specified in the drawing.","no ",{"v":1,"d":"1.00"}]
["2.6.3","R.C.C Bench for Prison "]
[{"v":1,"d":"(1)"},"R.C.C Bench for prison including concrete, filing , reforcement, forwork,   as per specified in the drawing","no",{"v":1,"d":"1.00"}]
[]
["2.6.4","R.C steps","item",{"v":3,"d":"3.00"}]
["2.6.5","100mm R.C Sink slab as specified in the Drawing","item",{"v":1,"d":"1.00"}]
{"$rows_empty":8}
[null,"BILL No: 02 - CONCRETE WORKS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"MASONRY AND PLASTERING"]
[]
[3.1,"General"]
[null,"(a) Rates shall include for: cleaning out cavities, forming rebated reveals and pointing and cleaning down to reveals where necessary; fractional size blocks, all necessary machine cutting, cutting or forming chases or edges of "]
[null,"floor slabs, cutting or leaving holes and openings as recesses for and building in pipes, conduits, sleeves and similar as required for all trades; leaving surfaces rough or raking out joints for plastering and flashings, bedding "]
[null,"frames or plates, building in joists, bearers or similar, temporary supports to openings, templates, reinforcement in walls and for all necessary making good"]
[]
[3.2,"Cement brickwork"]
[null,"Ground floor"]
["3.2.1","127 mm wide full block masonry wall, laid on and incl. mortar  tie rods, compression joint gap filling material such as mastic sealent as specified external walls ","m²",{"v":33,"d":"33.00"}]
["3.2.2","100 mm wide hollow block masonry wall, laid on and incl. mortar  tie rods, compression joint gap filling material such as mastic sealent as specified internal walls ","m²",88.58]
[3.3,"Plastering"]
[null,"(a) Cement plastering on walls and concrete surfaces as specified incl. wire mesh at the joints of concrete surfaces and walls "]
["3.3.1","23mm thick plastering one layer as per specified drawing (external surface )","m²",{"v":171,"d":"171.00"}]
["3.3.2","17mm thick plastering one layer as per specified drawing (internal surface)","m²",{"v":690,"d":"690.00"}]
["3.3.3","Plastering one layer in Columns","m²",{"v":109,"d":"109.00"}]
[]
[3.4,"Cement Screed"]
[null,"50 mm thick floor screed on  ground floor ","m²",{"v":326,"d":"326.00"}]
[]
[3.5,"Cement Block"]
[null,"100mm thk Street payment cement blocks ","m²",107.77]
[]
[null,"BILL No: 03 - MASONRY AND PLASTERING"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No: 04"]
[null,"WOOD & METAL WORKS"]
[]
[4.1,"General"]
[null,"(a) Rates shall include for: all labour in framing, notching and fitting around projections, pipes, light fittings, hatches, grilles and similar and complete with cleats, packers, wedges and similar and all nails and screws."]
[]
[4.2,"Roof structure"]
[{"v":1,"d":"(1)"},"Timber rafters, 50 x 200 mm.","m",{"v":611,"d":"611.00"}]
[{"v":2,"d":"(2)"},"Purlin timber, 50 x 38 mm","m",{"v":720,"d":"720.00"}]
[{"v":3,"d":"(3)"},"Hardwood ridge beame, 50 x 150 mm","m",{"v":83,"d":"83.00"}]
[{"v":4,"d":"(4)"},"Wall plate, 50 x 125 mm","m",{"v":72,"d":"72.00"}]
[{"v":6,"d":"(6)"},"Fascia Board 200x8 mm ","m",{"v":82,"d":"82.00"}]
[]
[4.3,"Wooden rack "]
[{"v":1,"d":"(1)"},"Wooden rack to full height in archive as specified in the drawing.","item ",{"v":15,"d":"15.00"}]
[]
[4.4,"Timber Counter"]
[{"v":1,"d":"(1)"},"Timber counter finishing including the overhead cabinets as per specified in the  drawing","item ",{"v":1,"d":"1.00"}]
[]
[4.5,"Sink Cupboard Door & Shelf "]
[null,"Sink Cupboard door & Shelf as specified in drawing","item ",{"v":1,"d":"1.00"}]
[]
[null,"METAL WORKS"]
[4.5,"General"]
[null,"(a) Rates shall include for: all fabrication work, welding, marking, drilling for bolts including those securing timbers, steel plates, bolts, nuts and any type of washer, riveted work, counter sinking and tapping for bolts or machine screws."]
[null,"(b) Rates shall include for all painting and finishing as specified"]
[null,"(c) Rates shall include for fabrication and erection and temporary supports and fixing into position"]
[]
[{"v":1,"d":"(1)"},"Prison cell"]
[null,"Providing and fixing 16mm dia. Bar (tor steel) underneath the foundation beam at all joints and to the roof beam. The spacing of the iron bars should be 150 mm C/C both ways  including three coats of paints","Nos",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Fabricate and install steel prison door of size 1500 x 2100 mm including three coats of paints. The door is to be specially prapared with 16 dia. Iron bar @ spacing of 150mm c/c and 2.5 inch x 2.5 inch angle iron frame including locking system.","Nos",{"v":1,"d":"1.00"}]
[4.6,"Flag post"]
[{"v":1,"d":"(1)"},"75mm dia SS Flag Post including base plate and head plate as specified in the drawing. ","Nos",{"v":2,"d":"2.00"}]
[]
[4.7,"Windows Grill "]
[{"v":1,"d":"(1)"},"Grill to be fixed at all exterior windows as specified in the drawing.","item ",{"v":1,"d":"1.00"}]
[]
[null,"BILL No: 04 - WOOD & METAL WORKS"]
[null,"TOTAL OF BILL No: 04 - Carried over to summary"]
[null,"BILL No: 05"]
[null,"ROOFING"]
[]
[5.1,"General"]
[null,"(a) Rates shall include for: fair edges, dressing over angel fillets, turning into grooves, all other labours, circular edges, nails, screws and other fixings and laps."]
[5.2,"Roof Coverings"]
[{"v":1,"d":"(1)"},"Lysaght or equivalent roofing sheet, including all fixings, fixed in accordance with manufacturer's instructions.","m²",{"v":464,"d":"464.00"}]
[5.3,"Cappings and Flashings"]
[{"v":1,"d":"(1)"},"Ridge capping","m",{"v":60.4,"d":"60.40"}]
[{"v":2,"d":"(2)"},"Flashing","m",{"v":8.2,"d":"8.20"}]
[5.4,"Gutter"]
[null,"Lysaght or equivalent gutter including framing, and supports, straps, brackets, clips, stop ends, overflow, downpipe outlets, mesh flashings and all fixings and fastenings."]
[{"v":1,"d":"(1)"},"200 x 150 gutter ","m",{"v":78,"d":"78.00"}]
[{"v":2,"d":"(2)"},"400 X 150 Valley Gutter","m",{"v":12,"d":"12.00"}]
[5.5,"Down Pipes"]
[{"v":1,"d":"(1)"},"75 mm dia PVC down pipes including bends, junctions, straps, brackets, clips and all fixings.","m",{"v":60,"d":"60.00"}]
[5.6,"Insulation"]
[{"v":1,"d":"(1)"},"75mm thick glass insulation for roof with Aluminium foil on both sides and secured by wire mesh.","m²",{"v":464,"d":"464.00"}]
[]
[]
[null,"BILL No: 05 - ROOFING"]
[null,"TOTAL OF BILL No: 05 - Carried over to summary"]
[null,"BILL N0: 06"]
[null,"DOORS AND WINDOWS"]
[]
[6.1,"General"]
[null,"(a) Rates shall include for locks, latches, closers, push plates, pull handles, bolts, kick plates, hinges and all door & window hardware."]
[null,"(b) Rates shall include for door frames and window frames, mullions, transoms, trims, glazing, tinting, timber panels, boardings, framing, lining, fastenings and all fixings and installation."]
[null,"(c) All door frames and window frames shall be as specified in the drawing"]
[null,"(d) Rates shall include for all painting and putty as specified."]
[]
[6.2,"Door Units"]
[{"v":1,"d":"(1)"},"Door D1,   (8.56m²)","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Door D2,    (1.89 m²)","no",{"v":14,"d":"14.00"}]
[{"v":3,"d":"(3)"},"Door D3,  (1.89 m²)","no",{"v":4,"d":"4.00"}]
[{"v":4,"d":"(4)"},"Door D4,   (1.47 m²)","no",{"v":3,"d":"3.00"}]
[]
[6.3,"Window Units"]
[{"v":1,"d":"(1)"},"Window W1,   (2.63 m²)","no",{"v":5,"d":"5.00"}]
[{"v":3,"d":"(3)"},"Ventilater V1,   (0.42 m²)","no",{"v":7,"d":"7.00"}]
[]
[6.4,"Windows Blinds"]
[null,"Windows Vertical Blinds to be fixed at all exterior windows as specified in the Information Sheet","no",{"v":5,"d":"5.00"}]
[]
[]
[null,"BILL N0: 06 -  DOORS AND WINDOWS"]
[null,"TOTAL OF BILL No: 06 - Carried over to summary"]
[null,"BILL No: 07"]
[null,"CEILINGS"]
[]
[7.1,"Gypsum Ceilings"]
[]
[{"v":1,"d":"(1)"},"9 mm thick Gypsum ceiling with Cement fibre cornice  boarder,  including  timber framing , trimming, nails, screws, 50 x 50 mm tinber frame at 600c/c  and other fixings ","m²",{"v":370,"d":"370.00"}]
[{"v":2,"d":"(2)"},"Cement fibre board ceiling including fixings. (Out Door)","m²",{"v":45,"d":"45.00"}]
{"$rows_empty":26}
[null,"BILL N0: 07 CEILINGS"]
[null,"TOTAL OF BILL No: 07 - Carried over to summary"]
[null,"BILL No: 8"]
[null,"PAINTING"]
[8.1,"General"," "]
[null,"(a) Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window"]
[null,"(b) All painting work shall be carried in accordance with the Specifications"]
[null,"(c) Painting system shall be Nippon or Equivalent"]
[null,"(d) Weather proof emulsion paint system with textured finish on plastered and concrete surfaces of external and normal emulsion paint on  internal walls"]
["8.2.1","External painting 1 coat of wall sealer, 1 coat tex compound & 2 coats of paints","m²",{"v":171,"d":"171.00"}]
["8.2.2","Emulsion paint putty finish system on plastered and concrete surfaces of internal walls. Internal painting 1 coat of wall sealer, 2 coats of paints","m²",{"v":690,"d":"690.00"}]
["8.2.3","Emulsion paint putty finish system on plastered and concrete surfaces of Columns. Internal painting 1 coat of wall sealer, 2 coats of paints","m²",{"v":109,"d":"109.00"}]
[8.3,"Ceilings"]
[{"v":1,"d":"(1)"},"Emulsion paint finish on ceiling","m²",{"v":326,"d":"326.00"}]
{"$rows_empty":11}
[null,"BILL No: 08 - PAINTING"]
[null,"TOTAL OF BILL No: 08 - Carried over to summary"]
[null,"BILL N0: 09"]
[null,"FINISHES"]
[]
[9.1,"General"]
[null,"(a) Rates shall include for: fixing, bedding, grouting, and pointing materials; making good around pipes, sanitary fixtures, and similar; cleaning down and polishing."]
[]
[9.2,"Ceramic floor tiles"]
[]
[{"v":1,"d":"(1)"},"300 x 300mm Ceramic floor tiles","m²",{"v":251,"d":"251.00"}]
[{"v":2,"d":"(2)"},"300 x300mm all Toilet non slip ceramic floor tiles","m²",{"v":16.4,"d":"16.40"}]
[{"v":3,"d":"(3)"},"300 x 300mm  Portico, Veranda and Steps non slip outdoor Homogeneous floor tiles","m²",{"v":45,"d":"45.00"}]
[{"v":4,"d":"(4)"},"300 x300mm all toilet Glazed  ceramic wall tiles","m²",{"v":61,"d":"61.00"}]
[{"v":5,"d":"(5)"},"300 x300mm all pantry Glazed  ceramic wall tiles","m²",{"v":1.4,"d":"1.40"}]
[{"v":6,"d":"(6)"},"300 x300mm all cell Glazed  ceramic wall tiles","m²",{"v":21,"d":"21.00"}]
{"$rows_empty":18}
[null,"BILL No: 9 - FINISHES"]
[null,"TOTAL OF BILL No: 9 - Carried over to summary"]
[null,"BILL N0: 10"]
[null,"FIRE FIGHTING SYSTEM"]
[]
[10.1,"General"]
[null,"(a) Provide and install fire fighting equipment inclusive of all necessary connection as per local requlations as described."]
[]
[null,"a) All cables must be fire resistant cables"]
[{"v":1,"d":"(1)"},"Smoke Detector","Nos",{"v":13,"d":"13.00"}]
[{"v":2,"d":"(2)"},"CO2  Extinguisher (2 lit)","Nos",{"v":2,"d":"2.00"}]
[{"v":3,"d":"(3)"},"H2O Extinguisher (9 lit)","Nos",{"v":2,"d":"2.00"}]
[{"v":4,"d":"(4)"},"Fire Alarm Sound Strobe 85DS","Nos",{"v":1,"d":"1.00"}]
[{"v":5,"d":"(5)"},"Fire Alarm Control Panel","Nos",{"v":1,"d":"1.00"}]
[{"v":6,"d":"(6)"},"Manual Call Point","Nos",{"v":1,"d":"1.00"}]
[{"v":7,"d":"(7)"},"Exit Sign Board","Nos",{"v":2,"d":"2.00"}]
{"$rows_empty":13}
[null,"BILL No: 10 - FIRE FIGHTING SYSTEM"]
[null,"TOTAL OF BILL No: 10 - Carried over to summary"]
[null,"BILL No: 11"]
[null,"HYDRAULICS & DRAINAGE"]
[]
[11.1,"Hydraulics"]
["11.1.1","General"]
[null,"(a) Rates shall include for: sockets, running joints, connectors, elbows, junctions, reducers, expansion joints; backnuts and similar; incidental fittings, clips, saddles, brackets, straps, hangers, screws, nails and "]
[null,"fixing complete, including cutting and forming holes; excavating, laying pipes and backfilling trenches."]
[null,"(b) All pipework shall be UPVC."]
[null,"(c) Rate shall include for supply and fixing of all pipes"]
[]
["11.1.2","Ground water supply pipework"]
[{"v":1,"d":"(1)"},"Allow for supply and installation of  pipework to and from pump to all toilets and pantry  including all the necessary accessories & fittings."]
[null,"12 mm dia. uPVC high pressure pipe from well upto toilets.","m",{"v":50,"d":"50.00"}]
[null,"12 mm dia. high uPVC high pressure pipe to fixtures","m",{"v":63,"d":"63.00"}]
["11.1.3","Sanitary fixtures & accessories"]
[null,"Sanitary fixtures complete including brackets, flush pipes, overflows, plugs and washers, as specified"]
[{"v":1,"d":"(1)"},"WC complete","no",{"v":5,"d":"5.00"}]
[{"v":2,"d":"(2)"},"Toilet Porcelain Basins with taps","no",{"v":3,"d":"3.00"}]
[{"v":3,"d":"(3)"},"Rest room Porcelain Basins tap","no",{"v":1,"d":"1.00"}]
[{"v":4,"d":"(4)"},"Kitchen Sinks with tap","no",{"v":1,"d":"1.00"}]
[{"v":5,"d":"(5)"},"Floor drain with water trap.","no",{"v":6,"d":"6.00"}]
[{"v":6,"d":"(6)"},"Basin taps","no",{"v":4,"d":"4.00"}]
[{"v":7,"d":"(7)"},"Taps","no",{"v":5,"d":"5.00"}]
[{"v":8,"d":"(8)"},"Taps (Out Door)","no",{"v":3,"d":"3.00"}]
[{"v":9,"d":"(9)"},"Muslim Showers","no",{"v":5,"d":"5.00"}]
[{"v":10,"d":"(10)"},"Stop valve","no",{"v":6,"d":"6.00"}]
[{"v":11,"d":"(11)"},"Angle valve","no",{"v":10,"d":"10.00"}]
[]
["11.1.4","Mirrors"]
[null,"Mirrors incl. all fixings and framings"]
[{"v":1,"d":"(1)"},"Readymade Mirror Set","no",{"v":5,"d":"5.00"}]
[]
["11.1.5","Pumps"]
[null,"Supply and installation of water pump complete including connecting to pipework and electricity as specified."]
[{"v":1,"d":"(1)"},"Ground water pump (electric)","no",{"v":1,"d":"1.00"}]
[]
[11.2,"Drainage"]
["11.2.1","General"]
[null,"(a) Rates shall include for: excavation, maintaining faces of drain pipe trenches and pits, backfilling, disposal of surplus spoil; bends, junctions, reducers, expansion joints and all joints and other incidental materials."]
[null,"(b) All pipework shall be uPVC"]
["11.2.2","Discharge & Ventilation Pipework"]
[{"v":1,"d":"(1)"},"Allow for supply and installation of  pipework including all the necessary accessories & fittings.","item",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"100mm dia waste water pipes","m",{"v":53,"d":"53.00"}]
[{"v":2,"d":"(2)"},"75mm dia waste water pipes","m",{"v":22,"d":"22.00"}]
[]
[]
[null,"BILL No: 11 - HYDRAULICS & DRAINAGE"]
[null,"TOTAL OF BILL No: 11 - Carried over to summary"]
[null,"BILL No:12"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[12.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each Light/ light fixture and its switch is measured as one one point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[null,"(f) All main distribution boards distribution boards are 3 phase."]
[]
[12.2,"Mains connection"]
[{"v":1,"d":"(1)"},"Allow for connection to electrical mains (3phase Cable)","m",{"v":42,"d":"42.00"}]
[12.3,"Electrical boards"]
[null,"Complete installation, including for all connections, earthing, painting, testing and similar of:"]
[{"v":1,"d":"(1)"},"Electric meter (3phase Meter)","no",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Main distribution board","no",{"v":1,"d":"1.00"}]
[12.4,"Electrical wiring"]
[null,"Electrical wiring with copper conductor cable in conduits in walls and in casing on soffits of slab as specified to:"]
[{"v":1,"d":"(1)"},"Wiring with 2.5 mm² cable to lighting, switches & fans","point",{"v":184,"d":"184.00"}]
[{"v":2,"d":"(2)"},"Wiring with 2.5 mm² cable to power points","point",{"v":59,"d":"59.00"}]
[{"v":3,"d":"(3)"},"Wiring with 2.5 mm² cable to AC points","point",{"v":13,"d":"13.00"}]
[12.5,"Ceiling fan"]
[{"v":1,"d":"(1)"},"1.3m dia. Ceiling fan, ","no",{"v":15,"d":"15.00"}]
[]
[12.6,"Lighting"]
[{"v":1,"d":"(1)"},"Down light C/W 24W enery savers","no",{"v":97,"d":"97.00"}]
[{"v":2,"d":"(2)"},"Emergency light ","no",{"v":13,"d":"13.00"}]
[{"v":3,"d":"(3)"},"Wall light Bulb - weatherproof","no",{"v":13,"d":"13.00"}]
[{"v":4,"d":"(4)"},"Water Proof Sopt light (Flag Post Light)","no",{"v":2,"d":"2.00"}]
[]
[12.7,"Socket outlets"]
[null,"(a) All socket outlets shall be \"Clipsal\" or equivalent."]
[{"v":1,"d":"(1)"},"1 x13A socket outlet ","no",{"v":19,"d":"19.00"}]
[{"v":2,"d":"(2)"},"2 x13A socket outlet","no",{"v":25,"d":"25.00"}]
[{"v":3,"d":"(3)"},"1 x15A socket outlet ","no",{"v":14,"d":"14.00"}]
[12.8,"Switches"]
[null,"(a) All light switches shall be \"Clipsal\" or equivalent."]
[{"v":1,"d":"(1)"},"One gang switch","no",{"v":6,"d":"6.00"}]
[{"v":2,"d":"(2)"},"Two gang switch","no",{"v":13,"d":"13.00"}]
[{"v":3,"d":"(3)"},"Three gang switch","no",{"v":17,"d":"17.00"}]
[{"v":4,"d":"(4)"},"Four gang switch","no",{"v":3,"d":"3.00"}]
[{"v":5,"d":"(5)"},"Fan regulators","no",{"v":15,"d":"15.00"}]
[{"v":6,"d":"(6)"},"Photo cell switch","no",{"v":5,"d":"5.00"}]
[]
[12.9,"Lightening Protection System"]
[{"v":1,"d":"(1)"},"Design, supply and installation of Erco, Eritech or equivalent lightening Protection System (Approve by Client)","item",{"v":1,"d":"1.00"}]
[]
[{"v":12.1,"d":"12.10"},"Internet line"]
[null,"Provide & install Network fittings, wiring(CAT6),   equipment inclusive of all necessary connection as per drawing"]
[null,"Rates shall include Cable, box,face plate, and fixsing "]
[{"v":1,"d":"(1)"},"Network Switch (Specification attached)","nos",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Network points","nos",{"v":27,"d":"27.00"}]
{"$rows_empty":9}
[null,"BILL No:12 - ELECTRICAL INSTALLATIONS"]
[null,"TOTAL OF BILL No:12 - Carried over to summary"]
[null,"BILL No:13"]
[null,"CCTV SYSTEM (SECURITY SYSTEM)"]
[]
[13.1,"General"]
[null," Rates shall include Supply and installation of CCTV  security system as per specifications (Refer to the ICT specification) including all Wiring connection,  equipment inclusive of all necessary connection"]
[null,"(b) Rates shall include for supply and complete installation , fittings, Framing and fixtures, Cablings & testing "]
[null,"Supply and installation of CCTV  security system as per specifications (Refer to the ICT specification) including all Wiring connection,  equipment inclusive of all necessary connection"]
[{"v":1,"d":"(1)"},"Ultra Wide Dome Camera","nos",{"v":4,"d":"4.00"}]
[{"v":2,"d":"(2)"},"Varifocal bullet Camera","nos",{"v":8,"d":"8.00"}]
[{"v":3,"d":"(3)"},"Fisheye view Camera","nos",{"v":1,"d":"1.00"}]
[{"v":4,"d":"(4)"},"Cabling ","nos",{"v":13,"d":"13.00"}]
[{"v":5,"d":"(5)"},"NVR","nos",{"v":1,"d":"1.00"}]
[{"v":6,"d":"(6)"},"Network Cabinet","nos",{"v":1,"d":"1.00"}]
[]
[null,"BILL No:14 - CCTV SYSTEM (SECURITY SYSTEM)"]
[null,"TOTAL OF BILL No:14 - Carried over to summary"]
[null,"BILL No: 14"]
[null,"AIR-CONDITIONING SYSTEM"]
[]
[14.1,"General"]
[null,"(a) Rates shall include for supplying and complete installation of air-conditioning systems; including all pipework, electrical wiring, insulation, stands for outdoor units etc. (refer to drawing for outdoor stands)"]
[]
[14.2,"Air-conditioning"]
["14.2.1","Wall Mount & Celing Mount Split type unit as shown in drawings"]
[1,"Air Condition outdoor& indoor wall mount unit 18000 BTU/H (Inverter)","nos",{"v":2,"d":"2.00"}]
[2,"Air Condition outdoor& indoor wall mount unit 12000 BTU/H (Inverter)","nos",{"v":4,"d":"4.00"}]
[3,"Air Condition outdoor& indoor wall mount unit 9000  BTU/H (Inverter)","nos",{"v":1,"d":"1.00"}]
[4,"Air Condition outdoor& indoor ceiling mount unit 24000 BTU/H (Inverter)","nos",{"v":3,"d":"3.00"}]
[5,"Air Condition outdoor& indoor ceiling mount unit 18000 BTU/H (Inverter)","nos",{"v":2,"d":"2.00"}]
[6,"Air Condition outdoor& indoor ceiling mount unit 9000 BTU/H (Inverter)","nos",{"v":1,"d":"1.00"}]
{"$rows_empty":11}
[null,"BILL No:14 - AIR-CONDITIONING SYSTEM"]
[null,"TOTAL OF BILL No:14 - Carried over to summary"]
[null,"BILL No: 15"]
[null,"FURNITURE"]
[]
[15.1,"General"]
[null,"(a) Rates shall include for supplying and complete installation and arrangement of furnitures."]
[null,"(b) Contractor shall submit to the consultant and client for the approvals before supply and installation."]
[null,"(c)Admin staff chair and Conference hall chair is Eurotech Ergohuman collection high back mesh ergonomic chair it designed to be the ultimate in comfort. Specifically intended for users who are in their chair for five or more hours per day, Ergohuman features exclusive flex zones that ensure constant back and lumbar support. With a wide range of ergonomic adjustments required,  the Ergohuman high back chair can be easily customized to fit virtually any user. Instant lift seat adjustment is controlled by a lever located beneath the right front of the seatpan, and positions seat height from 17\"-21\".\n"]
[null,"(d)Elegant finish on hardwood arms and leg caps, with tailored leather padding on armrests for a truly distinguished look.  Passive ergonomic seating with built-in lumbar support provides lasting comfort. Back size is 22\"H x 21\"W. Seat size is 21\"W x 20-1/2\"D. Mahogany wood finish on wood legs. Weight Capacity is 250 lbs.\n"]
[null,"(e)8' Treck shape conference table by Regency it is constructed of a thermal fused laminate, finished with 3mm matching PVC edge. Table seats up to 8 people.  Table features a 2\" thick top, wire management on the underside of the table, and wire grommets for easy cabling access in the table top. Adjustable leveling glides keep provide stability on uneven floors. \n"]
[null,"(f)It is constructed of laminated engineered wood with a durable Classic Cherry laminate finish. Office suite includes an executive desk, computer credenza with hutch, lateral file cabinet, open bookcase, and doored bookcase. Executive desk has three file drawers with heavy duty-metal full extension glides that accommodate letter and legal files. File drawers in left pedestal lock. Desk should two small drawers and a center pencil drawer/keyboard tray with metal slides and safety stops. Grommet hole in top surface keeps cords organized. Dimensions: 65-1/2\"W x 31-1/8\"D x 29-5/8\"H.  Computer credenza features a box drawer and a letter size file drawer in the left drawer pedestal. Right door pedestal houses a vertical CPU compartment with an adjustable shelf. Pull-out laptop/keyboard drawer in center has full-extension slides and a built-in power strip with three outlets. Desktop grommet allows easy routing of cords. \n\n"]
[null,"(g)Wall Street collection sofa by Avenue Six provides a sound investment for those who take stock in high fashion design and unsurpassed seating comfort. \n\nWall Street gives you the options to fashion the size and style best suited for your office. Sofa features easy care Espresso faux leather upholstery, dacron wrapped foam cushions, chrome steel base and legs, and a kiln dried hardwood frame. \n\n\n•Corner-blocked, dowelled,\n•glued, screwed & stapled\n•High density foam\n•Removeable back\n•Sinuous wire springs"]
[null,"TV stand is constructed of hardwood solids and veneers. TV stand features two spacious shelves that hold audio/video equipment, two small storage drawers, and rear cut-outs for easy cord accessibility. Holds TVs weighing 95 lbs or less and with a base up to 42\"W. \n\n"]
[15.2,"Furniture"]
[{"v":1,"d":"(1)"},"Conference 8ft Table including 8 chairs(Fabric)","Nos ",{"v":1,"d":"1.00"}]
[{"v":2,"d":"(2)"},"Circular Conference 4ft Table including 4 chairs(Fabric)","Nos ",{"v":1,"d":"1.00"}]
[{"v":3,"d":"(3)"},"Dining Tables  including 04 chairs ","Nos ",{"v":1,"d":"1.00"}]
[{"v":4,"d":"(4)"},"Exective Table 5ft x 2.5ft","Nos ",{"v":3,"d":"3.00"}]
[{"v":5,"d":"(5)"},"Exective Chair hight back","Nos ",{"v":4,"d":"4.00"}]
[{"v":6,"d":"(6)"},"banquet chair (Fabric, Steel frame)","Nos ",{"v":34,"d":"34.00"}]
[{"v":7,"d":"(7)"},"Readymade Work Station1200mm x 1200mm with patition (table 4drawer)","Nos ",{"v":3,"d":"3.00"}]
[{"v":8,"d":"(8)"},"Secretary Chair  (Fabric)","Nos ",{"v":10,"d":"10.00"}]
[{"v":9,"d":"(9)"},"Readymade Partition 1800mm x 3600mm","Nos ",{"v":1,"d":"1.00"}]
[{"v":10,"d":"(10)"},"Readymade Partition 1800mm x 5000mm","Nos ",{"v":1,"d":"1.00"}]
[]
[null,"BILL No:15 - FURNITURE"]
[null,"TOTAL OF BILL No:15 - Carried over to summary"]
[null,"BILL No: 16"]
[null,"COURT ROOMS FURNITURE "]
[]
[16.1,"General"]
[null,"(a) Rates shall include for all fixing, cutting, trimmings, nails, screws and other fixings according to manufacturers' instructions."]
[null,"(b) Rates shall include for timber priming and all putty work as specified in the drawing"]
[null,"(c) Rates shall include for all labour in framing, notching and fitting around projections, pipes, electrical fittings, hatches, grilles and similar complete with cleats, packers, wedges and timber beeding etc. similar and all nails and screws"]
[null,"(d) Rates shall include for fair edges, dressing over angle fillets, turning into grooves, all other labours, circular edges, nails, screws and other fixing and laps.  "]
[null,"(e) Rates shall include for supply of all required materials and complete installation of the furnishings."]
[null,"(f) All timber used for internal framework shall be applied with Solignum Timber Treatment chemical 24 hrs prior to fabrication of frame"]
[null,"(g) All dimensions shall be checked on site before fabrication"]
[null,"(h) All materials used shall be as specified by the architect as given in the drawings and specifications, unless otherwise specified"]
[]
[16.2,"Backdrop Panel (Court Room)"]
[null,"Finished with 3mm Nyatoh Veneer plywood in selected Matte-Clear Lacquer Spray finish.Standard internal frame work 600mm C/C."]
[null,"Refer to drawings.\n"]
[{"v":1,"d":"(1)"},"2770mm high and 6096mm wide panel","Nos ",{"v":1,"d":"1.00"}]
[16.3,"Judjes Panel Carpet"]
[null,"1696mm Wx 6090 mm Lx 305 mm H stage finished with Red Carpet on top and sides.","Nos ",{"v":1,"d":"1.00"}]
[]
[16.4,"Judges Panel Table"]
[{"v":1,"d":"(1)"},"Refer to drawings.","Nos ",{"v":1,"d":"1.00"}]
[null,"Judges Panel Table"]
[16.5,"Registrars/Lawyer/Witness Tables"]
[null,"Refer to drawings."]
[{"v":1,"d":"(1)"},"Table  1600x600mm","Nos ",{"v":1,"d":"1.00"}]
[{"v":1,"d":"(1)"},"Table  800x450mm","Nos ",{"v":5,"d":"5.00"}]
[16.6,"Stage flag"]
[null,"Refer to information sheet"]
[{"v":1,"d":"(1)"},"flag with ground post","Nos ",{"v":2,"d":"2.00"}]
[16.7,"Divider Partition"]
[null,"Refer to drawings."]
[{"v":1,"d":"(1)"},"900mm x 6096mm Divider Partition with 600mm door","Nos ",{"v":1,"d":"1.00"}]
[]
[null,"BILL No:16 - COURT ROOMS FURNITURE "]
[null,"TOTAL OF BILL No:16 - Carried over to summary"]
[null,"BILL No: 17"]
[null,"TENDERER'S ADJUSTMENTS"]
[]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[16.1,"Additions"]
[{"v":1,"d":"(1)"},"Preliminaries - Bill no. 1"]
[{"v":2,"d":"(2)"},"Concrete - Bill no. 2"]
[{"v":3,"d":"(3)"},"Masonry and plastering - Bill no. 3"]
[{"v":4,"d":"(4)"},"Wood & metal works - Bill no. 4"]
[{"v":5,"d":"(5)"},"Roofing - Bill no. 5"]
[{"v":6,"d":"(6)"},"Doors and windows - Bill no. 6"]
[{"v":7,"d":"(7)"},"Ceiling - Bill no. 7"]
[{"v":8,"d":"(8)"},"Painting - Bill no. 8"]
[{"v":9,"d":"(9)"},"Finishes - Bill no.  9"]
[{"v":10,"d":"(10)"},"Fire fighting system - Bill no.  10"]
[{"v":11,"d":"(11)"},"Hydraulics & Drainage -  Bill no.11"]
[{"v":12,"d":"(12)"},"Electrical Installation - Bill no. 12"]
[{"v":13,"d":"(13)"},"CCTV System (Securuty System) - Bill no. 13"]
[{"v":14,"d":"(14)"},"Air - condition system - Bill no. 14"]
[{"v":15,"d":"(15)"},"Furuiture - Bill no. 15"]
[{"v":16,"d":"(16)"},"Court Room Furuiture - Bill no. 16"]
[null,"ADDITIONS TOTAL"]
[]
[16.2,"Omissions"]
[{"v":1,"d":"(1)"},"Preliminaries - Bill no. 1"]
[{"v":2,"d":"(2)"},"Concrete - Bill no. 2"]
[{"v":3,"d":"(3)"},"Masonry and plastering - Bill no. 3"]
[{"v":4,"d":"(4)"},"Wood & metal works - Bill no. 4"]
[{"v":5,"d":"(5)"},"Roofing - Bill no. 5"]
[{"v":6,"d":"(6)"},"Doors and windows - Bill no. 6"]
[{"v":7,"d":"(7)"},"Ceiling - Bill no. 7"]
[{"v":8,"d":"(8)"},"Painting - Bill no. 8"]
[{"v":9,"d":"(9)"},"Finishes - Bill no.  9"]
[{"v":10,"d":"(10)"},"Fire fighting system - Bill no.  10"]
[{"v":11,"d":"(11)"},"Hydraulics & Drainage -  Bill no.11"]
[{"v":12,"d":"(12)"},"Electrical Installation - Bill no. 12"]
[{"v":13,"d":"(13)"},"CCTV System (Securuty System) - Bill no. 13"]
[{"v":14,"d":"(14)"},"Air - condition system - Bill no. 14"]
[{"v":15,"d":"(15)"},"Furuiture - Bill no. 15"]
[{"v":16,"d":"(16)"},"Court Room Furuiture - Bill no. 16"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 17- TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 17 - Carried over to summary"]
["BOUNDARY WALL"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"]
[null,"m - metre"]
[null,"No - numbers"]
[null,"m³ - cubic metre"]
[null,"m² - square metre"]
[null,"Lm - Linear metre"]
[null,"t - tonnes"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[1.2,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","item",{"v":1,"d":"1.00"}]
{"$rows_empty":14}
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"GROUND WORKS"]
[]
[2.1,"General"]
[null,"(a) Rates shall include for: leveling, grading, trimming, compacting to faces of excavation, keep sides plumb, backfilling, consolidating and disposing surplus soil."]
[]
[2.2,"Excavation"]
[null,"(a) Excavation quantities are measured to the faces of concrete members. Rates shall include for all additional excavation required to place the formwork. "]
[null,"Excavation for "]
[{"v":1,"d":"(1)"},"Footing Beam.","m³",4.85]
{"$rows_empty":22}
[null,"BILL No: 02 - GROUND WORKS"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"CONCRETE"]
[]
[3.1,"General"]
[null,"(a) Rates shall include for: placing in position; making good after removal of formwork and casting in all required items; additional concrete required to conform to structural and excavated tolerances."]
[null,"(b) Mix ratio for  reinforced concrete shall be 1:2:3 and lean concrete shall be 1:2:6 by volume."]
[]
[3.2,"Plain Concrete"]
[null,"(a) Quantity is measured to the edges of concrete foundation members. Rates shall be inclusive for any additional concrete required to place the formwork."]
[{"v":1,"d":"(1)"},"50mm thick lean concrete to bottom of footing beam.","m³",1.53]
[]
[3.3,"Reinforced Concrete"]
[" ","In-situ reinforced concrete to:"]
[]
["3.3.1","Foundations"]
[{"v":1,"d":"(1)"},"Footing Beam","m³",4.85]
[]
["3.3.2","Above Ground"]
[{"v":1,"d":"(1)"},"Stiffner Columns","m³",1.21]
[{"v":2,"d":"(2)"},"Capping Beam","m³",2.42]
[]
[3.4,"Formwork"]
[null,"(a) Rates shall include for: all necessary boarding, supports, erecting, framing, temporary cambering, cutting, perforations for reinforcing bars, bolts, straps, ties, hangers, pipes and removal of formwork."]
["3.4.1","Foundations"]
[{"v":1,"d":"(1)"},"Footing Beam","m²",50.89]
[]
[]
["3.4.2","Above Ground"]
[{"v":1,"d":"(1)"},"Stiffner Columns","m²",33.93]
[{"v":2,"d":"(2)"},"Capping Beam","m²",38.78]
[]
[]
[3.5,"Reinforcement"]
[null,"(a) Rates shall include for: cleaning, fabrication, placing, the provision for all necessary temporary fixings, and supports including tie wire and chair supports, laps, distribution bars, spacer bar  and wastage."]
[null,"(b) All reinforcing bars shall be high strength bars."]
[]
["3.5.1","Foundation"]
[{"v":1,"d":"(1)"},"Footing Beam"]
[null,"10mm dia bars ","kg",361.11]
[null,"6mm dia bars","kg",{"v":112.7,"d":"112.70"}]
[]
[]
["3.5.2","Above Ground"]
[{"v":1,"d":"(1)"},"Stiffner Columns"]
[null,"10mm dia bars","kg",173.28]
[null,"6 mm dia bars","kg",38.78]
[]
[{"v":3,"d":"(3)"},"Capping Beam"]
[null,"10mm dia bars","kg",181.77]
[null,"6 mm dia bars","kg",15.75]
[]
[3.6,"Other concrete works"]
[]
["3.6.1","Water proofing"]
[null," Rates shall include for: dressing around and sealing to all penetrations"]
[]
[{"v":1,"d":"(1)"},"Bituminous paint waterproofing for all concrete surfaces  below ground level","m²",76.34]
{"$rows_empty":15}
[null,"BILL No: 03 - CONCRETE WORKS"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No: 04"]
[null,"MASONRY AND PLASTERING"]
[]
[4.1,"General"]
[null,"(a) Rates shall include for: cleaning out cavities, forming rebated reveals and pointing and cleaning down to reveals where necessary; fractional size blocks, all necessary machine cutting, cutting or forming chases or edges of "]
[null,"floor slabs, cutting or leaving holes and openings as recesses for and building in pipes, conduits, sleeves and similar as required for all trades; leaving surfaces rough or raking out joints for plastering and flashings, bedding "]
[null,"frames or plates, building in joists, bearers or similar, temporary supports to openings, templates, reinforcement in walls and for all necessary making good"]
[]
[4.2,"Cement brickwork"]
["4.2.1","200mm thick cement solid blocks, laid on and incl. mortar  tie rods, compression joint gap filler, nylon/plastic mesh as specified."]
[{"v":1,"d":"(1)"},"External Wall","m²",145.41]
[]
[]
[4.3,"Plastering"]
[null,"(a) Cement plastering on walls and concrete surfaces as specified incl. wire mesh at the joints of concrete surfaces and walls "]
["4.3.1","15mm thick cement plastering  (surface of walls)"]
[{"v":1,"d":"(1)"},"Wall including capping beam.","m²",{"v":288.4,"d":"288.40"}]
[]
[]
[]
[]
[]
[null,"BILL No: 04 - MASONRY AND PLASTERING"]
[null,"TOTAL OF BILL No: 04 - Carried over to summary"]
[null,"BILL No: 05"]
[null,"METAL"]
[]
[5.1,"General"]
[null,"(a) Rates shall include for: all fabrication work, welding, marking, drilling for bolts including those securing timbers, steel plates, bolts, nuts and any type of washer, riveted work, counter sinking and tapping for bolts or machine screws."]
[null,"(b) Rates shall include for all painting and finishing as specified in the specification."]
[null,"(c) Rates shall include for fabrication and erection and temporary supports and fixing into position."]
[]
[]
[5.2,"GATES"]
[{"v":1,"d":"(1)"},"Fabricating and fixing of SS pipe gate as per the drawing ","item",{"v":2,"d":"2.00"}]
{"$rows_empty":22}
[null,"BILL No: 05 - METAL WORKS"]
[null,"TOTAL OF BILL No: 05 - Carried over to summary"]
[null,"BILL No: 06"]
[null,"PAINTING"]
[]
[6.1,"General"," "]
[null,"(a) Rates shall include for: the provision, erection and removal of scaffolding, preparation, rubbing down between coats and similar work, the protection and/or masking floors, fittings and similar work, removing and replacing door and window"]
[null,"(b) All painting work shall be carried in accordance with the Specifications"]
[null,"(c) Paint system shall be Dulux"]
[]
[6.2,"Wall painting"]
["6.2.1","Emulsion paint finish on cement plastered surfaces (external surface of wall)"]
[{"v":1,"d":"(1)"},"Baundary wall","m²",{"v":288.4,"d":"288.40"}]
{"$rows_empty":24}
[null,"BILL No :6 - PAINTING"]
[null,"TOTAL OF BILL No: 06 - Carried over to summary"]
[null,"BILL No:7"]
[null,"ELECTRICAL INSTALLATIONS"]
[]
[7.1,"General"]
[null,"(a) Rates shall include for: screws, nails, bolts, nuts, standard cable fixing or supporting clips, brackets, straps, rivets, plugs and all incidental accessories"]
[null,"(b) Rates for work in trench shall include for: excavation, maintaining faces of excavations, backfilling, compaction, appropriate cable covers, warning tape and disposal of surplus spoil"]
[null,"(c) Rates shall include for electrical conduits, fittings, equipment and similar all fixings to various building surfaces"]
[null,"(d) Each Light/ light fixture and its switch is measured as one  point; similarly each fan or each socket outlet is measured as one point;"]
[null,"(e) Rates shall include for supply and complete installation "]
[]
[7.2,"Electrical wiring"]
[null,"Electrical wiring with copper conductor cable in conduits in walls and in casing on soffits of slab as specified to:"]
[{"v":1,"d":"(1)"},"Wiring with 2.5 mm² cable to lighting","points",{"v":4,"d":"4.0"}]
[]
[7.3,"Lighting"]
[{"v":1,"d":"(1)"},"Waterproof Gate globe Light","no",{"v":4,"d":"4.0"}]
[]
[7.4,"Light switches"]
[null,"(a) All light switches shall be \"Clipsal\" or equivalent."]
[{"v":1,"d":"(1)"},"Photo cell switch","no",{"v":2,"d":"2.0"}]
[{"v":2,"d":"(2)"},"One Gang switch","no",{"v":2,"d":"2.0"}]
[]
[]
[]
[]
[]
[]
[null,"BILL No: 7- ELECTRICAL INSTALLATIONS"]
[null,"TOTAL OF BILL No: 07 - Carried over to summary"]
[null,"BILL No: 8"]
[null,"TENDER'S ADJUSTMENT"]
[]
[8.1,"Additions"]
[{"v":1,"d":"(1)"},"Preliminaries - Bill 01"]
[{"v":2,"d":"(2)"},"Ground works - Bill 02"]
[{"v":3,"d":"(3)"},"Concrete - Bill 03"]
[{"v":4,"d":"(4)"},"Masonry andPlastering - Bill 04"]
[{"v":5,"d":"(5)"},"Metal works - Bill 05"]
[{"v":6,"d":"(6)"},"Painting - Bill 06"]
[{"v":7,"d":"(7)"},"Electric Installation - Bill 07"]
[]
[]
[8.2,"Omissions"]
[{"v":1,"d":"(1)"},"Preliminaries - Bill 01"]
[{"v":2,"d":"(2)"},"Ground works - Bill 02"]
[{"v":3,"d":"(3)"},"Concrete - Bill 03"]
[{"v":4,"d":"(4)"},"Masonry andPlastering - Bill 04"]
[{"v":5,"d":"(5)"},"Metal works - Bill 05"]
[{"v":6,"d":"(6)"},"Painting - Bill 06"]
[{"v":7,"d":"(7)"},"Electric Installation - Bill 07"]
{"$rows_empty":7}
[null,"BILL No: 8 - TENDER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 08 - Carried over to summary"]