Specification for Layer 2+ Manage Switch

|  |  |
| --- | --- |
| Interfaces | **24 x 1Gb RJ-45 Ports****2x 10Gb sfp+ Uplink Ports (Minimum)** |
| Max packet forwarding Rate | **Higher than 35 Mpps** |
| FEATURES | **Supported features:*** **Port-based VLAN**
* **Loopback Detection**
* **WEB UI**
 |