Specification for Layer 2+ Manage Switch

|  |  |
| --- | --- |
| Interfaces | **24 x 1Gb RJ-45 Ports**  **2x 10Gb sfp+ Uplink Ports (Minimum)** |
| Max packet forwarding Rate | **Higher than 35 Mpps** |
| FEATURES | **Supported features:**   * **Port-based VLAN** * **Loopback Detection** * **WEB UI** |