|  |  |  |  |
| --- | --- | --- | --- |
| Mandatory PPE for everyday use. *PPE obligatorio para el uso diario*. | | | |
| Image result for v guard hard hat Hard hat  *Casco* | Image result for safety glassesSafety glasses  *Lentes de*  *seguridad* | Image result for type 3 vestReflective Vest  *Chaleco* | Image result for work bootWork boots  *Botas de trabajo* |

Drills

|  |  |
| --- | --- |
| Image result for Drill | Related imageImage result for respiratorImage result for face shield hard hatImage result for ear plugs    (if above PEL) (if flying Debris) (if above PEL) |
| Image result for Drill | DeWalt DWH050K Large Hammer Dust Extraction - Hole CleaningImage result for dewalt vacuumRelated imageImage result for respiratorImage result for breaker plug extension cord  Image result for face shield hard hat    (if above PEL for silica dust) |
| Image result for portable drill press | DeWalt DWH050K Large Hammer Dust Extraction - Hole CleaningImage result for dewalt vacuumImage result for respiratorRelated image    Image result for respirator  (if above PEL) (silica dust) |

Saws

|  |  |
| --- | --- |
| Image result for quick saw | Image result for welding pantsImage result for water pump sprayerRelated imageImage result for face shield hard hat  Concrete  (Cut Retardant,  Leather Mat.)    (if above PEL) |
| Image result for welding pantsImage result for respiratorRelated imageImage result for face shield hard hatImage result for fire extinguisher  Metal  (Cut Retardant,  Leather Mat.)  (if above PELP) |
| Image result for skil saw | Image result for respiratorRelated image  (if above PEL) |
| Image result for chain saw | Related imageImage result for cut resistant pants  (Cut Retardant,  Nylon Mat.) |
| Image result for chop saw | Related image |
| Image result for saw saw | Image result for respiratorRelated imageImage result for face shield hard hat  Image result for construction goggles (if above PEL) |

Pneumatic – (jack hammers, chipping guns, rivet busters, impact wrenches, scalers, tie tampers, nail guns)

|  |  |
| --- | --- |
| Image result for pneumatic chipping hammer | DeWalt DWH050K Large Hammer Dust Extraction - Hole CleaningImage result for dewalt vacuumImage result for respiratorImage for West Chester Pro Series SM Brute Patch Palm Foam Gel Gloves from White Cap (if above PEL for silica dust) |
| Image result for pneumatic jack hammer | DeWalt DWH050K Large Hammer Dust Extraction - Hole CleaningImage result for metal toe guard constructionImage result for respiratorImage for West Chester Pro Series SM Brute Patch Palm Foam Gel Gloves from White CapImage result for face shield hard hat (anti-vibration gloves) (if visible dust) |

Compactors

|  |  |
| --- | --- |
| Image result for hand compactors | Image for West Chester Pro Series SM Brute Patch Palm Foam Gel Gloves from White Cap  Image result for metal toe guard construction |
| Image result for hand compactors | Image for West Chester Pro Series SM Brute Patch Palm Foam Gel Gloves from White Cap |

\*\*PEL: Permissible Exposure Limit\*\*

|  |  |  |  |
| --- | --- | --- | --- |
| Mandatory PPE for everyday use. *PPE obligatorio para el uso diario*. | | | |
| Image result for v guard hard hat Hard hat  *Casco* | Image result for safety glassesSafety glasses  *Lentes de*  *seguridad* | Image result for type 3 vestReflective Vest  *Chaleco* | Image result for work bootWork boots  *Botas de trabajo* |

Grinders

|  |  |
| --- | --- |
| Image result for grinder | Image result for dewalt grinder vacuum attachmentImage result for dewalt vacuumImage result for dewalt grinder vacuum attachmentImage for ATG MaxiGard LG Dyneema Nitrile Coated Level 5 Cut Resistant Gloves from White CapImage result for welding pantsImage result for respiratorImage result for fire extinguisher  Image result for no loose clothing sign  (ANSI 5 CUT) (if above PEL for silica dust) |

Percussion – (hammer, hammer drills, rotary hammer)

|  |  |
| --- | --- |
| Image result for hammer drill | Image result for dewalt vacuumRelated image (if above PEL  for silica dust)  DeWalt DWH050K Large Hammer Dust Extraction - Hole Cleaning  (if flying debris) |

Welding Machine

|  |  |
| --- | --- |
| Image result for stick welding machine | 9040Image result for welding jacketImage result for welding sleevesImage result for welding pantsImage result for respiratorImage result for welding helmets leather jacket,  chaps, or sleeves  depending (if above PEL)  on task |

Cutting Torch

|  |  |
| --- | --- |
| Image result for cutting torch | 9040Image result for cutting torch gogglesImage result for welding jacketImage result for welding sleevesImage result for welding pantsImage result for respirator leather jacket,  chaps, or sleeves  depending (if above PEL)  on task |

Concrete Vibrator

|  |  |
| --- | --- |
| Image result for concrete vibrator | Image result for anti-vibration glovesImage result for rubber bootsRelated image (anti-vibration gloves) (Boots need to be taped when work in concrete) |

Pressure Washer

|  |  |
| --- | --- |
| Image result for pressure washer | Related image |

Weed Eater

|  |  |
| --- | --- |
| Image result for weed eater | Related image |

Post Pounder

|  |  |
| --- | --- |
| Image result for Post pounder | Related image |

Gloves

|  |  |
| --- | --- |
| General Wet/Oil Grip Gloves; | Image for Brigade Sm Gray 15 Ga Nylon With Black Foam Nitrile Dipped Palm Gloves from White Cap |

|  |  |
| --- | --- |
| General Duty Leather Gloves; | Image for West Chester SM Select Grain Pigskin Gloves from White CapRelated image |

|  |  |
| --- | --- |
| Dorsal Impact Gloves; | Image for West Chester Pro Series SM Brute Patch Palm Foam Gel Gloves from White Cap |

ANSI 3 CUT ANSI 5 CUT

|  |  |
| --- | --- |
| Chemical Gloves; | Image for West Chester 14 |

|  |  |
| --- | --- |
| Wedding Gloves;  Wear when: wedding, torch cutting, | 9040 |

|  |  |
| --- | --- |
| ANSI 3 CUT & ANSI 5 CUT; | Image for West Chester LG Gray Posigrip PU Dipped ANSI 3 Cut Resistant Gloves from White CapImage for ATG MaxiGard LG Dyneema Nitrile Coated Level 5 Cut Resistant Gloves from White Cap |