;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 08/28/2014,11.0.0000.00000
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat

[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1


[Manufacturer]
%ProviderName% = Google, NTx86, NTamd64


[Google.NTx86]

;Google Nexus One
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01

;Google Nexus S
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01

;Google Nexus 7
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01

;Google Nexus Q
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11

;Google Nexus (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001

;Google Glass
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01

;Google Glass EE1

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9003
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9003&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_9004

;Google Glass EE2

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9005
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9005&MI_00
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_9006

;Project Tango (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4D00
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D02&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D04&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D06&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D07

;FCNT (BLG)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1011&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1012&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1013&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1014&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103F

;FCNT (KOT)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1016&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1018&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1040

;FCNT (SBS)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1020&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1022&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1023&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1048&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1049&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1041

;FCNT (SBR)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1042

;FCNT (SBD)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1030&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1033&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1043

;FCNT (TUB)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1037&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1038&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1044

;FCNT7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1051
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1053&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1055&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1058&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1059&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105B&MI_03

;FCNT8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1061&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1062&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1064&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1065&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1066&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1067&MI_03

;FCNT9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1069
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1070&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1071&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1072&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1073&MI_03

;FCNT10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1075
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1077&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1079&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107F&MI_03

;FCNT11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1081
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1083&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1085&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1086&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1088&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1089&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108B&MI_03

;FCNT12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1091&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1092&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1094&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1095&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1096&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1097&MI_03

;FCNT13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1099
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A3&MI_03

;FCNT14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AE&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AF&MI_03

;FCNT15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BA&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BB&MI_02

;FCNT1-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BD
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C8&MI_01

;FCNT1-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D4&MI_01

;FCNT1-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DE&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DF&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E0&MI_01

;FCNT1-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E9&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EA&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EC&MI_01

;FCNT1-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10ED
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F8&MI_01

;FCNT1-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1100&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1101&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1102&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1103&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1104&MI_01

;FCNT1-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1105
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1107&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1109&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1110&MI_01

;FCNT1-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1111
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1113&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1115&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1116&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1118&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1119&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111C&MI_01

;FCNT1-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1121&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1122&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1124&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1125&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1126&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1127&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1128&MI_01

;FCNT1-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1129
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1130&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1131&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1132&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1133&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1134&MI_01

;FCNT1-11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1135
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1137&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1139&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1140&MI_01

;FCNT1-12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1141
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1143&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1145&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1146&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1148&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1149&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114C&MI_01

;FCNT1-13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1151&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1152&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1154&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1155&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1156&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1157&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1158&MI_01

;FCNT1-14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1159
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1160&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1161&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1162&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1163&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1164&MI_01

;FCNT1-15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1165
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1167&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1169&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1170&MI_01

;FCNT1-16
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1171
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1173&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1175&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1176&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1178&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1179&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117C&MI_01

;FCNT2-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1181&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1182&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1184&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1185&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1186&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1187&MI_02

;FCNT2-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1188
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1190&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1191&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1192&MI_02

;FCNT2-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1193
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1195&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1197&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1198&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119B&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119C&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119D&MI_02

;FCNT2-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119E
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A8&MI_02

;FCNT2-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B3&MI_02

;FCNT2-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BB&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BC&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BD&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BE&MI_02

;FCNT2-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BF
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C9&MI_02

;FCNT2-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CA
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D4&MI_02

;FCNT2-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DD&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DE&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DF&MI_02

;FCNT2-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E0
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EA&MI_02

;FCNT1-17
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F6&MI_01

;FCNT1-18
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FF&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1200&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1201&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1202&MI_01

;FCNT1-19
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1203
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1205&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1207&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1208&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120E&MI_01

;FCNT1-20
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120F
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1211&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1213&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1214&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1216&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1217&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1218&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1219&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121A&MI_01

;FCNT1-21
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1220&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1222&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1223&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1224&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1225&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1226&MI_01

;FCNT1-22
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1227
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1229&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1230&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1231&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1232&MI_01

;FCNT1-23
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1233
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1235&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1237&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1238&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123E&MI_01

;FCNT1-24
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123F
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1241&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1243&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1244&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1246&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1247&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1248&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1249&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124A&MI_01

;FCNT1-25
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1250&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1252&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1253&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1254&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1255&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1256&MI_01

;FCNT1-26
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1257
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1259&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1260&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1261&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1262&MI_01

;FCNT3-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1263
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1265&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1267&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1268&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126A&MI_02

;FCNT3-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1270&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1272&MI_02

;FCNT3-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1273
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1275&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1277&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1278&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127A&MI_02

;FCNT3-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1280&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1282&MI_02

;FCNT3-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1283
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1285&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1287&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1288&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128A&MI_02

;FCNT3-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1290&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1292&MI_02

;FCNT3-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1293
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1295&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1297&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1298&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129A&MI_02

;FCNT3-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A2&MI_02

;FCNT3-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AA&MI_02

;FCNT3-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B2&MI_02

;FCNT3-11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BA&MI_02

;FCNT3-12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C2&MI_02

;FCNT3-13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CA&MI_02

;FCNT3-14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D2&MI_02

;FCNT3-15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DA&MI_02

;FCNT3-16
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E2&MI_02

;FCNT3-17
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EA&MI_02

;FCNT3-18
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F2&MI_02

;FCNT3-19
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12FA&MI_02

;FCNT3-20
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x1300&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x1302&MI_02

;FCNT3-21
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1303
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1305&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1307&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1308&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130A&MI_02

;FCNT3-22
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1310&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1312&MI_02

;FCNT3-23
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1313
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1315&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1317&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1318&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131A&MI_02

;FCNT3-24
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1320&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1322&MI_02

;FCNT3-25
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1323
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1325&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1327&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1328&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132A&MI_02

;FCNT3-26
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1330&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1332&MI_02

;FCNT3-27
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1333
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1335&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1337&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1338&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133A&MI_02

;FCNT3-28
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1340&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1342&MI_02

;FCNT3-29
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1343
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1345&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1347&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1348&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134A&MI_02

;FCNT3-30
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1350&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1352&MI_02

;FCNT3-31
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1353
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1355&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1357&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1358&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135A&MI_02

;FCNT3-32
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1360&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1362&MI_02

;FCNT3-33
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1363
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1365&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1367&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1368&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136A&MI_02

;FCNT3-34
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1370&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1372&MI_02

;FCNT3-35
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1373
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1375&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1377&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1378&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137A&MI_02

;FCNT3-36
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1380&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1382&MI_02

;FCNT3-37
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1383
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1385&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1387&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1388&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138A&MI_02

;FCNT3-38
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1390&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1392&MI_02

;FCNT3-39
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1393
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1395&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1397&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1398&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139A&MI_02

;FCNT3-40
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A2&MI_02

;FCNT3-41
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AA&MI_02

;FCNT3-42
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B2&MI_02

;FCNT3-43
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BA&MI_02

;FCNT3-44
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C2&MI_02

;FCNT3-45
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CA&MI_02

;FCNT3-46
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D2&MI_02

;FCNT3-47
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DA&MI_02

;FCNT3-48
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E2&MI_02

;FCNT3-49
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EA&MI_02

;FCNT3-50
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F2&MI_02

[Google.NTamd64]

;Google Nexus One
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01

;Google Nexus S
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01

;Google Nexus 7
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01

;Google Nexus Q
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11

;Google Nexus (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001

;Google Glass
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01

;Google Glass EE1

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9003
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9003&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_9004

;Google Glass EE2

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9005
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9005&MI_00
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_9006

;Project Tango (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4D00
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D02&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D04&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D06&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D07

;FCNT (BLG)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_100F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1011&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1012&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1013&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1014&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103F

;FCNT (KOT)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1016&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1018&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_101E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1040

;FCNT (SBS)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1020&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1022&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1023&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1048&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1049&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1041

;FCNT (SBR)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1042

;FCNT (SBD)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_102E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1030&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1033&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_104F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1043

;FCNT (TUB)
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1037&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1038&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_103D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1044

;FCNT7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1051
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1053&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1055&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1058&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1059&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105B&MI_03

;FCNT8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_105F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1061&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1062&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1064&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1065&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1066&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1067&MI_03

;FCNT9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1069
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_106E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1070&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1071&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1072&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1073&MI_03

;FCNT10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1075
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1077&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1079&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_107F&MI_03

;FCNT11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1081
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1083&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1085&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1086&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1088&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1089&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108B&MI_03

;FCNT12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_108F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1091&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1092&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1094&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1095&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1096&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1097&MI_03

;FCNT13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1099
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_109E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A3&MI_03

;FCNT14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AE&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10AF&MI_03

;FCNT15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10B9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BA&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BB&MI_02

;FCNT1-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BD
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C8&MI_01

;FCNT1-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10C9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10CE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D4&MI_01

;FCNT1-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10D9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DE&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10DF&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E0&MI_01

;FCNT1-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10E9&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EA&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EC&MI_01

;FCNT1-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10ED
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F8&MI_01

;FCNT1-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10F9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_10FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1100&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1101&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1102&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1103&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1104&MI_01

;FCNT1-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1105
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1107&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1109&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_110F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1110&MI_01

;FCNT1-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1111
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1113&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1115&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1116&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1118&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1119&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111C&MI_01

;FCNT1-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_111F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1121&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1122&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1124&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1125&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1126&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1127&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1128&MI_01

;FCNT1-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1129
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_112E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1130&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1131&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1132&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1133&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1134&MI_01

;FCNT1-11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1135
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1137&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1139&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_113F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1140&MI_01

;FCNT1-12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1141
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1143&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1145&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1146&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1148&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1149&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114C&MI_01

;FCNT1-13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_114F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1151&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1152&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1154&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1155&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1156&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1157&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1158&MI_01

;FCNT1-14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1159
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_115E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1160&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1161&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1162&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1163&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1164&MI_01

;FCNT1-15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1165
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1167&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1169&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_116F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1170&MI_01

;FCNT1-16
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1171
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1173&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1175&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1176&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1178&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1179&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117C&MI_01

;FCNT2-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117D
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_117F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1181&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1182&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1184&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1185&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1186&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1187&MI_02

;FCNT2-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1188
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_118F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1190&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1191&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1192&MI_02

;FCNT2-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1193
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1195&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1197&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1198&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119B&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119C&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119D&MI_02

;FCNT2-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_119E
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A8&MI_02

;FCNT2-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11A9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11AE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B3&MI_02

;FCNT2-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11B9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BB&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BC&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BD&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BE&MI_02

;FCNT2-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11BF
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11C9&MI_02

;FCNT2-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CA
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11CF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D4&MI_02

;FCNT2-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11D9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DD&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DE&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11DF&MI_02

;FCNT2-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E0
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11E9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EA&MI_02

;FCNT1-17
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F6&MI_01

;FCNT1-18
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_11FF&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1200&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1201&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1202&MI_01

;FCNT1-19
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1203
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1205&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1207&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1208&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120E&MI_01

;FCNT1-20
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_120F
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1211&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1213&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1214&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1216&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1217&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1218&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1219&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121A&MI_01

;FCNT1-21
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_121F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1220&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1222&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1223&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1224&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1225&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1226&MI_01

;FCNT1-22
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1227
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1229&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_122F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1230&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1231&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1232&MI_01

;FCNT1-23
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1233
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1235&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1237&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1238&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123E&MI_01

;FCNT1-24
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_123F
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1241&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1243&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1244&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1246&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1247&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1248&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1249&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124A&MI_01

;FCNT1-25
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_124F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1250&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1252&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1253&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1254&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1255&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1256&MI_01

;FCNT1-26
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1257
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1259&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_125F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1260&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1261&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1262&MI_01

;FCNT3-1
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1263
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1265&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1267&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1268&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126A&MI_02

;FCNT3-2
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_126F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1270&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1272&MI_02

;FCNT3-3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1273
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1275&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1277&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1278&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127A&MI_02

;FCNT3-4
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_127F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1280&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1282&MI_02

;FCNT3-5
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1283
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1285&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1287&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1288&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128A&MI_02

;FCNT3-6
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_128F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1290&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1292&MI_02

;FCNT3-7
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1293
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1295&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1297&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1298&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129A&MI_02

;FCNT3-8
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_129F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A2&MI_02

;FCNT3-9
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12A8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AA&MI_02

;FCNT3-10
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B2&MI_02

;FCNT3-11
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BA&MI_02

;FCNT3-12
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C2&MI_02

;FCNT3-13
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CA&MI_02

;FCNT3-14
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D2&MI_02

;FCNT3-15
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12D8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DA&MI_02

;FCNT3-16
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12DE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E2&MI_02

;FCNT3-17
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EA&MI_02

;FCNT3-18
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F2&MI_02

;FCNT3-19
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12F8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_12FA&MI_02

;FCNT3-20
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x12FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x1300&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_0x1302&MI_02

;FCNT3-21
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1303
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1305&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1307&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1308&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130A&MI_02

;FCNT3-22
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_130F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1310&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1312&MI_02

;FCNT3-23
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1313
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1315&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1317&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1318&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131A&MI_02

;FCNT3-24
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_131F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1320&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1322&MI_02

;FCNT3-25
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1323
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1325&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1327&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1328&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132A&MI_02

;FCNT3-26
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_132F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1330&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1332&MI_02

;FCNT3-27
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1333
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1335&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1337&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1338&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133A&MI_02

;FCNT3-28
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_133F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1340&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1342&MI_02

;FCNT3-29
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1343
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1345&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1347&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1348&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134A&MI_02

;FCNT3-30
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_134F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1350&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1352&MI_02

;FCNT3-31
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1353
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1355&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1357&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1358&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135A&MI_02

;FCNT3-32
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_135F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1360&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1362&MI_02

;FCNT3-33
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1363
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1365&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1367&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1368&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136A&MI_02

;FCNT3-34
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_136F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1370&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1372&MI_02

;FCNT3-35
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1373
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1375&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1377&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1378&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137A&MI_02

;FCNT3-36
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_137F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1380&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1382&MI_02

;FCNT3-37
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1383
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1385&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1387&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1388&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138A&MI_02

;FCNT3-38
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_138F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1390&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1392&MI_02

;FCNT3-39
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1393
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1395&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1397&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_1398&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139A&MI_02

;FCNT3-40
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139B
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_139F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A2&MI_02

;FCNT3-41
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13A8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AA&MI_02

;FCNT3-42
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B2&MI_02

;FCNT3-43
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13B8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BA&MI_02

;FCNT3-44
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C2&MI_02

;FCNT3-45
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CA&MI_02

;FCNT3-46
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D2&MI_02

;FCNT3-47
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13D8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DA&MI_02

;FCNT3-48
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13DF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E2&MI_02

;FCNT3-49
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EA&MI_02

;FCNT3-50
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EB
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13ED&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F2&MI_02

;generic
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F3
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13F8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_30EE&PID_13FA&MI_02

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "Google, Inc."
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Device"
