(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "1.8V")
  (net 2 "3.3V")
  (net 3 "GND")
  (net 4 "AVDD")
  (net 5 "AGND")
  (net 6 "N$1")
  (net 7 "N$2")
  (net 8 "GPIO5")
  (net 9 "GPIO0")
  (net 10 "GPIO1")
  (net 11 "GPIO4")
  (net 12 "GPIO2")
  (net 13 "GPIO3")
  (net 14 "GPIO6")
  (net 15 "GPIO7")
  (net 16 "MISO")
  (net 17 "MOSI_3V")
  (net 18 "SCLK_3V")
  (net 19 "TX")
  (net 20 "RX")
  (net 21 "CS_3V")
  (net 22 "MICP")
  (net 23 "MICN")
  (net 24 "RST_3V")
  (net 25 "DREQ")
  (net 26 "SDCS_3V")
  (net 27 "CLKOUT")
  (net 28 "LEFT")
  (net 29 "RIGHT")
  (net 30 "N$5")
  (net 31 "N$6")
  (net 32 "RIGHT_FILTERED")
  (net 33 "LEFT_FILTERED")
  (net 34 "MOSI_5V")
  (net 35 "CS_5V")
  (net 36 "SDCS_5V")
  (net 37 "XDCS_3V")
  (net 38 "XDCS_5V")
  (net 39 "RST_5V")
  (net 40 "SCLK_5V")
  (net 41 "SD_DETECT")
  (net 42 "RX_5V")
  (net 43 "R_LINEOUT")
  (net 44 "L_LINEOUT")
  (net 45 "LINE2")
  (net 46 "N$13")
  (net 47 "N$17")
  (net 48 "~{RESET}")
  (net 49 "N$19")
  (net 50 "N$20")
  (net 51 "N$3")
  (net 52 "N$4")
  (net 53 "N$7")
  (net 54 "N$25")
  (net 55 "N$28")
  (net 56 "N$29")
  (net 57 "N$30")
  (net 58 "N$36")
  (net 59 "N$37")
  (net 60 "N$38")
  (net 61 "N$39")
  (net 62 "N$40")
  (net 63 "N$41")
  (net 64 "+5V")
  (net 65 "GAIN0")
  (net 66 "SHUTDOWN")
  (net 67 "OUT-L-N")
  (net 68 "OUT-L-P")
  (net 69 "OUT-R-N")
  (net 70 "OUT-R-P")
  (net 71 "N$8")
  (net 72 "N$9")
  (net 73 "N$10")
  (net 74 "N$11")
  (net 75 "N$14")
  (net 76 "N$12")
  (net 77 "N$15")
  (net 78 "N$16")
  (net 79 "N$21")
  (net 80 "D13")
  (net 81 "D11")
  (net 82 "D12")
  (net 83 "D10")
  (net 84 "D9")
  (net 85 "D8")
  (net 86 "N$18")
  (net 87 "N$22")
  (net 88 "N$23")
  (net 89 "N$24")
  (net 90 "N$26")
  (net 91 "N$27")
  (net 92 "N$31")
  (net 93 "GBUF")
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 159.996 52.580895 180)
    (fp_text reference "C3" (at -1.5125 1.0525) (layer "F.SilkS"))
    (fp_text value "10µF" (at 2.4765 0.508) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X07_ROUND_70" (layer "F.Cu")
    (tedit 0)
    (at 238.794 96.716)
    (fp_text reference "JP7" (at -8.9662 -1.8288) (layer "F.SilkS"))
    (fp_text value "" (at -8.89 3.175) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -7.62 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 39 "RST_5V") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at -5.08 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 66 "SHUTDOWN") (solder_mask_margin 0.0508))
    (pad "3" thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 19 "TX") (solder_mask_margin 0.0508))
    (pad "4" thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 42 "RX_5V") (solder_mask_margin 0.0508))
    (pad "5" thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 41 "SD_DETECT") (solder_mask_margin 0.0508))
    (pad "6" thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 35 "CS_5V") (solder_mask_margin 0.0508))
    (pad "7" thru_hole circle (at 7.62 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 38 "XDCS_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805_10MGAP" (layer "F.Cu")
    (tedit 0)
    (at 227.237 122.243 180)
    (fp_text reference "C24" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at -1.778 -1.143) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 1.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "MICP") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.05 0 180) (size 1.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 246.414 100.78 90)
    (fp_text reference "R19" (at -1.5875 -0.9525 90) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.0795 -0.762 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "XDCS_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:PANASONIC_C" (layer "F.Cu")
    (tedit 0)
    (at 218.965 114.326)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C</b>")
    (fp_text reference "C2" (at -2.95 -1.3 90) (layer "F.SilkS"))
    (fp_text value "220uF" (at 1.941 -0.381) (layer "F.Fab"))
    (pad "+" smd rect (at 2.05 0) (size 2.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "LEFT_FILTERED") (solder_mask_margin 0.0508))
    (pad "-" smd rect (at -2.05 0) (size 2.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "L_LINEOUT") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 215.134 105.994 -90)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "C19" (at -1.5875 -1.1525 90) (layer "F.SilkS"))
    (fp_text value "10µF" (at 1.2065 -1.905 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 270) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 270) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 248.573 100.78 90)
    (fp_text reference "R20" (at -1.5875 -0.9525 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.8415 0.381 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "SDCS_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 238.154 126.926 90)
    (fp_text reference "C20" (at -0.5125 1.0525 90) (layer "F.SilkS"))
    (fp_text value "10µF" (at 1.6825 2.296 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 246.054 115.226 180)
    (fp_text reference "C5" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "15pF" (at -4.0005 0.127) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N$1") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 231.428 118.179)
    (fp_text reference "C23" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at -1.397 0.508) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "MICN") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X03-CLEANBIG" (layer "F.Cu")
    (tedit 0)
    (at 138.0111 127.3336 90)
    (fp_text reference "JP2" (at 3.5062 1.4288 90) (layer "F.SilkS"))
    (fp_text value "" (at -3.81 3.175 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.54 0 180) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "MICN") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at 0 0 180) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "MICP") (solder_mask_margin 0.0508))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "LINE2") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOIC16" (layer "F.Cu")
    (tedit 0)
    (at 219.744 99.256 90)
    (descr "<b>SMALL OUTLINE INTEGRATED CIRCUIT</b>")
    (fp_text reference "U5" (at -3.937 -0.381 90) (layer "F.SilkS"))
    (fp_text value "74HC4050D" (at -3.937 4.445 90) (layer "F.Fab"))
    (pad "1" smd rect (at -4.445 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at -3.175 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "RST_3V") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "RST_5V") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "CS_3V") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "CS_5V") (solder_mask_margin 0.0508))
    (pad "6" smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "XDCS_3V") (solder_mask_margin 0.0508))
    (pad "7" smd rect (at 3.175 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "XDCS_5V") (solder_mask_margin 0.0508))
    (pad "8" smd rect (at 4.445 2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "9" smd rect (at 4.445 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "SCLK_5V") (solder_mask_margin 0.0508))
    (pad "10" smd rect (at 3.175 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "SCLK_3V") (solder_mask_margin 0.0508))
    (pad "11" smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "MOSI_5V") (solder_mask_margin 0.0508))
    (pad "12" smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "MOSI_3V") (solder_mask_margin 0.0508))
    (pad "13" smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
    (pad "14" smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "SDCS_5V") (solder_mask_margin 0.0508))
    (pad "15" smd rect (at -3.175 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "SDCS_3V") (solder_mask_margin 0.0508))
    (pad "16" smd rect (at -4.445 -2.6 90) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_REFLOW_NOPASTE" (layer "F.Cu")
    (tedit 0)
    (at 254.923 102.812 180)
    (fp_text reference "SJ3" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "ISCP_SCLK" (at -14.097 3.5369 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 78 "N$16") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 40 "SCLK_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 229.635 107.253 180)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "FB2" (at -0.2125 1.6525) (layer "F.SilkS"))
    (fp_text value "FERITTE" (at 1.0605 -0.5096) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.606 114.242)
    (fp_text reference "R17" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GPIO6") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 231.597 120.053)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "FB1" (at -1.8125 -0.8475) (layer "F.SilkS"))
    (fp_text value "FERITTE" (at 2.868293 -0.270993) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "AVDD") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 243.054 112.026 90)
    (fp_text reference "R1" (at -1.5875 -0.9525 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.8227 -0.635 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N$1") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "N$2") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 237.354 123.888)
    (fp_text reference "C6" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "10µF" (at 1.9685 -2.159) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:WQFN20" (layer "F.Cu")
    (tedit 0)
    (at 147.907 50.157895 180)
    (descr "<p>20-PWQFN 4.0x4.0mm 0.5mm pitch</p>\n<b>Source</b>: http://www.ti.com/lit/ds/symlink/tpa2012d2.pdf")
    (fp_text reference "U4" (at -2.024 -2.532) (layer "F.SilkS"))
    (fp_text value "TS2012" (at -3.167 1.516) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 1.975 180) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 90 "N$26") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at -0.5 1.975 180) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 68 "OUT-L-P") (solder_mask_margin 0.0508))
    (pad "3" smd roundrect (at 0 1.975 180) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "4" smd roundrect (at 0.5 1.975 180) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "5" smd roundrect (at 1 1.975 180) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 67 "OUT-L-N") (solder_mask_margin 0.0508))
    (pad "6" smd roundrect (at 1.975 1 270) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
    (pad "7" smd roundrect (at 1.975 0.5 270) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 66 "SHUTDOWN") (solder_mask_margin 0.0508))
    (pad "8" smd roundrect (at 1.975 0 270) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 66 "SHUTDOWN") (solder_mask_margin 0.0508))
    (pad "9" smd roundrect (at 1.975 -0.5 270) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 75 "N$14") (solder_mask_margin 0.0508))
    (pad "10" smd roundrect (at 1.975 -1 270) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
    (pad "11" smd roundrect (at 1 -1.975) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 69 "OUT-R-N") (solder_mask_margin 0.0508))
    (pad "12" smd roundrect (at 0.5 -1.975) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "13" smd roundrect (at 0 -1.975) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "14" smd roundrect (at -0.5 -1.975) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 70 "OUT-R-P") (solder_mask_margin 0.0508))
    (pad "15" smd roundrect (at -1 -1.975) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 65 "GAIN0") (solder_mask_margin 0.0508))
    (pad "16" smd roundrect (at -1.975 -1 90) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 74 "N$11") (solder_mask_margin 0.0508))
    (pad "17" smd roundrect (at -1.975 -0.5 90) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 73 "N$10") (solder_mask_margin 0.0508))
    (pad "18" smd roundrect (at -1.975 0 90) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 76 "N$12") (solder_mask_margin 0.0508))
    (pad "19" smd roundrect (at -1.975 0.5 90) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 72 "N$9") (solder_mask_margin 0.0508))
    (pad "20" smd roundrect (at -1.975 1 90) (size 0.28 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
      (net 71 "N$8") (solder_mask_margin 0.0508))
    (pad "21" smd rect (at 0 0 180) (size 2.45 2.45) (layers "F.Cu" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 141.638 51.187895 180)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "FB3" (at 2.0125 2.3475) (layer "F.SilkS"))
    (fp_text value "ferrite" (at -0.6705 -0.362) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "N$14") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 216.414 124.577 180)
    (fp_text reference "C12" (at -2.0125 -0.3475) (layer "F.SilkS"))
    (fp_text value "1µF" (at -1.8975 -0.031) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "N$9") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 225.554 115.242 180)
    (fp_text reference "R3" (at -2.2125 -3.1475) (layer "F.SilkS"))
    (fp_text value "22" (at -0.6985 0.381) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "LEFT") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "N$5") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOD-323" (layer "F.Cu")
    (tedit 0)
    (at 239.543 100.899 -90)
    (descr "<b>SOD323</b> (2.5x1.2mm)")
    (fp_text reference "D1" (at 0.6 1.1 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -2.878 1.919 90) (layer "F.Fab"))
    (pad "A" smd rect (at 1.27 0 270) (size 1.35 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "RX") (solder_mask_margin 0.0508))
    (pad "C" smd rect (at -1.27 0 270) (size 1.35 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "RX_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_ARROW_NOPASTE" (layer "F.Cu")
    (tedit 0)
    (at 144.164 54.289895)
    (fp_text reference "SJ1" (at -1.778 -1.27) (layer "F.SilkS"))
    (fp_text value "+6dB" (at -1.651 1.651) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.016 0) (size 0.762 1.524) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 65 "GAIN0") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 1.016 0) (size 0.762 1.524) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 64 "+5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.606 126.942)
    (fp_text reference "R8" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GPIO1") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:TERMBLOCK_1X2-3.5MM" (layer "F.Cu")
    (tedit 0)
    (at 116.697 127.107 -90)
    (fp_text reference "LEFTSPK0" (at -3 -3.89 90) (layer "F.SilkS"))
    (fp_text value "3.5mm Term" (at -5.588 5.715 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 1.8 0 270) (size 2.1844 2.1844) (drill 1) (layers *.Cu *.Mask)
      (net 67 "OUT-L-N") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at -1.7 0 270) (size 2.1844 2.1844) (drill 1) (layers *.Cu *.Mask)
      (net 68 "OUT-L-P") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 122.941 50.682895)
    (fp_text reference "C11" (at 2.0125 1.6475) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 1.9685 0.254) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOD-323" (layer "F.Cu")
    (tedit 0)
    (at 230.285 102.685 90)
    (descr "<b>SOD323</b> (2.5x1.2mm)")
    (fp_text reference "D2" (at -1.1 -1 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 2.583 0.014 90) (layer "F.Fab"))
    (pad "A" smd rect (at 1.27 0 90) (size 1.35 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "RST_5V") (solder_mask_margin 0.0508))
    (pad "C" smd rect (at -1.27 0 90) (size 1.35 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "~{RESET}") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 231.154 126.926 -90)
    (fp_text reference "C7" (at -0.8125 1.0525 90) (layer "F.SilkS"))
    (fp_text value "10µF" (at -1.8415 -0.508 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:LQFP48" (layer "F.Cu")
    (tedit 0)
    (at 236.054 111.526 90)
    (fp_text reference "U1" (at -2.974 -5.3001 90) (layer "F.SilkS"))
    (fp_text value "VS1053B" (at 2.6409 3.3311) (layer "F.Fab"))
    (pad "1" smd rect (at -4.2 -2.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 22 "MICP") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at -4.2 -2.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 23 "MICN") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at -4.2 -1.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 24 "RST_3V") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at -4.2 -1.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at -4.2 -0.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
    (pad "6" smd rect (at -4.2 -0.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "7" smd rect (at -4.2 0.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
    (pad "8" smd rect (at -4.2 0.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 25 "DREQ") (solder_mask_margin 0.0508))
    (pad "9" smd rect (at -4.2 1.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 12 "GPIO2") (solder_mask_margin 0.0508))
    (pad "10" smd rect (at -4.2 1.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 13 "GPIO3") (solder_mask_margin 0.0508))
    (pad "11" smd rect (at -4.2 2.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 14 "GPIO6") (solder_mask_margin 0.0508))
    (pad "12" smd rect (at -4.2 2.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 15 "GPIO7") (solder_mask_margin 0.0508))
    (pad "13" smd rect (at -2.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 37 "XDCS_3V") (solder_mask_margin 0.0508))
    (pad "14" smd rect (at -2.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "15" smd rect (at -1.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 27 "CLKOUT") (solder_mask_margin 0.0508))
    (pad "16" smd rect (at -1.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "17" smd rect (at -0.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 6 "N$1") (solder_mask_margin 0.0508))
    (pad "18" smd rect (at -0.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 7 "N$2") (solder_mask_margin 0.0508))
    (pad "19" smd rect (at 0.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "20" smd rect (at 0.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "21" smd rect (at 1.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "22" smd rect (at 1.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "23" smd rect (at 2.25 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 21 "CS_3V") (solder_mask_margin 0.0508))
    (pad "24" smd rect (at 2.75 4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
    (pad "25" smd rect (at 4.2 2.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 8 "GPIO5") (solder_mask_margin 0.0508))
    (pad "26" smd rect (at 4.2 2.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 20 "RX") (solder_mask_margin 0.0508))
    (pad "27" smd rect (at 4.2 1.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 19 "TX") (solder_mask_margin 0.0508))
    (pad "28" smd rect (at 4.2 1.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 18 "SCLK_3V") (solder_mask_margin 0.0508))
    (pad "29" smd rect (at 4.2 0.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 17 "MOSI_3V") (solder_mask_margin 0.0508))
    (pad "30" smd rect (at 4.2 0.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 16 "MISO") (solder_mask_margin 0.0508))
    (pad "31" smd rect (at 4.2 -0.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
    (pad "32" smd rect (at 4.2 -0.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "33" smd rect (at 4.2 -1.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 9 "GPIO0") (solder_mask_margin 0.0508))
    (pad "34" smd rect (at 4.2 -1.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 10 "GPIO1") (solder_mask_margin 0.0508))
    (pad "35" smd rect (at 4.2 -2.25 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "36" smd rect (at 4.2 -2.75 90) (size 1.1 0.285) (layers "F.Cu" "F.Paste")
      (net 11 "GPIO4") (solder_mask_margin 0.0508))
    (pad "37" smd rect (at 2.75 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "38" smd rect (at 2.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 4 "AVDD") (solder_mask_margin 0.0508))
    (pad "39" smd rect (at 1.75 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 29 "RIGHT") (solder_mask_margin 0.0508))
    (pad "40" smd rect (at 1.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "41" smd rect (at 0.75 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "42" smd rect (at 0.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 93 "GBUF") (solder_mask_margin 0.0508))
    (pad "43" smd rect (at -0.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 4 "AVDD") (solder_mask_margin 0.0508))
    (pad "44" smd rect (at -0.75 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 91 "N$27") (solder_mask_margin 0.0508))
    (pad "45" smd rect (at -1.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 4 "AVDD") (solder_mask_margin 0.0508))
    (pad "46" smd rect (at -1.75 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 28 "LEFT") (solder_mask_margin 0.0508))
    (pad "47" smd rect (at -2.25 -4.2 90) (size 0.285 1.1) (layers "F.Cu" "F.Paste")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "48" smd rect (at -2.75 -4.2 90) (size 0.28 1.1) (layers "F.Cu" "F.Paste")
      (net 45 "LINE2") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "F.Cu")
    (tedit 0)
    (at 259.622 102.812 180)
    (fp_text reference "SJ6" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "D13_SCLK" (at -13.335 3.302 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 80 "D13") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 40 "SCLK_5V") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 180) (size 0.635 0.2032) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_REFLOW_NOPASTE" (layer "F.Cu")
    (tedit 0)
    (at 254.923 105.352 180)
    (fp_text reference "SJ4" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "ICSP_MOSI" (at -15.367 6.2039 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 77 "N$15") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 34 "MOSI_5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "F.Cu")
    (tedit 0)
    (at 259.622 105.352 180)
    (fp_text reference "SJ7" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "D11_MOSI" (at -14.732 5.461 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 81 "D11") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 34 "MOSI_5V") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 180) (size 0.635 0.2032) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.606 124.275)
    (fp_text reference "R13" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "GPIO2") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_REFLOW_NOPASTE" (layer "F.Cu")
    (tedit 0)
    (at 254.923 100.272 180)
    (fp_text reference "SJ2" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "ICSP_MISO" (at -12.7 0.9969 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 79 "N$21") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 16 "MISO") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 226.189 109.51)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "R6" (at -2.1525 0.6875 90) (layer "F.SilkS"))
    (fp_text value "100" (at 1.2065 -0.508) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "RIGHT_FILTERED") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "RIGHT") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 132.861 52.003895 180)
    (fp_text reference "C16" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "10µF" (at -1.8415 1.778) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.479 116.655)
    (fp_text reference "R16" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "GPIO5") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.479 121.735)
    (fp_text reference "R14" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "GPIO3") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:CRYSTAL_3.2X2.5" (layer "F.Cu")
    (tedit 0)
    (at 246.054 112.126 90)
    (descr "3.2mm x 2.5mm Thin SMT Crystal")
    (fp_text reference "Y1" (at 0.632 2.278 90) (layer "F.SilkS"))
    (fp_text value "ABM8G-12.288MHZ-4Y-T3" (at 6.9822 4.0686 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.8 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "N$1") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.1 -0.8 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "N$2") (solder_mask_margin 0.0508))
    (pad "GND1" smd rect (at -1.1 -0.8 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
    (pad "GND2" smd rect (at 1.1 0.8 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOT23-6" (layer "F.Cu")
    (tedit 0)
    (at 234.654 126.926 -90)
    (descr "<b>Small Outline Transistor</b> - 6 Pin")
    (fp_text reference "U2" (at -2 0.749) (layer "F.SilkS"))
    (fp_text value "AP7312-1833W6-7" (at 4.029 6.671) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0 1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at 0.95 1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at 0.95 -1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at 0 -1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "6" smd rect (at -0.95 -1.3 270) (size 0.55 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1.8V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 228.647 102.389 -90)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "C26" (at 1.9125 0.7475 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -2.5195 0.026 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 270) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "RST_5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 270) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 122.941 48.926895 180)
    (fp_text reference "C10" (at -2.0125 -0.8475) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.8695 -0.439) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "N$12") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 226.189 106.237)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "C22" (at -1.1875 -1.1525) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 1.6415 -0.6324) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "N$6") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 119.286 48.950895)
    (fp_text reference "C9" (at 0.6875 1.7525) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -2.2225 0.381) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "N$14") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "N$12") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 223.173 111.702 180)
    (fp_text reference "C18" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "0.047uF" (at -1.778 0.127) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "N$31") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:4UCONN_19269" (layer "F.Cu")
    (tedit 0)
    (at 114.8461 105.5116)
    (descr "<br>\n4UCONN: 19269\n<br>\n4UCONN: 19268\n<br>\n4UCONN: 19267\n<br>\nhttp://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19267&seriesno_a=18")
    (fp_text reference "X1" (at 5.85 -3.61) (layer "F.SilkS"))
    (fp_text value "19621" (at 4.445 4.445) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 10.5 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "1" smd rect (at 2.5 3.5) (size 2 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 11.7 3.5) (size 2 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "L_LINEOUT") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at 4.3 -3.5) (size 2 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "R_LINEOUT") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at 15.8 -0.75 90) (size 2 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "L_LINEOUT") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at 1.5 -3.5) (size 1.2 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "R_LINEOUT") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 225.554 113.415)
    (fp_text reference "R7" (at -2.0525 0.5875 90) (layer "F.SilkS"))
    (fp_text value "100" (at 1.0795 -0.508) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "LEFT_FILTERED") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "LEFT") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 226.729 119.703 180)
    (fp_text reference "C25" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at -1.905 0.254) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "LINE2") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:EVQ-Q2" (layer "F.Cu")
    (tedit 0)
    (at 116.986 53.527895)
    (fp_text reference "SW2" (at -3 -3.5) (layer "F.SilkS"))
    (fp_text value "SPST_TACT-EVQQ2" (at -5.994 -4.852) (layer "F.Fab"))
    (pad "A" smd rect (at -3.4 2) (size 3.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "~{RESET}") (solder_mask_margin 0.0508))
    (pad "A'" smd rect (at 3.4 2) (size 3.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "~{RESET}") (solder_mask_margin 0.0508))
    (pad "B" smd rect (at -3.4 -2) (size 3.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "B'" smd rect (at 3.4 -2) (size 3.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 216.414 128.204 180)
    (fp_text reference "C14" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "1µF" (at -2.0245 -0.397) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "RIGHT") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "N$11") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 233.079 101.288)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "R9" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.2065 -1.143) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "RST_5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X10_ROUND70" (layer "F.Cu")
    (tedit 0)
    (at 144.4371 84.6836)
    (fp_text reference "JP6" (at 3.4242 1.6088) (layer "F.SilkS"))
    (fp_text value "" (at -12.7 3.175) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -11.43 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 51 "N$3") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at -8.89 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 52 "N$4") (solder_mask_margin 0.0508))
    (pad "3" thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 53 "N$7") (solder_mask_margin 0.0508))
    (pad "4" thru_hole circle (at -3.81 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "5" thru_hole circle (at -1.27 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 80 "D13") (solder_mask_margin 0.0508))
    (pad "6" thru_hole circle (at 1.27 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 82 "D12") (solder_mask_margin 0.0508))
    (pad "7" thru_hole circle (at 3.81 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 81 "D11") (solder_mask_margin 0.0508))
    (pad "8" thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 83 "D10") (solder_mask_margin 0.0508))
    (pad "9" thru_hole circle (at 8.89 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 84 "D9") (solder_mask_margin 0.0508))
    (pad "10" thru_hole circle (at 11.43 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 85 "D8") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 235.111 104.209 90)
    (fp_text reference "R2" (at 2.032 0.127 90) (layer "F.SilkS"))
    (fp_text value "100K" (at -1.905 2.032 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "GPIO0") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 90) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 240.199 104.218)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "R10" (at 0.8875 1.17) (layer "F.SilkS"))
    (fp_text value "10K" (at 2.5876 0.109) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "RX") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.479 119.195)
    (fp_text reference "R15" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 2.032 0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "GPIO4") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 216.414 122.75 180)
    (fp_text reference "C13" (at -2.0125 -0.1475) (layer "F.SilkS"))
    (fp_text value "1µF" (at -2.0245 -0.002) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "LEFT") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "N$8") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 222.792 117.29 -90)
    (fp_text reference "C27" (at 2.032 0.127 90) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at -2.413 0.508 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "LEFT_FILTERED") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_ARROW_NOPASTE" (layer "F.Cu")
    (tedit 0)
    (at 216.315 120.719)
    (fp_text reference "SJ12" (at -1.778 -1.27) (layer "F.SilkS"))
    (fp_text value "+12dB" (at -1.651 1.651) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.016 0) (size 0.762 1.524) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 90 "N$26") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 1.016 0) (size 0.762 1.524) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 64 "+5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 223.427 109.035 -90)
    (fp_text reference "C28" (at 2.032 0.127 90) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 1.143 -0.635 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "RIGHT_FILTERED") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:2X07_ROUND_70MIL" (layer "F.Cu")
    (tedit 0)
    (at 254.034 119.576 90)
    (fp_text reference "MP3GPIO0" (at -9.475 2.49) (layer "F.SilkS") hide)
    (fp_text value "" (at -8.89 4.445 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -7.62 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at -7.62 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 10 "GPIO1") (solder_mask_margin 0.0508))
    (pad "3" thru_hole circle (at -5.08 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "4" thru_hole circle (at -5.08 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 12 "GPIO2") (solder_mask_margin 0.0508))
    (pad "5" thru_hole circle (at -2.54 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "6" thru_hole circle (at -2.54 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 13 "GPIO3") (solder_mask_margin 0.0508))
    (pad "7" thru_hole circle (at 0 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "8" thru_hole circle (at 0 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 11 "GPIO4") (solder_mask_margin 0.0508))
    (pad "9" thru_hole circle (at 2.54 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "10" thru_hole circle (at 2.54 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GPIO5") (solder_mask_margin 0.0508))
    (pad "11" thru_hole circle (at 5.08 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "12" thru_hole circle (at 5.08 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 14 "GPIO6") (solder_mask_margin 0.0508))
    (pad "13" thru_hole circle (at 7.62 1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "14" thru_hole circle (at 7.62 -1.27 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GPIO7") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X06-CLEANBIG" (layer "F.Cu")
    (tedit 0)
    (at 171.3611 125.3236 180)
    (fp_text reference "JP8" (at -4.1038 1.5288) (layer "F.SilkS"))
    (fp_text value "" (at -7.62 3.175) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 58 "N$36") (solder_mask_margin 0.0508))
    (pad "2" thru_hole roundrect (at -3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 59 "N$37") (solder_mask_margin 0.0508))
    (pad "3" thru_hole roundrect (at -1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 60 "N$38") (solder_mask_margin 0.0508))
    (pad "4" thru_hole roundrect (at 1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 61 "N$39") (solder_mask_margin 0.0508))
    (pad "5" thru_hole roundrect (at 3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 62 "N$40") (solder_mask_margin 0.0508))
    (pad "6" thru_hole roundrect (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 63 "N$41") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 243.874 100.78 -90)
    (fp_text reference "R21" (at -1.5875 -0.9525 90) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.4605 2.413 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "CS_5V") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 229.65 105.606 180)
    (fp_text reference "C17" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "1µF" (at -1.27 0.635) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "N$27") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 226.729 111.702 180)
    (fp_text reference "R5" (at 2.032 0.127) (layer "F.SilkS"))
    (fp_text value "10" (at -0.762 0.381) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "GBUF") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "N$31") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:MICROSD" (layer "F.Cu")
    (tedit 0)
    (at 128.998 65.746 -90)
    (descr "Courtesy: Adafruit Industries")
    (fp_text reference "CN1" (at 0.96 -0.73 90) (layer "F.SilkS"))
    (fp_text value "2908-05WB-M6" (at 1.287 8.004 90) (layer "F.Fab"))
    (pad "1" smd rect (at 9 10.64 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 7.9 10.24 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "SDCS_3V") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at 6.8 10.64 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "MOSI_3V") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at 5.7 11.04 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "3.3V") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at 4.6 10.64 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "SCLK_3V") (solder_mask_margin 0.0508))
    (pad "6" smd rect (at 3.5 11.04 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "7" smd rect (at 2.4 10.64 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "MISO") (solder_mask_margin 0.0508))
    (pad "8" smd rect (at 1.3 10.64 270) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
    (pad "CD1" smd rect (at 2 0.44) (size 1.4 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "SD_DETECT") (solder_mask_margin 0.0508))
    (pad "CD2" smd rect (at 8 0.44) (size 1.4 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.0508))
    (pad "MT1" smd rect (at 0.4 13.54 270) (size 1.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "MT2" smd rect (at 13.6 14.44 270) (size 1.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 138.406 50.596895)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "R12" (at 2.0125 0.6475) (layer "F.SilkS"))
    (fp_text value "100K" (at -1.4605 -1.27) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "SHUTDOWN") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "+5V") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:TERMBLOCK_1X2-3.5MM" (layer "F.Cu")
    (tedit 0)
    (at 116.762 140.35 -90)
    (fp_text reference "RIGHTSPK0" (at -2.1 -3.89 90) (layer "F.SilkS"))
    (fp_text value "3.5mm Term" (at -2.54 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 1.8 0 270) (size 2.1844 2.1844) (drill 1) (layers *.Cu *.Mask)
      (net 70 "OUT-R-P") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at -1.7 0 270) (size 2.1844 2.1844) (drill 1) (layers *.Cu *.Mask)
      (net 69 "OUT-R-N") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 258.225 111.194 -90)
    (fp_text reference "R18" (at 2.032 0.127 90) (layer "F.SilkS"))
    (fp_text value "100K" (at -2.032 -1.27 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GPIO7") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "F.Cu")
    (tedit 0)
    (at 259.622 100.272 180)
    (fp_text reference "SJ5" (at -1.651 -1.27) (layer "F.SilkS"))
    (fp_text value "D12_MISO" (at -12.065 0.508 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 82 "D12") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers "F.Cu" "F.Mask")
      (net 16 "MISO") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 180) (size 0.635 0.2032) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 225.554 117.069)
    (fp_text reference "C21" (at 2.2125 0.3475) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 2.4865 -0.469) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "N$5") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X08-CLEANBIG" (layer "F.Cu")
    (tedit 0)
    (at 151.0411 125.3236 180)
    (fp_text reference "JP4" (at -6.8038 1.5288) (layer "F.SilkS"))
    (fp_text value "" (at -10.16 3.175) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at -8.89 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 46 "N$13") (solder_mask_margin 0.0508))
    (pad "2" thru_hole roundrect (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "3" thru_hole roundrect (at -3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "4" thru_hole roundrect (at -1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 64 "+5V") (solder_mask_margin 0.0508))
    (pad "5" thru_hole roundrect (at 1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 47 "N$17") (solder_mask_margin 0.0508))
    (pad "6" thru_hole roundrect (at 3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 48 "~{RESET}") (solder_mask_margin 0.0508))
    (pad "7" thru_hole roundrect (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 49 "N$19") (solder_mask_margin 0.0508))
    (pad "8" thru_hole roundrect (at 8.89 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 50 "N$20") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:PANASONIC_C" (layer "F.Cu")
    (tedit 0)
    (at 218.965 108.726)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C</b>")
    (fp_text reference "C1" (at -2.95 -1.1 90) (layer "F.SilkS"))
    (fp_text value "220uF" (at 2.154 -0.408) (layer "F.Fab"))
    (pad "+" smd rect (at 2.05 0) (size 2.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "RIGHT_FILTERED") (solder_mask_margin 0.0508))
    (pad "-" smd rect (at -2.05 0) (size 2.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "R_LINEOUT") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 119.286 50.613895)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "FB4" (at -2.0125 -0.0475) (layer "F.SilkS"))
    (fp_text value "ferrite" (at -0.7265 -0.522) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "N$12") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X08-CLEANBIG" (layer "F.Cu")
    (tedit 0)
    (at 168.8211 84.6836)
    (fp_text reference "JP1" (at 9.8162 1.7088) (layer "F.SilkS"))
    (fp_text value "" (at -10.16 3.175) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at -8.89 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 86 "N$18") (solder_mask_margin 0.0508))
    (pad "2" thru_hole roundrect (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 87 "N$22") (solder_mask_margin 0.0508))
    (pad "3" thru_hole roundrect (at -3.81 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 54 "N$25") (solder_mask_margin 0.0508))
    (pad "4" thru_hole roundrect (at -1.27 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 89 "N$24") (solder_mask_margin 0.0508))
    (pad "5" thru_hole roundrect (at 1.27 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 88 "N$23") (solder_mask_margin 0.0508))
    (pad "6" thru_hole roundrect (at 3.81 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 55 "N$28") (solder_mask_margin 0.0508))
    (pad "7" thru_hole roundrect (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 56 "N$29") (solder_mask_margin 0.0508))
    (pad "8" thru_hole roundrect (at 8.89 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 57 "N$30") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 226.189 107.937 180)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "R4" (at -2.6125 -0.4475) (layer "F.SilkS"))
    (fp_text value "22" (at -0.9525 0.381) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "RIGHT") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 180) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "N$6") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 216.414 126.377 180)
    (fp_text reference "C15" (at -2.0125 -0.3475) (layer "F.SilkS"))
    (fp_text value "1µF" (at -2.0245 -0.368) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "N$10") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:_0805MP" (layer "F.Cu")
    (tedit 0)
    (at 229.281 111.526 90)
    (descr "<b>0805 MicroPitch</b>")
    (fp_text reference "C8" (at -0.7875 -0.9525 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -1.5891 0.525 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.016 0 90) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "AVDD") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 1.016 0 90) (size 1.2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "AGND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:1X02_ROUND" (layer "F.Cu")
    (tedit 0)
    (at 252.764 96.716)
    (fp_text reference "JP3" (at -2.6162 -1.8288) (layer "F.SilkS"))
    (fp_text value "" (at -2.54 3.175) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.27 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 36 "SDCS_5V") (solder_mask_margin 0.0508))
    (pad "2" thru_hole circle (at 1.27 0 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 25 "DREQ") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:0805-NO" (layer "F.Cu")
    (tedit 0)
    (at 246.054 109.026)
    (fp_text reference "C4" (at -1.5875 -0.9525) (layer "F.SilkS"))
    (fp_text value "15pF" (at -1.9685 -0.762) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "N$2") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.95 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "B.Cu")
    (tedit 0)
    (at 254.034 94.176 -90)
    (fp_text reference "SJ11" (at -1.651 1.27 -270) (layer "B.SilkS"))
    (fp_text value "" (at -1.524 -1.651 -270) (layer "B.Fab"))
    (pad "1" smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 88 "N$23") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 25 "DREQ") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 270) (size 0.635 0.2032) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "B.Cu")
    (tedit 0)
    (at 251.494 94.176 -90)
    (fp_text reference "SJ10" (at -1.651 1.27 -270) (layer "B.SilkS"))
    (fp_text value "" (at -1.524 -1.651 -270) (layer "B.Fab"))
    (pad "1" smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 89 "N$24") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 36 "SDCS_5V") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 270) (size 0.635 0.2032) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "B.Cu")
    (tedit 0)
    (at 246.414 94.176 -90)
    (fp_text reference "SJ9" (at -1.651 1.27 -270) (layer "B.SilkS"))
    (fp_text value "" (at -1.524 -1.651 -270) (layer "B.Fab"))
    (pad "1" smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 87 "N$22") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 38 "XDCS_5V") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 270) (size 0.635 0.2032) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.0508))
  )
  (footprint "Qplayer unplaced unrouted original size:SOLDERJUMPER_CLOSEDWIRE" (layer "B.Cu")
    (tedit 0)
    (at 243.874 94.176 -90)
    (fp_text reference "SJ8" (at -1.651 1.27 -270) (layer "B.SilkS"))
    (fp_text value "" (at -1.524 -1.651 -270) (layer "B.Fab"))
    (pad "1" smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 86 "N$18") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers "B.Cu" "B.Mask")
      (net 35 "CS_5V") (solder_mask_margin 0.0508))
    (pad "WIRE" smd rect (at 0 0 270) (size 0.635 0.2032) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.0508))
  )
  (gr_rect (start 112.718 62.346) (end 204.811 147.377) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "RST" (at 147.3581 88.6206 90) (layer "F.SilkS"))
  (gr_text "L2" (at 135.8941 123.5516 90) (layer "F.SilkS"))
  (gr_text "RX" (at 155.3111 88.5186 90) (layer "F.SilkS"))
  (gr_text "Stereo" (at 119.7991 109.9566) (layer "F.SilkS"))
  (gr_text "MCS" (at 160.3121 88.4936 90) (layer "F.SilkS"))
  (gr_text "+12dB" (at 129.8321 112.6236) (layer "F.SilkS"))
  (gr_text "DRQ" (at 170.5991 88.4936 90) (layer "F.SilkS"))
  (gr_text "M+" (at 135.9541 126.0646 90) (layer "F.SilkS"))
  (gr_text "Reset" (at 127.0381 84.1756 90) (layer "F.SilkS"))
  (gr_text "DCS" (at 162.8521 88.4936 90) (layer "F.SilkS"))
  (gr_text "CCS" (at 167.9321 88.4936 90) (layer "F.SilkS"))
  (gr_text "M-" (at 135.9141 128.7316 90) (layer "F.SilkS"))
  (gr_text "TX" (at 152.9581 88.5186 90) (layer "F.SilkS"))
  (gr_text "Line Out" (at 121.3231 101.9556) (layer "F.SilkS"))
  (gr_text "CD" (at 157.9181 88.5186 90) (layer "F.SilkS"))
  (gr_text "+ R -" (at 123.1011 125.7046 90) (layer "F.SilkS"))
  (gr_text "SPK\nOff" (at 151.0411 88.6206 90) (layer "F.SilkS"))
  (gr_text "- L +" (at 123.1011 118.3386 90) (layer "F.SilkS"))
  (gr_text "Mic In" (at 140.1191 129.5146 90) (layer "F.SilkS"))
)
