I suggest using my universal print files (gcodes) instead of slicing.

Upload the gcodes on an SD card and insert it in the printer. Launch the gcode from the printer interface. Adjust temperature once the print starts to fit your filament needs.

Printer requirements for the gcodes: 0.4mm or 0.6mm nozzle and at least 180x180mm buildplate 


Website: https://www.riverfamily.art/

Contact: alessio@riverfamily.art

How to slice: https://www.youtube.com/watch?v=9SbpQj1s48o


Settings (Cura):
- layer height: 0.3mm
- line width: 0.6mm
- wall line count: 0
- top layers: 0
- bottom layers: 0
- initial bottom layers: 0
- infill line distance: 6mm
- infill pattern: grid
- connect infill lines: yes
- infill line direction: [90,0]


settings modifier 
- wall line count: 6


LICENSE: Public Domain

https://creativecommons.org/share-your-work/public-domain/cc0/

Also applies to gcodes, slicing process, pictures, videos and names



