Watch this video to understand how Evo is made: https://www.youtube.com/watch?v=7STE_GT0obQ


Upload the universal Evo.gcode on an SD card and insert it in any printer. Launch the gcode from the printer interface, ignore warnings and proceed. Adjust temperature and fan speed once the print starts to fit your filament needs

Printer requirements for the gcodes: preferably 0.6mm nozzle and at least 180x180mm buildplate


Evo sliced with Bambu Studio has slightly different infill pattern with same functionality.


Evo works with 120mm fans. The frame of the fan has to be removed by cutting with pliers. Then the fan is attached to the cap mid-print with thick double-sided tape.

The best fan is UpHere, which is smaller then usual 120mm fans, that is why there is a custom "uphere" version of Evo. If you choose a USB fan, you can add a "usb fan speed controller" (Google it) to adjust and increase USB fan speed. 

Cut Hepa filters from "Frameless hepa filter" sheets (link1: https://aliexpress.com/item/4001298732898.html , link2: https://aliexpress.com/item/1005001619559275.html)



Cura slicer print settings:

Layer Height: 0.6
infill line width: 0.4
Infill Flow: 200%
wall line width: 1
Walls: 0
Bottom Layers: 0
Top Layers: 0
Infill Density: 9% (line distance 4.44mm)
Infill Pattern: Zig Zag
Infill Lines Direction: [0,0,0,30,30,30,60,60,60,120,120,120,150,150,150]
Infill Speed: 30 mm/s
Print cooling: off

Evo_2 (should be merged with Evo_1, Evo_3, Evo_4)
walls: 1
bottom layers: 100
initial bottom layers: 100
skin overlap %: 90%


Evo_3, Evo_4
infill line distance: 8
infill pattern: grid
infill line directions: [0,90]
infill flow: 300%


Pause for fan insertion inserted as follows (uncomment/comment to change for Prusa or Bambulab pause commands): 


G0 F42000 X128.66 Y63.115 Z33.9
;TIME_ELAPSED:2197.355497
;LAYER:55

;M400 U1 ; Bambulab pause
;M601 ; Prusa Pause

;Generic pause start
G0 X150.000 Y200.000 Z150.000 ; move away from the part

M18 S0 ; disable stepper inactivity timeout
M25 ; pause print

G0 X150.000 Y2000.000 Z151.000 ; buffer lines: some printers pause a few lines below M25
G0 X150.000 Y2000.000 Z152.000
G0 X150.000 Y2000.000 Z153.000
G0 X150.000 Y2000.000 Z154.000
G0 X150.000 Y2000.000 Z155.000
;Generic pause end



License Public Domain:
https://creativecommons.org/public-domain/cc0/