Fits any 120mm fan

Dome.gcode should work on any direct drive printer with 0.4mm/0.6mm nozzle and at least 150x150x150 build volume

Print time is around 3h, it pauses after around 1.5h at layer 112 to let fan insertion. Click to unpause 

It is sliced for PLA: 50° bed, 210° nozzle

Has been tested on:

- Prusa MK3S 0.4 nozzle 
- Prusa MK3S 0.6 nozzle 
- Prusa Mini 0.6 nozzle -> a lot of stringing
- Creality Ender 3 v2 0.6 nozzle -> a lot of stringing
- Qidi XMAX 0.6 nozzle -> a lot of stringing

Postprocess stringing with fire

If you test it on a different printer, please contact me to add it to the list 

If you manage to make a better .gcode, please share it with me

alessio@riverfamily.art



Print Settings:

dome_1.stl:

infill line width: 0.6
infill flow: 200% (might use 1.2mm line width with 100% infill flow instead)
bottom layers: 0
top layers: 0
walls: 0 
infill: grid
infill line distance: 8
Connect infill lines: no

dome_2.stl:

use it as modifier and merge it with dome_1.stl
bottom layers: 100
walls: 2

Insert M25 gcode at height 34mm to pause print for fan insertion 



LICENSE: Public Domain

https://creativecommons.org/share-your-work/public-domain/cc0/