Preferably use 0.6 nozzle

---

Bambu Studio / Orca Slicer settings:

Global, E7_1:
 
- layer height: 0.28mm
- line width sparse infill: 0.9mm
- line width walls: 0.65mm
- wall loops: 0
- top shell layers: 0
- bottom shell layers: 0
- sparse infill density: 43%
- Infill pattern: Grid
- Infill anchor: 1000 (unlimited)
- Max infill anchor: 1000 (unlimited)
- Infill direction: 45°
- infill/wall overlap: 90%
- Detect narrow internal solid infill: no
- Speed sparse infill: 18 mm/s
- Reduce infill retraction: no
- Enable support: no

E7_2:

Not merged with other models to ensure models overlapping for shoe integrity

- Walls: 2
- Sparse infill density: 100%
- Sparse infill pattern: rectilinear

E7_3:

- Sparse infill density: 33%
- Line width sparse infill: 0.6mm

E7_4:

- Part type: modifier
- Line width sparse infill: 1mm
- Sparse infill density: 80%


Filament:

- Retraction: 2.4mm
- Wipe: no
- Z hop: 1.2mm, Normal type
- Max volumetric speed: 4.8 mm^3/s 


---

Video: https://www.youtube.com/shorts/ZXtAueYBw-Y

How to design and slice: https://www.youtube.com/watch?v=nnkCee3quc0

Website: https://www.riverfamily.art/

---

LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names