Sizes: EU


---

Filament: Recreus 82A, 3Dfils 85A 

Use TPU 95A first (Overture), don't use "high speed", "high flow" (too stiff, uncomfortable)

Nozzle: preferably 0.6mm, especially with softer filaments

---

Bambu Studio settings:

Overlap 2 identical models, same settings except infill line direction.
A "grid" pattern is made by overlapping 2 perpendicular zigzag patterns. 

Global

- layer height: 0.28mm
- line width sparse infill: 72mm
- wall loops: 0
- top shell layers: 0
- bottom shell layers: 0
- sparse infill density: 19%
- Infill pattern: zigzag
- Infill anchor: 1000 (unlimited)
- Max infill anchor: 1000 (unlimited)
- Infill direction: 45° (model 1) - 135° (model 2)
- Detect narrow internal solid infill: no
- Speed sparse infill: 18 mm/s
- Enable support: no
- Reduce infill retraction: no

Cube modifier (256x256x1.1mm around height 1.5mm to make a 3 layers platform):

- Infill density: 80% (model 1) - 0% (model 2)
- Infill pattern: Rectilinear
- Infill direction: 0°
 
Filament:

- Retraction: 2.4mm
- Wipe: no
- Z hop: 1.2mm, Normal type
- Max volumetric speed: 4.8 mm^3/s 

---

Video: https://www.youtube.com/watch?v=0uL_TtakyKE

Website: https://www.riverfamily.art/

---

LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names