Shoes sizes: EU



For the insert search "insert liner fur clogs":

- link 1: https://aliexpress.com/item/1005006979682528.html
- link 2: https://aliexpress.com/item/1005006249804202.html



Use TPU 95A first. Overture is good, many other 95A break fast, don't use "high speed", "high flow" (too rigid).


Use the Bambu Studio profile or the universal print files (gcodes) instead of slicing the 3d models. 

Upload the gcodes on an SD card and insert it in any printer with 0.6mm nozzle and minimum 250x250mm buildplate (256x256 for EU 46 size). Launch the gcode from the printer interface, ignore warnings and proceed. Adjust temperature once the print starts to fit your filament needs 

Depending on the size, each shoe takes 4 to 6 hours, weights 60 to 90 grams


---

Bambu Studio / Orca Slicer settings

Shoe:

layer height: 0.2
line width sparse infill: 0.6mm
wall loops: 0
top shell layers: 0
bottom shell layers: 0
sparse infill density: 62%
Infill pattern: Grid
Infill anchor: 1000 (unlimited)
Max infill anchor: 1000 (unlimited)
Infill direction: 45°
Detect narrow internal solid infill: no
Speed sparse infill: 18 mm/s
Enable support: no
Reduce infill retraction: no


Filament:

Retraction: 1.8mm
Wipe: no
Z hop: 1.2mm, Normal type
Max volumetric speed: 4.8 mm^3/s 


---


Settings (Cura):

- place the model diagonally (45°)
- layer height: 0.3mm
- infill line width: 0.6mm
- wall line count: 0
- top layers: 0
- bottom layers: 0
- initial bottom layers: 0
- infill line distance: 2mm
- infill pattern: grid
- connect infill lines: yes
- infill line direction: []
- infill overlap: 0mm
- infill speed: 18mm/s


Website: https://www.riverfamily.art/


LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names