
Bambu Studio / Orca Slicer settings:

Global:

- layer height: 0.2mm
- line width sparse infill: 0.6mm
- line width outer wall: 0.69mm
- walls: 0
- top shell layers: 0
- bottom shell layers: 0
- infill density: 33%
- infill pattern: Grid
- infill anchor: 1000 (unlimited)
- max infill anchor: 1000 (unlimited)
- infill direction: 45°
- detect narrow internal solid infill: no
- speed sparse infill: 18 mm/s
- reduce infill retraction: no
- enable support: yes, threshold angle 1°, on build plate only, 2 support enforcers: fort and middle 

mare_1:

- walls: 1
- object flow ratio: 1.05
- infill density: 100%
- infill pattern: rectilinear

mare_2:

- line width sparse infill: 0.3mm
- object flow ratio: 2


Filament:

- Retraction: 1.8mm
- Wipe: no
- Z hop: 1.2mm, Normal type
- Max volumetric speed: 2.5 mm^3/s 
- Temperature: 220°C - 230°C

--- 

made with Stepan: https://drunks.st/

website: https://www.riverfamily.art/

---

LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names