MRX x10 software installation

1.  Copy the extracted .fw file to a USB stick, root directory.  Very important:  Make sure there is only ONE .fw file in the root directory and that it is the latest for your model.  US=120V, EU=240V, CN=240V. 

2.  Connect USB stick to MRX rear panel.

3.  Turn the unit on.  Once it has completed startup, long-press the Select button on the front panel (8 sec) until installation starts.  Installation can also be initiated via the setup menu.  Installation takes about 10 minutes.

Very important:  Do not interfere while software is being installed.  The unit will turn on and off a few times and power on to normal display when installation is complete.

If software installation does not start and the MRX AC cord needs to be disconnected/reconnected to make unit operable again, try another USB stick, preferably containing fewer files or without unneeded software that may come with new USB sticks.


Technical support:

http://www.anthemav.com/support/contact-us.php


Changes in v1.2.9:

1.  When using ARC v1.1.2882 or later to load a file, there is no longer a 3 dB level reduction when ARC is enabled in MRX.

2.  Fixes for certain cases of sub channel muting after changing speaker configuration or tone settings.

3.  Fix for AnthemLogic not appearing on selection list under certain conditions.

4.  After Process Analog Input was set to No in setup menu, the corresponding N/A menu items weren't being grayed - fixed.

5.  When Back Amp was set to Zone 2 and its volume was set much higher than Main volume, noises sometimes resulted while making other changes - fixed.

6.  Fix for Zone 2 volume being too high if power-on volume was lowered in setup menu and Z2 was power cycled.


Changes in v1.2.6:

1.  DSP meant for main outputs was being applied to headphone output - fixed.
2.  Tuner station was misreported via IP during station seek - fixed.
3.  PLII Music adjustments (Center Width etc) weren't being saved at power-off - fixed.
4.  HDMI issue with certain 4K TV - fixed.
5.  Renamed Control 4 drivers:

Anthem MRX-710.c4i
Anthem MRX-510.c4i
Anthem MRX-310.c4i

to

receiver_Anthem_MRX-710.c4i
receiver_Anthem_MRX-510.c4i
receiver_Anthem_MRX-310.c4i

Note: For new ARC measurement or upload, ARC v1.1.2882 should be used as v1.0.1.7 may not connect reliably.


Changes in v1.2.1:

1.  Fixed issue where with certain source components, the first half-second of music tracks was muted.

2.  Fixes for AnthemLogic availability for certain speaker configurations, and output levels.

3.  Added Control4 SDDP.

4.  Various fixes and improvements for serial and IP communication and feedback (refer to notes in latest IP/serial command list).

5.  Zone 2 audio output wasn't always muting when Main was on and Zone 2 was off - fixed.
