PART 1     GENERAL

1.1   SUMMARY
A. Section Includes:
1. All room identification, workstation ID’s and signage for ADA and life safety code compliance.

B. Related Sections:
1. Division 1:  Administrative, procedural and temporary work requirements.
1.2   REFERENCES
A. Signs and their installation shall comply with applicable provisions of the latest edition of the following standards and with requirements of authorities having jurisdiction:
1. ADAAG – Americans with Disabilities Act Accessibility Guidelines; US Architectural and Transportation Barriers Compliance Board.
2. International Code Council/American National Standards Institute A117.1-Standard on Accessible and Usable Buildings Facilities.
3. National Fire Protection Association 101 Life Safety Code.
1.3   SUBMITTALS
A. Submittals for Review:
1. Sign finishes, location plan and copy shall be submitted within an interactive web-based database allowing digital review and approval within the context of the floor plans.
2. Approval drawings showing materials, construction detail, lay-out, copy, size and mounting methods.
3. Engineering drawings for each sign type.

4. Sample of (2) sign types for verification of materials, color, pattern, overall quality, and for adherence to drawings and requirements indicated.
1.4   QUALIFICATIONS
A. Manufacturer specializing in manufacturing the products specified in this section shall have a minimum of five years’ experience.  All products must meet characteristics specified below when quoting an alternate.  Alternates should be closely similar to the dimensions, material, color, pattern, function and quality.  Alternate offerings shall provide samples of (2) sign types to architect and/or owner.  Failure to identify the products quoted as the requested brand name or “equal” products shall be considered non-responsive.  All signs shall be obtained from one source and a single manufacturer.
1.5   WARRANTY 
A. Provide manufacturer’s warranty against defects in materials and workmanship for minimum 5 years. 

PART 2     PRODUCTS

2.1   MANUFACTURER
A. Signage shall be Fine Line using Fusion construction as manufactured by Takeform, 1.800.528.1398, www.takeform.net or Architect approved equal.  

B.
Substitutions:  Bidder must obtain prior written approval from the Architect and/or Owner to bid alternates or substitutions to the specification.

2.2   SIGN STANDARDS

1. Engineered and Tested:

1. The signage system shall have undergone testing to ensure longevity and optimal performance as defined below.  Testing shall include environmental testing to ensure that materials can withstand changes in temperature and humidity without distortion as well as testing to ensure resistance to chemicals and UV effects.  Further, mechanical testing shall ensure that the tensile and pull-out strength of mounting hardware is adequate to ensure a safe installation.  Test data shall be included with submittals. 
1. Typography:
1. Type style:  see drawings.  Copy shall be a true, clean, accurate reproduction of typeface(s) specified. Upper and lower case or all caps shall be as indicated in Sign Type drawings and Signage Schedule.  Letter spacing to be normal and interline spacing shall be set by manufacturer.

2. Arrows, symbols and logo art:  To be provided in style, sizes, colors and spacing as shown in drawings.

3. Grade II Braille utilizing perfectly round, clear insertion beads.
1. Color and Finishes:
1. Colors, patterns and artwork:  see drawings.
2. Message Background:  see drawings.

3. Finishes are to utilize decorative laminate faces as called out in the drawings with applied graphics including tactile requirements in adherence to ADA specifications.
2.3   SIGNS

A. Signage System:
A. All signs shall have a matching appearance and constructed utilizing the same manufacturing process to ensure a consistent look throughout.

B. Materials: 

B. Sign face shall be 0.035” (nominal) standard grade, high pressure surface laminate.  A painted sign face shall not be acceptable.

B. The sign shall incorporate balanced construction, specifically a core material as described under “Construction” sandwiched between identical laminates to prevent warping.  Laminate on the sign face only shall not be acceptable.

B. Tactile lettering shall be precision machined, raised 1/32", matte PETG and subsurface colored for scratch resistance.  

C. Construction:
C. Insert components shall have a .080 thickness non-glare acrylic window and shall be inlaid flush to sign face for a smooth, seamless appearance.

C. The laminates (front and back) shall be pressure laminated and precision machined together to a 90-degree angle.  Edges shall be smooth, void of chips, burrs, sharp edges and marks.

C. The signage shall utilize an acrylic sphere for Grade II Braille inserted directly into a scratch resistant, high pressure laminate sign face.  Braille dots are to be pressure fit in high tolerance drilled holes.

C. Braille dots shall be half hemispherical domed and protruding to a minimum 0.025”.

C. The signage shall utilize a pressure activated adhesive.  The adhesive shall be nonhazardous and shall allow for flexing and deflection of the adhered components due to changes in temperature and moisture without bond failure.

C. The core material shall not contain PVC.  It shall also provide dimensional stability in the face of changing humidity and temperature.

C. All signs shall be provided with appropriate mounting hardware.  Hardware shall be finished and architectural in appearance and suitable for the mounting surface.
D. Printed Inserts:
D. The signage shall accommodate polyester inserts (for opaque), polycarbonate inserts (for clear), or printed paper inserts by Owner to allow updating as required.  

D. Manufacturer shall provide a template containing layout, font, color, artwork and trim lines to allow Owner to produce inserts on laser or ink jet printer.  The template shall be in a PDF or Word format.

E. Quantities: 
Code and Facility Signage:
Sign Type A
Directory



​_________________
Sign Type B
Directional



_________________
Sign Type C
Overhead



_________________
Sign Type D  
Evacuation Map


_________________
Sign Type E  
Stairs




_________________
Sign Type E.2  
Restroom



_________________
Sign Type E.3  
Misc. Room ID


_________________
Sign Type F  
Small Room ID 


_________________
Sign Type G  
Medium Room ID 


_________________
Sign Type G.2  
Large Room ID 


_________________
Sign Type H 
Room ID Changeable Insert

_________________
Sign Type I  
Room ID Changeable Insert

_________________
Sign Type J  
Conference Room


_________________
Sign Type L 
Workstation ID


_________________
Sign Type M  
Flag Mount



_________________
Sign Type N  
Interior Stairwell


_________________
Sign Type N.2
Informational or 



Caution/Prohibitory


_________________

Sign Type S
Free-Standing (Stance)

_________________

PART 3     EXECUTION

3.1   SITE VISITS

A. Programming – sign contractor shall perform all wayfinding & programming.  Programming shall include location plan, message schedule, and/or plots, fire/evacuation maps and insert graphics.  All programming materials shall be submitted for approval.

3.2   CODE COMPLIANCE

A. It shall be the responsibility of the successful bidder to meet any and all local, state, and federal code requirements in fabricating and installing signs.   

3.3   DELIVERY, STORAGE, PROTECTION

A. Package to prevent damage or deterioration during shipment, handling, storage and installation.  Products should remain in original packaging until removal is necessary.  Store products in a dry, indoor location.

3.4   EXAMINATION

A. Installer shall examine signs for defects, damage and compliance with specifications.  Installation shall not proceed until unsatisfactory conditions are corrected.
3.5   INSTALLATION

A. General:  Installation locations shall be in accordance with ADA specifications.  Locate signs where indicated using mounting methods in compliance with manufacturer's written instructions:
1. The signage contractor shall coordinate installation schedules with the Owner and/or Construction Manager.

2. Installation shall be performed by manufacturer’s personnel trained and certified in manufacturer’s methods and procedures.

3. The signage contractor shall submit a CAD generated location plan noting the location of all signage and cross referenced to message schedule or plots for architect’s approval.

4. Installer to conduct a pre-installation survey prior to manufacturing to verify copy and sign location. Each location shall be noted using a low tack vinyl reproduction of actual sign.  Full scale renderings of directories and directionals shall also be provided.  Any location discrepancy or message issues shall be submitted to architect for review.

5. Signs shall be level, plumb, and at heights indicated with sign surfaces free from defects.

6. Upon completion of the work, signage contractor shall remove unused or discarded materials, containers and debris from site.

3.6   DIGITAL SIGN MANAGER
A. Manufacturer shall provide a cloud-based, password protected sign management platform enabling the Owner to view and manage their sign assets.  Every sign, sign type, mounting surface, copy, graphic treatment and building location shall be viewable and accessible through the platform.  The online sign management tool shall facilitate sign changes and additions seamlessly updating the system to reflect current conditions.
END OF SECTION
