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Casting
	Description
	Specifications

	New Thickness/ Measured At
	[bookmark: _GoBack]

	Minimum Thickness
	

	Warp Spec.
	.003" OVERALL (.076 MM)

	Chamber Volume (cc)
	55 OR 65 CC

	Surface Finish
	

	OHC Camshaft Bore Diameter
	

	Injector Tip Protrusion
	

	Lifter Bore Diameter
	

	Comments
	* 1ST ALL BOLTS IN SEQUENCE 22 FT/LBS, 2ND BOLTS IN FINAL PASS SEQUENCE SHORT 55°, MEDIUM 65°, LONG 75° DEGREES. * UPPER 44,88 INCH/LBS


Valve
Collapse [image: ]
	Valve Information
	Intake
	Exhaust

	Installed Stem Height
	1.990-2.000" (50.546-50.800 MM)
	1.990-2.000" (50.546-50.800 MM)

	Stem Diameter
	.3410-.3417" (8.661-8.679 MM)
	.3410-.3417" (8.661-8.679 MM)

	Total Length
	4.9120" (124.765 MM)
	4.9280" (125.171 MM)

	Head Diameter
	1.840" (46.736 MM)
	1.500" (38.100 MM)

	Angle
	45°
	45°

	Margin
	.031" (.787 MM)
	.031" (.787 MM)

	Recession
	
	

	Valve Guide Information
	Intake
	Exhaust

	Guide Height
	
	

	Guide Clearance
	.0010-.0030" (.025-.076 MM)
	.0010-.0030" (.025-.076 MM)

	Guide OD
	
	

	Valve Seal Type
	
	

	Valve Seat Information
	Intake
	Exhaust

	Seat Width
	.045-.070" (1.143-1.778 MM)
	.065-.098" (1.651-2.489 MM)

	Seat Angle
	46°
	46°

	Seat Outside Diameter
	
	

	Seat Inside Diameter
	
	

	Seat Insert Height
	
	

	Seat Insert Bore Diameter
	
	

	Seat Insert Bore Depth
	
	


Valve Spring
Collapse [image: ]
	Outer or Single Spring
	Intake
	Exhaust

	Free Length
	2.020" (51.308 MM)
	2.020" (51.308 MM)

	Installed Height
	1.690-1.710" (42.926-43.434 MM)
	1.690-1.710" (42.926-43.434 MM)

	Open Test Press
	187-203# @1.270
	187-203# @1.270

	Close Test Press
	76-84# @ 1.700
	76-84# @ 1.700

	Inner Spring
	Intake
	Exhaust

	Free Length
	
	

	Installed Height
	
	

	Open Test Press
	
	

	Close Test Press
	
	


Rocker Shaft
Collapse [image: ]
	Description
	Specifications

	Shaft Diameter
	

	Bore Diameter
	

	Oil Clearance
	

	Rock Arm Ratio
	


Installation
Collapse [image: ]
	Description
	Specifications

	Intake Valve Lash
	ZERO + 1 TURN DOWN

	Exhaust Valve Lash
	ZERO + 1 TURN DOWN

	Lash Adjustment Method
	

	Precup Torque Spec.
	

	Cyl Head Torque
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