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Roscan Gold discovers a high-grade extension at Kabaya intersecting 3.29 gpt gold over 22m including 5.78 gpt over 4m in the fresh rock
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Roscan Gold Corporation News Release September 13, 2022 


Toronto, Ontario. – September 13, 2022 – Roscan Gold Corporation (“Roscan” or the “Company”) (TSX-V: ROS; FSE:2OJ; OTCQB:RCGCF) is pleased to announce positive Reverse Circulation (“RC”) drilling results at Kabaya KB1 & KB2 (Figure 1) from an additional 21 holes totaling 3,122 meters (m). 

The recent drilling results provide significant intercepts at depth, in the fresh rock, demonstrating the continuity of the mineralization beyond the gold envelope under the $1,500 pit shell (see press release of June 8th, 2022), confirming the resource upside potential in this area. A similar southern plunge as KB1 was demonstrated in KB2 by drill hole RCDBS22-0112, creating the opportunity to grow the resources despite a lack of gold signature at the surface (see section figure 2).

The total strike length of KB1 & KB2 is currently 1,100 m, 180 m horizontal width and 250m vertical depth. This zone is open at depth and laterally. 

Drilling Highlights: 
Kabaya - RC Drill Holes

· 3.29 gpt gold over 22m from drill hole RCDBS22-0112 from 151m 
· Including 5.78 gpt gold over 4m from 159m
· Including 5.05 gpt gold over 4m from 169m

· [bookmark: _Hlk98488649]1.99 gpt gold over 21 m from drill hole RCDBS22-0111 from 86m 
· Including 5.84 gpt over 3m from100m

· 3.11 gpt gold over 7m from drill hole RCDBS22-0115 from 138m
· Including 15.25 gpt gold over 1m from 139m

· 1.74 gpt gold over 12m from drill hole RCDBS22-0084 from 6m
· Including 7.99 gpt gold over 1m from 10m
· Including 4.48 gpt gold over 1m from 13m.
And 1.10 gpt gold over 14m from 98m
· Including 3.24 gpt gold aver 2m from 101m

· 1.76 gpt gold over 8m from drill hole RCDBS22-0108 from 39m
· Including 4.4 gpt over 1m from 43m

· 1.44 gpt gold over 10m from drill hole RCDBS22-0113 from 70m 


Notes: 1: True width yet to be determined; 2: Table 1 – Assay Highlights, 3: 0.5gpt used as cut-off with 2m internal dilution, 4: No top-cut.

Nana Sangmuah, President and CEO, stated, "Drilling at Kabaya continues to expand the footprint of the gold mineralization which bodes well for further resource growth as expected. We are excited by new high-grade intercept in the fresh rock, suggesting a southern plunge in KB2, which is wide open for follow up drilling.” 

[image: Map

Description automatically generated]
Figure 1: Kabaya KB1 & KB2 drilling plan view, gold and lithological contouring envelopes projected to the surface and drill hole locations.

  
The gold mineralization at Kabaya KB1 & 2 is disseminated and associated with a strong kaolinization. From rock observations, this powdery zone (strong kaolinization) corresponds in the fresh rock at depth, with the albite-dolomite-pyrite-arsenopyrite alteration in a volcano-sedimentary sequence. The gold host rock is an alternate between tuffaceous and greywacke facies. As in the Mankouke gold deposit, the carbonaceous bedded mudstone constitutes the footwall for KB1 and the hanging wall for KB2. The gold zone is also limited by an NNE-SSW weakness, fractured, and sheared zones in hanging and footwall contacts resulting in rheology contrast.

The higher-grade zone doesn’t appear at the surface and from the longitudinal section the mineralization is plunging around -25° to the South. This higher-grade extension hasn’t been captured in the resource estimation (Press Release June 8th, 2022). 
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Figure 2: Kabaya gold deposit, KB1-KB2, section A 1389400N
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Figure 3: Kabaya KB2, Leapfrog Geo longitudinal section 
The Kabaya Deposit is part of the prolific regional Siribaya-Mankouke-Seko structural corridor (Figure 4). The Kabaya gold mineralized body is on the Eastern edge of this major structure and is well within the Roscan land package. 

Several additional positive assay results from the last Kandiole KN1, Kabaya KB3, and Mankouke South drilling program will be available soon.
[image: ]
Figure 4: Roscan permits on the Airborne Magnetic geophysics background with the Roscan resources zones, the targets in development, the gold deposits around

Drilling and Analytical Protocol

Roscan uses Geodrill Reverse Circulation (RC) to drill until maximum 170m to reach the target. In 2021, (holes RCDBS21-026 to RCDBS21-048), the samples have sent for preparation and 50g fire assays to Bureau Veritas Bamako laboratory and since January 2022, the samples are sent to the ALS Laboratories in Bamako, Mali and assayed at their analytical facilities to Ouagadougou for 2 kg Bottle Roll with atomic absorption finish including tail analysis for results more than 0.05ppm. Roscan applied industry-standard QA/QC procedures to the program using reference materials, blanks, standards, and duplicates.

Table 1: Drillhole Highlights at Kabaya KB3 (Dabia South)
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Table 2: Drillhole ID of Kabaya (Dabia South) 
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Qualified Person (QP) and NI 43-101 Disclosure
Greg Isenor, P. Geo., Director for the Company, is the designated Qualified Person for this news release within the meaning of National Instrument 43-101 (“NI 43-101”) and has reviewed and verified that the technical information contained herein is accurate and approves of the written disclosure of same.

About Roscan
Roscan Gold Corporation is a Canadian gold exploration company focused on the exploration and acquisition of gold properties in West Africa. The Company has assembled a significant land position of 100%-owned permits in an area of producing gold mines (including B2 Gold’s Fekola Mine which lies in a contiguous property to the west of Kandiole), and major gold deposits, located both north and south of its Kandiole Project in West Mali.

For further information, please contact: 

Nana Sangmuah
President & CEO 
Tel: (902) 832-5555
Email: info@Roscan.ca  

Forward Looking Statements 
This news release contains forward-looking information which is not comprised of historical facts. Forward-looking information is characterized by words such as “plan”, “expect”, “project”, “intend”, “believe”, “anticipate”, “estimate” and other similar words, or statements that certain events or conditions “may” or “will” occur. Forward-looking information involves risks, uncertainties and other factors that could cause actual events, results, and opportunities to differ materially from those expressed or implied by such forward-looking information. Factors that could cause actual results to differ materially from such forward-looking information include, but are not limited to, changes in the state of equity and debt markets, fluctuations in commodity prices, delays in obtaining required regulatory or governmental approvals, and other risks involved in the mineral exploration and development industry, including those risks set out in the Company’s management’s discussion and analysis as filed under the Company’s profile at www.sedar.com. Forward-looking information in this news release is based on the opinions and assumptions of management considered reasonable as of the date hereof, including that all necessary governmental and regulatory approvals will be received as and when expected. Although the Company believes that the assumptions and factors used in preparing the forward-looking information in this news release are reasonable, undue reliance should not be placed on such information. The Company disclaims any intention or obligation to update or revise any forward-looking information, other than as required by applicable securities laws. 

Neither the TSX Venture Exchange nor its Regulation Services Provider (as that term is defined in the policies of the TSX Venture Exchange) accepts responsibility for the adequacy or accuracy of this release.
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image7.emf
Hole ID From (m) To (m) Interval (m) gpt Au Comment

RCDBS22-0084 6 18 12 1.74 Saprolite

including 10 11 1 7.99 Saprolite

including 13 14 1 4.48 Saprolite

21 23 2 1.17 Saprolite

25 27 2 3.29 Saprolite

47 48 1 1.12 Saprolite

54 61 7 1.43 Saprolite

including 56 57 1 3.49 Saprolite

69 72 3 0.42 Saprolite

74 75 1 0.52 Saprolite

82 84 2 0.85 Saprolite

93 94 1 0.65 Saprolite

98 112 14 1.10 Saprolite

including 101 103 2 3.24 Saprolite

117 120 3 0.92 Saprolite

124 130 6 0.68 Saprolite

133 134 1 0.53 Saprolite

148 152 4 0.96 Saprolite

154 155 1 2.72 Saprolite

158 160 2 0.59 Saprolite

RCDBS22-0085 0 1 1 0.52 Laterite

13 16 3 2.61 Saprolite

including 14 15 1 6.25 Saprolite

18 19 1 2.76 Saprolite

51 54 3 0.58 Saprolite

64 70 6 0.85 Saprolite

RCDBS22-0086 34 35 1 0.79 Saprolite

47 50 3 1.80 Saprolite

80 82 2 0.69 Saprolite

84 85 1 0.58 Saprolite

98 100 2 4.02 Saprolite

105 107 2 0.90 Saprock

127 132 5 0.77 Fresh rock

134 140 6 0.64 Fresh rock

RCDBS22-0087 1 2 1 0.80 Laterite
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Hole ID From (m) To (m) Interval (m) gpt Au Comment

RCDBS22-0089 35 36 1 1.43 Fresh rock

42 43 1 0.74 Fresh rock

RCDBS22-0090 118 119 1 0.71 Saprolite

121 122 1 0.52 Saprolite

128 129 1 1.20 Saprolite

132 134 2 1.34 Saprolite

137 138 1 0.62 Saprolite

140 147 7 0.86 Saprolite

RCDBS22-0091 144 145 1 0.72 Saprolite

RCDBS22-0092 157 160 3 1.21 Saprolite

RCDBS22-0105 117 119 2 0.97 Saprolite

126 138 12 0.91 Saprolite

144 165 21 1.02 Saprolite

162 165 3 1.05 Saprolite

167 168 1 2.77 Saprolite

170 173 3 0.74 Saprolite

RCDBS22-0106 49 50 1 0.78 Saprolite

RCDBS22-0107 103 105 2 0.82 Saprolite

111 114 3 0.45 Saprolite

117 119 2 0.59 Saprolite

162 163 1 0.71 Saprolite

166 167 1 1.06 Saprolite

170 173 3 0.64 Saprolite

177 180 3 0.51 Saprolite

RCDBS22-0108 2 3 1 4.17 Laterite

39 47 8 1.76 Saprolite

including 43 44 1 4.44 Saprolite

49 50 1 0.92 Saprolite

61 72 11 1.07 Saprolite

74 78 4 0.81 Saprolite

106 107 1 0.62 Saprolite

RCDBS22-0110 119 123 4 0.73 Saprolite

135 140 5 0.56 Saprolite

142 147 5 0.95 Saprolite

RCDBS22-0111 61 62 1 1.00 Saprolite

73 75 2 1.42 Saprolite

77 79 2 0.59 Saprolite

81 84 3 0.74 Saprolite

86 107 21 1.99

Saprolite & 

Fresh rock

including 100 103 3 5.84 Fresh rock

109 112 3 1.45 Fresh rock

114 115 1 0.65 Fresh rock

119 128 9 1.59 Fresh rock

including 124 125 1 3.27 Fresh rock

130 133 3 0.60 Fresh rock

140 151 11 0.81 Fresh rock

162 174 12 0.85 Fresh rock
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Hole ID From (m) To (m) Interval (m) gpt Au Comment

RCDBS22-0112 10 11 1 1.08 Saprolite

40 41 1 0.73 Saprolite

119 123 4 1.05 Saprolite

125 129 4 0.96 Saprock

131 135 4 4.32 Fresh rock

including 132 133 1 13.75 Fresh rock

137 140 3 1.03 Fresh rock

144 145 1 0.98 Fresh rock

147 149 2 0.77 Fresh rock

151 173 22 3.29 Fresh rock

including 159 163 4 5.78 Fresh rock

including 169 173 4 5.05 Fresh rock

RCDBS22-0113 62 63 1 0.77 Saprolite

64 68 4 0.87 Saprolite

70 80 10 1.44

Saprolite & 

Saprock

86 90 4 8.01

Fresh rock 

& Saprolite

including 88 90 2 14.89 Saprolite

141 142 1 0.83 Fresh rock

151 152 1 0.74 Fresh rock

172 173 1 1.17 Fresh rock

RCDBS22-0114 10 11 1 0.75 Saprolite

14 18 4 0.73 Saprolite

RCDBS22-0115

0 12 12 0.91

Laterite & 

Saprolite

37 41 4 0.89 Saprolite

67 68 1 0.98 Saprolite

88 99 11 0.86

Saprock & 

Fresh rock

101 102 1 0.59 Fresh rock

114 117 3 1.45 Fresh rock

including 116 117 1 3.37 Fresh rock

126 133 7 0.67 Fresh rock

138 145 7 3.11 Fresh rock

including 139 140 1 15.25 Fresh rock

148 150 2 0.49 Fresh rock

RCDBS22-0116 0 8 8 2.36 Laterite

including 3 6 3 4.93 Laterite

71 72 1 1.06 Saprolite

162 163 1 0.51 Fresh rock

165 170 5 0.54 Fresh rock
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Hole ID X Collar Y Collar Zcolar Section AZM DIPEOH

RCDBS22-0084 265328 1389524 208 1389525 270 -50 200

RCDBS22-0085 265245 1389701 182 1389700 90 -50 115

RCDBS22-0086 265215 1389701 182 1389700 90 -50 140

RCDBS22-0087 265488 1389950 178 1389950 90 -50 125

RCDBS22-0088* 265349 1390204 168 1390205 270 -50 70

RCDBS22-0089 265398 1390199 166 1390200 270 -50 110

RCDBS22-0090 265180 1389401 175 1389400 90 -50 147

RCDBS22-0091 265219 1389352 177 1389350 90 -50 170

RCDBS22-0092 265179 1389349 174 1389350 90 -50 170

RCDBS22-0105 265176 1389393 182 1389395 90 -50 185

RCDBS22-0106 265260 1389354 185 1389355 90 -50 110

RCDBS22-0107 265185 1389598 185 1389600 90 -70 180

RCDBS22-0108 265276 1389392 186 1389390 90 -50 130

RCDBS22-0109* 265331 1389700 195 1389700 90 -70 112

RCDBS22-0110 265200 1389649 191 1389650 90 -70 170

RCDBS22-0111 265474 1389450 205 1389450 90 -70 175

RCDBS22-0112 265424 1389400 206 1389400 90 -50 173

RCDBS22-0113 265499 1389550 209 1389550 90 -70 175

RCDBS22-0114 265347 1389665 196 1389665 90 -70 120

RCDBS22-0115 265645 1389650 203 1389650 270 -60 175

RCDBS22-0116 265527 1389747 198 1389745 90 -70 170

* No significant result
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