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SPK-
OW6
6.5"
 
Surface
 
Mount
 
40W
 
Speaker,
 
8
 
Ohm/70V
) (
FEATURES
) (
•
•
•
•
•
•
) (
Excellent sound coverage with intelligible treble and powerful bass Sturdy ABS enclosure
Stylish design to match room decor Taps for 8 Ohm, 70 and 100 volts
Easy
 
installation
 
and
 
simple
 
power
 
settings
Adjustable
 
installation
 
brackets
) (
DESCRIPTION
) (
Hall
 
Technologies
 
Speakers
 
offer
 
versatility
 
and
 
convenience.
 
SPK-OW6
 
is
 
a
 
surface
 
mount,
 
40-watt
 
loudspeaker that
 
includes
 
taps
 
for
 
8
 
ohm,
 
100-volt
 
and
 
70-volt
 
audio
 
solutions
 
and
 
comes
 
in
 
a
 
white
 
finish.
 
SPK-OW6
 
is
 
perfect
for
 
K-12
 
classrooms,
 
higher-ed
 
classrooms
 
and
 
lecture
 
halls,
 
and
 
medium
 
to
 
large
 
meeting
 
spaces.
) (
Hall Technologies designs and builds complete solutions for AV applications. In order to provide our customers with
 
a complete solution we have to offer all the components necessary to build out the application. Many of our solutions include
 
built-in
 
and
 
external
 
audio
 
amplifiers.
 
We
 
offer
 
a
 
modest
 
yet
 
powerful
 
line
 
of
 
speakers
 
to
 
compliment
 
our
audio
 
solutions
 
and
 
add
 
convenience
 
to
 
our
 
customers
 
for
 
one
 
stop
 
shopping.
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Feature
) (
Detail
) (
Power at 
100V
) (
40W
) (
Power at 
70V
) (
20W
) (
SPL
 
(1W/1M)
) (
88dB
) (
Frequency Response 
7
) (
70Hz-20KHz
) (
Dispersion 
Angle
) (
90°
) (
Dimensions
) (
300mm
 
x
 
216mm
 
x
 
195mm
) (
Installation
) (
Wall
 
mounted
) (
Enclosure
 
Material
) (
ABS
) (
Weight
) (
3.3Kg
) (
Finish
) (
White
) (
Speakers
) (
1.5”x1“(Treble)
 
6”x1”
 
(Bass)
) (
SPL
 
(1W/1M)
) (
88dB
)
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