{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":5,"n_cols":11,"rows_kept":5,"merged":[[1,0,1,11],[4,0,4,10],[6,5,6,9]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES - NUMBER 2"]
[]
["MAINTENANCE AND SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING FOR A PERIOD OF TWO YEARS"]

{"sheet":"SUMMARY","index":1,"n_rows":17,"n_cols":5,"rows_kept":17,"merged":[[1,0,1,4],[2,0,3,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITIES - NUMBER 2"]
["MAINTENANCE AND SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING FOR A PERIOD OF TWO YEARS"]
[]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01",{"v":0,"d":"0.00"}]
[2,null,"MAINTENANCE AND SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING","Bill no. 02"]
[3,null,"CONDUCTING TRAINING SESSION AND DRILL FOR THE STAFF AT ROASHANEE BUILDING","Bill no. 03"]
[4,null,"TENDERER'S ADJUSTMENTS","Bill no. 04"]
[]
[null,null,"Sub total"]
[null,null,"GST 8%"]
[]
[]
[null,null,"GRAND TOTAL carried to form of bid",null,0]

{"sheet":"BoQ","index":2,"n_rows":88,"n_cols":8,"rows_kept":88,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["BILL OF QUANTITIES - NUMBER 2"]
["MAINTENANCE AND SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING FOR A PERIOD OF TWO YEARS"]
[]
[]
["Item","Description","Unit\n(U)","Quantity\n(Q)","Rate","Rate","Total Rate per Item \n(M+L)","Total Amount per Item\nQ x (M+L)"]
[{"$nulls":4},"Material (M)","Labour (L)"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"," "]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[]
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary",0,0,0,0,0,0]
[null,"BILL No: 02"]
[null,"MAINTENANCE AND SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING"]
[]
[2.1,"General"]
[null,"(a) Rates shall include for material, labour, and other expenses involved to complete the works."]
[]
[2.2,"Maintenance and Servicing of Fire Pump System at Roashanee Building for Two Years"]
[null,"(a) Rates shall include for the maintenance and servicing of the fire pump system at Roashanee Building, including the system's water delivery pipes and other parts/components."]
[null,"(b) Rates shall include for material, labor, and other expenses required for the comprehensive maintenance and servicing of the entire system. During the maintenance/servicing period, if any spare parts have to be replaced due to damages or wear & tear, the spare parts shall be replaced within this rate. No additional price  should be charged for the necessary replacement of spare parts during the maintenance period (2 years)."]
[{"v":1,"d":"(1)"},"Maintenance and servicing of the fire pump system for a period of two years. Once in every six months, the contractor shall conduct the following tasks;\n   -Performing a test run.\n   -Checking the power source.\n   -Lubricating the parts.\n   -Monitoring/recording the pressure gauge and system suction.\n   -Checking for leaks, discharges, ususual noises, or vibrations.\n   -Checking pump packing glands for slight discharge.\n   -Observing time for the motor to accelerate to full speed.\n   -Replacing the spare part if necessary.\n*A single rate shall be mentioned for every six months (6 months x 4 times = 24 months or 2 yrs)","Six Months",{"v":4,"d":"4.00"}]
[]
[2.3,"Maintenance and Servicing of Fire Alarms System at Roashanee Building for Two Years"]
[null,"(a) Rates shall include for the maintenance and servicing of the fire alarms system at Roashanee Building, including system's alarms/sounders, smoke detectors, manual call points (MCP), cables, and the control panel. "]
[null,"(b) Rates shall include for material, labor, and other expenses required for the comprehensive maintenance and servicing of the entire system. During the maintenance/servicing period, if any spare parts have to be replaced due to damages or wear & tear, the spare parts shall be replaced within this rate. No additional price  should be charged for the necessary replacement of spare parts during the maintenance period (2 years)."]
[{"v":1,"d":"(1)"},"Maintenance and servicing of the fire alarms system for a period of two years. Once in every six months, the contractor shall conduct the following tasks;\n   -Performing a test run.\n   -Checking the power source.\n   -Checking the alarms, detectors, manual call points, cables, and the control panel.\n   -Examining the batteries and connections.\n   -Replacing the spare parts if necessary.\n*A single rate shall be mentioned for every six months (6 months x 4 times = 24 months or 2 yrs)","Six Months",{"v":4,"d":"4.00"}]
[]
[2.4,"Maintenance and Servicing of Loudspeaker System at Roashanee Building for Two Years"]
[null,"(a) Rates shall include for the maintenance and servicing of the loudspeaker system at Roashanee Building, including system's ceiling-mounted speakers in each floor, microphone, mixer, power amplifier, cables, and adaptor plugs."]
[null,"(b) Rates shall include for material, labor, and other expenses required for the comprehensive maintenance and servicing of the entire system. During the maintenance/servicing period, if any spare parts have to be replaced due to damages or wear & tear, the spare parts shall be replaced within this rate. No additional price  should be charged for the necessary replacement of spare parts during the maintenance period (2 years)."]
[{"v":1,"d":"(1)"},"Maintenance and servicing of the loudspeaker system for a period of two years. Once in every six months, the contractor shall conduct the following tasks;\n   -Performing a test run.\n   -Checking the power source.\n   -Checking the ceiling-mounted speakers in each floor.\n   -Checking  the microphone, mixer, power amplifier, cables, and adaptor plugs.\n   -Examining the batteries and connections.\n   -Replacing the spare parts if necessary.\n*A single rate shall be mentioned for every six months (6 months x 4 times = 24 months or 2 yrs)","Six Months",{"v":4,"d":"4.00"}]
[]
[2.5,"Maintenance and Servicing of Fire Extinguisher Cylinders at Roashanee Building for Two Years"]
[null,"(a) Rates shall include for the maintenance and servicing of the fire extinguisher cylinders at Roashanee Building."]
[null,"(b) Rates shall include for material, labor, and other expenses required for the comprehensive maintenance and servicing of fire extinguisher cylinders. During the maintenance/servicing period, if any fire extinguisher cylinder has to be replaced due to damages or wear & tear, the fire extinguisher cylinder shall be replaced within this rate. No additional price  should be charged for the necessary replacement of fire extinguisher cylinder during the maintenance period (2 years)."]
[{"v":1,"d":"(1)"},"Maintenance and servicing of the fire extinguisher cylinders for a period of two years. Once in every six months, the contractor shall conduct the following tasks;\n   -Refilling the cylinders.\n   -Changing the nozzle, trigger, and handle of the fire extinguisher cylinders.\n*A single rate shall be mentioned for every six months (6 months x 4 times = 24 months or 2 yrs).\nThe  number of fire extinguisher cylinders at Roashanee Building are as follows;\n   -2KG CO2 Fire Extinguishers: 30 cylinders\n   -6KG DCP Fire Extinguishers: 5 cylinders\n   -9L Water Fire Extinguishers: 30 cylinders","Six Months",{"v":4,"d":"4.00"}]
[null,"BILL No: 02 - MAINTENANCE & SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No: 03"]
[null,"CONDUCTING TRAINING SESSION AND DRILL FOR THE STAFF AT ROASHANEE BUILDING"]
[]
[3.1,"General"]
[null,"(a) Rates shall include for material, labour, and all other expenses involved to complete the works."]
[]
[3.2,"Conducting Training Sessions for the Staff at Roashanee Building"]
[null,"(a) Rates shall include for material, labor, capital, and other additional works involved in conducting the tranining sessions. "]
[{"v":1,"d":"(1)"},"Conducting a basic training in form of an information/awareness session for all the staff working in the Roashanee Building (around 200 to 250 staff). For all these staff, one session shall be conducted in each year (two sessions for two years). For these sessions, a multipurpose event hall will be provided by the Ministry, which could cater 30 staff at a time.","Session",{"v":2,"d":"2.00"}]
[{"v":2,"d":"(2)"},"Conducting an advanced training in form of an information session and practical use of fire safety equipment for the focal points or fire managers of Roashanee Building (around 35 to 40 staff). One session shall be conducted in each year (two sessions for two years). ","Session",{"v":2,"d":"2.00"}]
[]
[3.3,"Conducting a Fire-Drill for the Staff at Roashanee Building"]
[null,"(a) Rates shall include for material, labor, capital, and other additional works involved in preparing, conducting, and completing the fire drill."]
[{"v":1,"d":"(1)"},"Conducting a fire drill for all the staff working in the Roashanee Building (around 200 to 250 staff). One drill shall be conducted within the two years.","Drill",{"v":1,"d":"1.00"}]
[null,"BILL No: 03 - CONDUCTING TRAINING SESSION & DRILL FOR THE STAFF AT ROASHANEE BUILDING"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]
[null,"BILL No:4"]
[null,"TENDERER'S ADJUSTMENTS"]
[4.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[4.2,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"MAINTENANCE & SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING, Bill no. 02"]
[{"v":3,"d":"(3)"},"CONDUCTING TRAINING SESSION AND DRILL FOR THE STAFF AT ROASHANEE BUILDING, Bill no. 03"]
[null,"ADDITIONS TOTAL"]
[]
[4.3,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"MAINTENANCE & SERVICING OF FIRE SAFETY EQUIPMENT AT ROASHANEE BUILDING, Bill no. 02"]
[{"v":3,"d":"(3)"},"CONDUCTING TRAINING SESSION AND DRILL FOR THE STAFF AT ROASHANEE BUILDING, Bill no. 03"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 4 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 4 - Carried over to summary"]