{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["COVER SHEET","SUMMARY","BoQ"],"not_rendered":{"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"COVER SHEET","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[1,0,1,11],[6,5,6,9]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10}," BILL OF QUANTITIES - LOT 3"]
[]
[{"$nulls":10},"ORANGE HIYA THIRD FLOOR - SUPPLY OF FURNITURES"]
[]
[{"$nulls":10},0]

{"sheet":"SUMMARY","index":1,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[1,0,1,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
[]
["SUMMARY OF BILLS OF QUANTITIES - LOT 3"]
["ORANGE HIYA THIRD FLOOR - SUPPLY OF FURNITURES"]
[]
["Bill No",null,"Description",null,"Amount"]
[]
[1,null,"PRELIMINARIES","Bill no. 01",0]
[2,null,"SUPPLY OF FURNITURES","Bill no. 02",0]
[3,null,"TENDERER'S ADJUSTMENTS","Bill no. 03",0]
[null,null,"Sub total",null,0]
[null,null,"GST 6%",null,0]
[]
[null,null,"GRAND TOTAL carried to form of bid",null,0]

{"sheet":"BoQ","index":2,"n_rows":62,"n_cols":8,"rows_kept":62,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,7,5,7]],"flags":["formulas_cached_only"]}
["BILL OF QUANTITIES - LOT 3"]
["ORANGE HIYA THIRD FLOOR - SUPPLY OF FURNITURES"]
[]
[]
["Item","Description","Unit","Quantity","Rate/ Unit ","Rate/ Unit ","Total Unit Rate","Amount"]
[{"$nulls":4},"Material","Labour","Rates per Units"]
[null,"BILL No: 01"]
[null,"PRELIMINARIES"]
[]
[1.1,"General Notes"]
["(1)","Abbreviations"," "]
[null,"m - meter"]
[null,"No - numbers"]
[null,"m³ - cubic meter"]
[null,"m² - square meter"]
[null,"Lm - Linear meter"]
[null,"KG - Kilograms"]
[null,"incl - including"]
[null,"mm - millimeter"]
[null,"dia - diameter"]
[null,"SS - Stainless Steel"]
[null,"GI - Galvanized Iron"]
[]
[1.2,"Clean-up"]
[{"v":1,"d":"(1)"},"Allow for clean-up of completed works and site upon completion.","Item",{"v":1,"d":"1.00"}]
[]
[null,"BILL No: 01 PRELIMINARIES"]
[null,"TOTAL OF BILL No: 01 - Carried over to summary"]
[null,"BILL No: 02"]
[null,"SUPPLY OF FURNITURE"]
[2.1,"General"]
[null,"(a) Rates shall include for supply, complete installation/assemble, and arrangement of furnitures in Orange Hiya third floor."]
[null,"(b) Contractor shall obtain approval of the Project Manager for each type of furniture prior to supply, installation/assemble, and arrangement. Also, contractor shall provide a catalogue (with photos)."]
[null,"(c) Contractor shall supply, install/assemble, and arrange the following furnitures;"]
[{"v":1,"d":"(1)"},"Rectangular Office-Table with Table Divider\nOffice table with two lockable drawers (1200mm Length x 750mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging.  Table should be seperated with a desk divider attached/fixed on the table.  The tables that require divider are shown in the annexed drawing with red lines. The color of the table and divider shall be shades of brown or gray.","No",{"v":78,"d":"78.00"}]
[{"v":2,"d":"(2)"},"Rectangular Office-Table\nOffice table with three lockable drawers (1300mm Length x 750mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging.  The color of the table shall be shades of brown or gray.","No",{"v":16,"d":"16.00"}]
[{"v":3,"d":"(3)"},"Rectangular Executive-Table for DDG Rooms and DG Room\nOffice table with three lockable drawers (1500mm Length x 750mm Depth x 750mm Height). Table should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging. The color of the table shall be shades of brown or gray.","No",{"v":5,"d":"5.00"}]
[{"v":4,"d":"(4)"},"Wooden Round Meeting Table \nThe table shall have a diameter of  3ft and the tabletop shall be of 25mm Melamine top with 2mm ABS Edging. The color of the table shall be shades of brown or gray.","No",{"v":10,"d":"10.00"}]
[{"v":5,"d":"(5)"},"Wooden Round Meeting Table for DG Room\nThe table shall have a diameter of  2.5ft and the tabletop shall be of 25mm Melamine top with 2mm ABS Edging. The color of the table shall be shades of brown or gray.","No",{"v":1,"d":"1.00"}]
[{"v":6,"d":"(6)"},"Wooden Round Meeting Table for Tea Room Area\nThe table shall have a diameter of  3ft and the tabletop shall be of 25mm Melamine top with 2mm ABS Edging. The table shall have X-panel legs. The color of the table shall be shades of brown or gray.","No",{"v":3,"d":"3.00"}]
[{"v":7,"d":"(7)"},"Wooden Conference Table for the Two Meeting Rooms\nTable should be of solid wood with a finishing of 25mm Melamine tabletop and 2mm ABS edging. The length of the table shall be around 14ft. The color of the table shall be shades of brown or gray.","No",{"v":2,"d":"2.00"}]
[{"v":8,"d":"(8)"},"Wooden Filing Rack. \nNumber of shelves in each filing rack: 5\nHeight of each shelve: minimum 15inch \nThe color of the table shall be shades of brown or gray.","No",{"v":25,"d":"25.00"}]
[]
[null,"BILL No: 02 - SUPPLY OF FURNITURES"]
[null,"TOTAL OF BILL No: 02 - Carried over to summary"]
[null,"BILL No:03"]
[null,"TENDERER'S ADJUSTMENTS"]
[3.1,"Any adjustments that the contractor may consider necessary should be written below and on similar continuation sheets if required, and the net amount of the adjustments is to be carried to the summary."]
[null,"(a) Provide detail description of work items under each bill and insert extra pages if required."]
[]
[3.2,"Additions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"SUPPLY OF FURNITURES, Bill no. 02"]
[null,"ADDITIONS TOTAL"]
[]
[3.3,"Omissions"]
[{"v":1,"d":"(1)"},"PRELIMINARIES, Bill no. 01"]
[{"v":2,"d":"(2)"},"SUPPLY OF FURNITURES, Bill no. 02"]
[null,"OMISSIONS TOTAL"]
[]
[null,"BILL No: 03 - TENDERER'S ADJUSTMENTS"]
[null,"TOTAL OF BILL No: 03 - Carried over to summary"]