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Abstract:
The preparation of polymeric nanofibers via electrospinning represents a significant part of nanotechnology. Nanofiber membranes are widely utilized in functional nanocomposite materials for applications such as environmental protection (sorption and filtration media, pollutant degradation), medical use (wound dressings with antimicrobial properties, drug delivery carriers, tissue engineering), and textiles for functional clothing. This presentation aims to demonstrate the advantages and potential applications of these nanofibers in the creation of functional nanocomposites for a broad range of practical uses.

Abstrakt:
Příprava polymerních nanovláken pomocí elektrického zvláknění je významnou součástí nanotechnologií a nanovlákenné membrány nacházejí široké uplatnění ve funkčních nanokompozitních materiálech pro využití v ochraně životního prostředí (sorpční a filtrační media, degradace polutantů), v medicínských aplikacích (krytí ran – antimikrobiální funkce, nosiče léčiv, tkáňové inženýrství) a v textiliích pro funkční oděvy. Cílem prezentace bude ukázat přednosti a možnosti využití těchto nanovláken pro tvorbu funkčních nanokompozitů pro širokou škálu praktických aplikací. 
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Scheme of polymeric nanofiber preparation via electrospinning
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