Sizes: EU

Filament: Recreus 82A, 3Dfils 85A

Use TPU 95A first (Overture), don't use "high speed", "high flow" (too stiff, uncomfortable)



Use the universal print files (gcodes) instead of slicing the 3d models.

Upload the gcodes on an SD card and insert them in the printer. Launch the gcodes from the printer interface, ignore warnings and proceed. Adjust temperature once the print starts to fit your filament needs 

Printer requirements for the gcodes: 0.6mm nozzle, 250 x 250 x 300 buildplate fits every size, 256 x 256 x 256 fits size 41, 250 x 250 x 250mm fits size 40

Depending on the size, each pair of shoes takes 9 to 12 hours, weights 120 to 160 grams 



Video: https://www.youtube.com/watch?v=y2OOk_2cu5w

Website: https://www.riverfamily.art/




Cura Slicer Settings (see Aspys_Cura_Project.3mf):


- layer height: 0.36mm
- infill line width: 0.65 (or 0.4 with 162% infill flow)
- wall line count: 0
- top layers: 0
- bottom layers: 0
- initial bottom layers: 0
- infill line distance: 3mm
- infill pattern: grid
- connect infill lines: yes
- infill line direction: []
- randomize infill start: yes
- infill overlap: 0mm
- infill speed: 18mm/s
- combing mode: off
- z hop: 1.2mm


settings modifier (200x200x2.4mm solid, placed at Z = 0) 

- infill flow: 300% (1.2 mm line width)
- infill speed: 9mm/s

How to design and slice: https://www.youtube.com/watch?v=6ae-rzo_zJM



BambuStudio settings (see "Aspys_BambuStudio_Project.3mf")

Shoe:
- layer height: 0.36mm
- line width sparse infill: 0.9mm
- wall loops: 0
- top shell layers: 0
- bottom shell layers: 0
- sparse infill density: 43%
- Infill pattern: Grid
- Infill anchor: 1000 (unlimited)
- Max infill anchor: 1000 (unlimited)
- Infill direction: 45°
- Detect narrow internal solid infill: no
- Speed sparse infill: 18 mm/s
- Enable support: no
- Reduce infill retraction: no

Cube modifier  (256x256x2.4mm at Z=0):

- Infill density: 60%
- Infill line width: 1.2mm


Filament:

- Retraction: 2.4mm
- Wipe: no
- Z hop: 1.2mm, Normal type
- Max volumetric speed: 4.8 mm^3/s 



LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names