
Bambu Studio / Orca Slicer settings:

Global, Taka_1, Taka_3:

- layer height: 0.2mm
- line width sparse infill: 0.6mm
- line width walls: 0.5mm
- wall loops: 0
- top shell layers: 0
- bottom shell layers: 0
- infill density: 62%
- infill pattern: Grid
- infill anchor: 1000 (unlimited)
- max infill anchor: 1000 (unlimited)
- infill direction: 45°
- infill/wall overlap: 90%
- detect narrow internal solid infill: no
- speed sparse infill: 18 mm/s
- reduce infill retraction: no
- enable support: no
- brim: outer and inner, gap 0mm

Taka_2:

- walls: 12
- object flow ratio: 1.2

Taka_4:

- line width sparse infill: 0.4mm
- infill density: 25%
- infill pattern: rectilinear
- infill direction: 0°

Taka_5:

- line width sparse infill: 0.4mm
- infill density: 25%

Taka_6:

- object flow ratio: 1.2
- infill density: 100%
- infill pattern: rectilinear
- infill direction: 0°

Taka_7:

- infill density: 99%
- infill direction: 0°

Taka_8:

- line width sparse infill: 0.3mm
- object flow ratio: 2
- infill density: 80%
- infill pattern: triangles

Taka_9:

- walls: 12

Filament:

- Retraction: 1.8mm
- Wipe: no
- Z hop: 1.2mm, Normal type
- Max volumetric speed: 2.5 mm^3/s 
- Temperature: 215°C - 225°C

--- 

Website: https://www.riverfamily.art/

---

LICENSE: Public Domain (https://creativecommons.org/share-your-work/public-domain/cc0/)

Also applies to gcodes, slicing process, pictures, videos and names