Erae Touch update:
Compatibility:
	•	MacOs 10.14 and above
	•	Windows 10 and above
	•	Ubuntu 20.04 and above (curl library might be required: sudo apt install libcurl4)

/!\ Make sure to  save your layout and close your DAW before updating the firmware /!\
Erae Lab 1.4.1:
Bug fixes:
	•	Fix communication issue between EraeLab and EraeTouch (failure to synchronize)

Erae Touch Firmware 1.4.1:
Bug fixes:
	•	Fix boot while USB plugged in

Erae Touch Firmware 1.3.0:
New features:
	•	CC and Channel numbers can be changed from the CC mapping menu
	•	User can choose whether to send MPE and non MPE MIDI data on different USB MIDI outputs or not
	•	Long press on Alt button when in CC Mapping mode will save all layouts (including MIDI channels, MIDI CC and scale information)
	•	Improved finger detection
	•	Revamped all MIDI FX
	•	Better finger pressure filter on slide
	•	Control Change & Program Change buttons state is now shared across all layouts
	•	MPE configuration messages are now only sent when changing layout
	•	MIDI Clock is now in internal mode by default
	•	Improved Sequencer Record Quantization

Bug fixes:
	•	Fixed button behaviour when using with DAW
	•	Fixed inconsistent internal BPM issue
	•	Fixed issue that caused some USB MIDI messages to not be transmitted
	•	Fixed sequencer sequence saving issues
	•	Fixed stuck note issue in sequencer (a single sequencer can now play at most 16 notes at the same time)
	•	Fixed button bugs
	•	Fixed imprecision of note selection in Harmonizer effect UI
	•	Fixed a bug that prevented some animations from being displayed
	•	Fixed BPM display issues and capped internal BPM to 999
	•	Fixed some visual bugs

Erae Touch Firmware 1.4.0:
New features:
	•	Animations on API zone
	•	Sequencer view shows lowest octave with notes by default
	•	Silent select feature (select element without playing it): Scale button + element click

Bug fixes:
	•	Project retro-compatibility bug fix

Erae Lab 1.4.0:
New features:
	•	Default enable halo animation when pressure is activated for Fader 1D/Fader 2D
	•	Automatic CC increment when adding new elements
	•	Automatic API zone index increment when adding API zone
	•	Automatic new version check: Firmware and Lab
	•	Change value on sliders with arrow keys

Bug fixes:
	•	Project retro-compatibility bug fix
	•	Minor UI fixes and changes
	•	Save / Save as bug fix

Erae Touch Firmware 1.3.0:
New features:
	•	CC and Channel numbers can be changed from the CC mapping menu
	•	User can choose whether to send MPE and non MPE MIDI data on different USB MIDI outputs or not
	•	Long press on Alt button when in CC Mapping mode will save all layouts (including MIDI channels, MIDI CC and scale information)
	•	Improved finger detection
	•	Revamped all MIDI FX
	•	Better finger pressure filter on slide
	•	Control Change & Program Change buttons state is now shared across all layouts
	•	MPE configuration messages are now only sent when changing layout
	•	MIDI Clock is now in internal mode by default
	•	Improved Sequencer Record Quantization

Bug fixes:
	•	Fixed button behaviour when using with DAW
	•	Fixed inconsistent internal BPM issue
	•	Fixed issue that caused some USB MIDI messages to not be transmitted
	•	Fixed sequencer sequence saving issues
	•	Fixed stuck note issue in sequencer (a single sequencer can now play at most 16 notes at the same time)
	•	Fixed button bugs
	•	Fixed imprecision of note selection in Harmonizer effect UI
	•	Fixed a bug that prevented some animations from being displayed
	•	Fixed BPM display issues and capped internal BPM to 999
	•	Fixed some visual bugs

Erae Lab 1.3.0:
New features:
	•	Project management
	•	Pitchbend in vibrato section
	•	Improved learn section
	•	Deactivate preview mode upon pulling layouts
Bug fixes:
	•	Fix duplicate elements bug
	•	Contraints relative CC initial value within min/max
	•	Various UI improvements